






Started logging.
09:58:33.742466 Language server launched with arguments:
09:58:33.742466   arg[0] = d:\Program Files\Arduino IDE\resources\app\node_modules\arduino-ide-extension\build\arduino-language-server.exe
09:58:33.742466   arg[1] = -clangd
09:58:33.742466   arg[2] = d:\Program Files\Arduino IDE\resources\app\node_modules\arduino-ide-extension\build\clangd.exe
09:58:33.742466   arg[3] = -cli-daemon-addr
09:58:33.742969   arg[4] = localhost:57938
09:58:33.742991   arg[5] = -cli-daemon-instance
09:58:33.742991   arg[6] = 1
09:58:33.742991   arg[7] = -fqbn
09:58:33.742991   arg[8] = arduino:avr:uno
09:58:34.074752   arg[9] = -skip-libraries-discovery-on-rebuild
09:58:33.754387 listen tcp 127.0.0.1:6060: bind: Only one usage of each socket address (protocol/network address/port) is normally permitted.
09:58:34.074981   arg[10] = -board-name
09:58:34.074981   arg[11] = "Arduino Uno"
09:58:34.074981   arg[12] = -no-real-time-diagnostics
09:58:34.074981   arg[13] = -log
09:58:34.074981   arg[14] = -logpath
09:58:34.074981   arg[15] = g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer
09:58:34.075583 logging to g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\inols.log
09:58:34.080538 LS: : Initial board configuration: arduino:avr:uno
09:58:34.080538 LS: : Language server build path: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764
09:58:34.080538 LS: : Language server build sketch root: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch
09:58:34.081041 LS: : Language server FULL build path: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1379094214
09:58:34.081093 IN Elapsed: 0s
09:58:34.081093 IDE --> LS REQU initialize 0
09:58:34.082181                 initialize 0: write-locked
09:58:34.082715                 initialize 0: write-unlocked
09:58:34.083309 INIT --- : initializing workbench: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer
09:58:34.083309 INIT --- : read-locked
09:58:34.083309 INIT --- : read-unlocked
09:58:34.083309                 initialize 0: initialization parameters: {"capabilities":{"textDocumentSync":{"openClose":true,"change":2,"save":{"includeText":true}},"completionProvider":{"triggerCharacters":[".","\u003c","\u003e",":","\"","/"],"allCommitCharacters":[" ","\t","(",")","[","]","{","}","\u003c","\u003e",":",";",",","+","-","/","*","%","^","\u0026","#","?",".","=","\"","'","|"],"completionItem":{}},"hoverProvider":{},"signatureHelpProvider":{"triggerCharacters":["(",","]},"definitionProvider":{},"documentHighlightProvider":{},"documentSymbolProvider":{},"codeActionProvider":{"codeActionKinds":["quickfix","refactor","info"]},"documentFormattingProvider":{},"documentRangeFormattingProvider":{},"documentOnTypeFormattingProvider":{"firstTriggerCharacter":"\n"},"renameProvider":{},"executeCommandProvider":{"commands":["clangd.applyFix","clangd.applyTweak"]},"workspaceSymbolProvider":{}},"serverInfo":{"name":"arduino-language-server","version":"0.7.1"}}
09:58:34.083825 IDE <-- LS RESP initialize 0
09:58:34.083825 OUT Elapsed: 0s
09:58:34.088706 IN Elapsed: 4.8807ms
09:58:34.088706 IDE --> LS NOTIF initialized
09:58:34.088706                  initialized: Notification is not propagated to clangd
09:58:34.088706 IN Elapsed: 0s
09:58:34.088706 IDE --> LS NOTIF textDocument/didOpen
09:58:34.088706                  textDocument/didOpen: write-locked
09:58:34.088706                  textDocument/didOpen: (throttled: waiting for clangd)
09:58:34.088706                  textDocument/didOpen: unlocked (waiting clangd)
09:58:34.391198 INIT --- : Running build with: {
  "instance": {
    "id": 1
  },
  "fqbn": "arduino:avr:uno",
  "sketch_path": "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣器等等传感器\\Code\\Lesson 5_Active_buzzer\\5_Active_buzzer",
  "build_path": "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1379094214",
  "verbose": true,
  "create_compilation_database_only": true
}
09:58:36.764153 INIT --- : Compile successful!
09:58:36.765782 INIT --- : ERROR: updating libraries.cache: open C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1379094214\libraries.cache: The system cannot find the file specified.
09:58:36.765911 INIT --- : read-locked
09:58:36.765911 INIT --- : read-unlocked
09:58:37.073133 INIT --- : Running build with: {
  "instance": {
    "id": 1
  },
  "fqbn": "arduino:avr:uno",
  "sketch_path": "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣器等等传感器\\Code\\Lesson 5_Active_buzzer\\5_Active_buzzer",
  "build_path": "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764",
  "verbose": true,
  "create_compilation_database_only": true,
  "skip_libraries_discovery": true
}
09:58:37.399152 INIT --- : Compile successful!
09:58:37.743601 INIT --- : Arduino Data Dir -> c:\Users\Administrator\AppData\Local\Arduino15
09:58:37.745674 INIT --- :     Starting clangd: d:\Program Files\Arduino IDE\resources\app\node_modules\arduino-ide-extension\build\clangd.exe -log=verbose --compile-commands-dir=C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764 -query-driver=C:\Users\Administrator\AppData\Local\Arduino15\packages\**
09:58:37.790412 logging to g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\inols-clangd.log
09:58:37.790935 logging to g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\inols-clangd-err.log
09:58:37.790935 IDE     LS --> Clangd REQU initialize 1
09:58:37.792123 OUT Elapsed: 685.5µs
09:58:37.870991 IN Elapsed: 79.5534ms
09:58:37.870991 IDE     LS <-- Clangd RESP initialize 1
09:58:37.870991 INIT --- : clangd successfully started: {"capabilities":{"textDocumentSync":{"openClose":true,"change":2,"save":{}},"completionProvider":{"triggerCharacters":[".","\u003c","\u003e",":","\"","/","*"],"allCommitCharacters":[" ","\t","(",")","[","]","{","}","\u003c","\u003e",":",";",",","+","-","/","*","%","^","\u0026","#","?",".","=","\"","'","|"]},"hoverProvider":{},"signatureHelpProvider":{"triggerCharacters":["(",")","{","}","\u003c","\u003e",","]},"declarationProvider":{},"definitionProvider":{},"typeDefinitionProvider":{},"implementationProvider":{},"referencesProvider":{},"documentHighlightProvider":{},"documentSymbolProvider":{},"codeActionProvider":{"codeActionKinds":["quickfix","refactor","info"]},"documentLinkProvider":{},"documentFormattingProvider":{},"documentRangeFormattingProvider":{},"documentOnTypeFormattingProvider":{"firstTriggerCharacter":"\n"},"renameProvider":{"prepareProvider":true},"executeCommandProvider":{"commands":["clangd.applyFix","clangd.applyTweak"]},"selectionRangeProvider":{},"callHierarchyProvider":{},"semanticTokensProvider":{"legend":{"tokenTypes":["variable","variable","parameter","function","method","function","property","variable","class","interface","enum","enumMember","type","type","unknown","namespace","typeParameter","concept","type","macro","comment"],"tokenModifiers":["declaration","deprecated","deduced","readonly","static","abstract","virtual","dependentName","defaultLibrary","usedAsMutableReference","functionScope","classScope","fileScope","globalScope"]},"range":false,"full":{"delta":true}},"workspaceSymbolProvider":{}},"serverInfo":{"name":"clangd","version":"clangd version 14.0.0 windows x86_64-pc-windows-msvc"}}
09:58:37.870991 IDE     LS --> Clangd NOTIF initialized
09:58:37.871496 OUT Elapsed: 504.4µs
09:58:37.871531 INIT --- : Done initializing workbench
09:58:37.871531                  textDocument/didOpen: locked (waiting clangd)
09:58:37.872155                  textDocument/didOpen: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:58:37.875681                  textDocument/didOpen: Increasing .ino tracked files count to 1
09:58:37.877208 IDE     LS --> Clangd NOTIF textDocument/didOpen
09:58:37.877717 OUT Elapsed: 502.8µs
09:58:37.877717                  textDocument/didOpen: write-unlocked
09:58:37.877717 IN Elapsed: 0s
09:58:37.877717 IDE --> LS REQU textDocument/codeAction 1
09:58:37.877717                 textDocument/codeAction 1: read-locked
09:58:37.877717                 textDocument/codeAction 1: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:14:11)
09:58:37.878801                 textDocument/codeAction 1: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:58:37.882373 IN Elapsed: 11.3822ms
09:58:37.882373 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
09:58:37.882633                             textDocument/publishDiagnostics: Ignored by configuration
09:58:37.883151                 textDocument/codeAction 1:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:14:11)
09:58:37.883679 IDE     LS --> Clangd REQU textDocument/codeAction 2
09:58:37.883795 OUT Elapsed: 54.5µs
09:58:37.886835 IN Elapsed: 4.4615ms
09:58:37.886835 IDE     LS <-- Clangd REQU window/workDoneProgress/create 0
09:58:37.886835 IDE     LS --> Clangd RESP window/workDoneProgress/create 0
09:58:37.886835 IDE <-- LS REQU window/workDoneProgress/create 1
09:58:37.886835 OUT Elapsed: 0s
09:58:37.887376 IN Elapsed: 0s
09:58:37.887376 IDE     LS <-- Clangd NOTIF $/progress
09:58:37.887376                             $/progress: backgroundIndexProgress BEGIN indexing, 0.0%
09:58:37.887376 IN Elapsed: 0s
09:58:37.887376 IDE     LS <-- Clangd NOTIF $/progress
09:58:37.887376                             $/progress: backgroundIndexProgress REPORT, 0/1, 0.0%
09:58:37.887986 OUT Elapsed: 1.1516ms
09:58:37.895490 IN Elapsed: 8.1136ms
09:58:37.895490 IDE     LS <-- Clangd NOTIF $/progress
09:58:37.895490                             $/progress: backgroundIndexProgress REPORT, 0/27, 0.0%
09:58:37.895490 IN Elapsed: 0s
09:58:37.895490 IDE     LS <-- Clangd NOTIF $/progress
09:58:37.895490                             $/progress: backgroundIndexProgress REPORT, 0/27, 0.0%
09:58:37.895490 IN Elapsed: 0s
09:58:37.895490 IDE     LS <-- Clangd NOTIF $/progress
09:58:37.895490                             $/progress: backgroundIndexProgress REPORT, 0/27, 0.0%
09:58:37.895490 IN Elapsed: 0s
09:58:37.896000 IDE     LS <-- Clangd NOTIF $/progress
09:58:37.896000                             $/progress: backgroundIndexProgress REPORT, 0/27, 0.0%
09:58:37.896000 IN Elapsed: 0s
09:58:37.896000 IDE     LS <-- Clangd NOTIF $/progress
09:58:37.896000                             $/progress: backgroundIndexProgress REPORT, 1/27, 3.0%
09:58:37.896000 IN Elapsed: 0s
09:58:37.896000 IDE     LS <-- Clangd NOTIF $/progress
09:58:37.896000                             $/progress: backgroundIndexProgress REPORT, 1/27, 3.0%
09:58:37.896000 IN Elapsed: 0s
09:58:37.896000 IDE     LS <-- Clangd NOTIF $/progress
09:58:37.896000                             $/progress: backgroundIndexProgress REPORT, 1/27, 3.0%
09:58:37.896000 IN Elapsed: 0s
09:58:37.896000 IDE     LS <-- Clangd NOTIF $/progress
09:58:37.896000                             $/progress: backgroundIndexProgress REPORT, 1/27, 3.0%
09:58:38.217451 IN Elapsed: 321.4515ms
09:58:38.217967 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
09:58:38.217967 IN Elapsed: 0s
09:58:38.217967                             textDocument/publishDiagnostics: Ignored by configuration
09:58:38.217967 IDE     LS <-- Clangd RESP textDocument/codeAction 2
09:58:38.217967                 textDocument/codeAction 1: read-unlocked
09:58:38.217967 IDE <-- LS RESP textDocument/codeAction 1
09:58:38.217967 OUT Elapsed: 0s
09:58:38.217967 IN Elapsed: 0s
09:58:38.217967 IDE --> LS REQU textDocument/documentSymbol 2
09:58:38.217967                 textDocument/documentSymbol 2: read-locked
09:58:38.219506                 textDocument/documentSymbol 2: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:58:38.219506 IDE     LS --> Clangd REQU textDocument/documentSymbol 3
09:58:38.219506 OUT Elapsed: 0s
09:58:38.220028 IN Elapsed: 2.0606ms
09:58:38.220028 IDE     LS <-- Clangd RESP textDocument/documentSymbol 3
09:58:38.220028                 textDocument/documentSymbol 2: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
09:58:38.220028                 textDocument/documentSymbol 2:   > convert SymbolKind:Variable 4:0-4:12
09:58:38.221564                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:0-4:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-2:12 (.ino)
09:58:38.223325                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
09:58:38.223842                 textDocument/documentSymbol 2: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:58:38.223842                 textDocument/documentSymbol 2:   > convert SymbolKind:Variable 6:0-6:18
09:58:38.225379                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
09:58:38.226917                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
09:58:38.226917                 textDocument/documentSymbol 2: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:58:38.227426                 textDocument/documentSymbol 2:   > convert SymbolKind:Function 8:0-8:12
09:58:38.228956                 textDocument/documentSymbol 2: Range is in PREPROCESSED section of the sketch
09:58:38.228956                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
09:58:38.228956                 textDocument/documentSymbol 2:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:58:38.228956                 textDocument/documentSymbol 2:   > convert SymbolKind:Function 10:0-10:11
09:58:38.230489                 textDocument/documentSymbol 2: Range is in PREPROCESSED section of the sketch
09:58:38.230489                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
09:58:38.230999                 textDocument/documentSymbol 2:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:58:38.230999                 textDocument/documentSymbol 2:   > convert SymbolKind:Function 12:0-12:17
09:58:38.232532                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
09:58:38.234576                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
09:58:38.234576                 textDocument/documentSymbol 2: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:58:38.234576                 textDocument/documentSymbol 2:   > convert SymbolKind:Function 13:0-22:1
09:58:38.236108                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
09:58:38.238157                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
09:58:38.238157                 textDocument/documentSymbol 2: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:58:38.238157                 textDocument/documentSymbol 2: read-unlocked
09:58:38.238157 IDE <-- LS RESP textDocument/documentSymbol 2
09:58:38.238157 OUT Elapsed: 0s
09:58:38.238157 IN Elapsed: 0s
09:58:38.238157 IDE --> LS RESP window/workDoneProgress/create 1
09:58:38.239416 IDE <-- LS NOTIF $/progress
09:58:38.239416 OUT Elapsed: 0s
09:58:38.239416 IDE <-- LS NOTIF $/progress
09:58:38.239416 OUT Elapsed: 0s
09:58:38.707777 IN Elapsed: 487.7496ms
09:58:38.707777 IDE     LS <-- Clangd NOTIF $/progress
09:58:38.707777                             $/progress: backgroundIndexProgress REPORT, 2/27, 7.0%
09:58:38.707777 IN Elapsed: 0s
09:58:38.707777 IDE     LS <-- Clangd NOTIF $/progress
09:58:38.707777 IDE <-- LS NOTIF $/progress
09:58:38.707777 OUT Elapsed: 0s
09:58:38.707777                             $/progress: backgroundIndexProgress REPORT, 2/27, 7.0%
09:58:38.707777 IDE <-- LS NOTIF $/progress
09:58:38.707777 OUT Elapsed: 0s
09:58:38.763070 IN Elapsed: 55.2927ms
09:58:38.763070 IDE     LS <-- Clangd NOTIF $/progress
09:58:38.763070                             $/progress: backgroundIndexProgress REPORT, 3/27, 11.0%
09:58:38.763070 IN Elapsed: 0s
09:58:38.763070 IDE     LS <-- Clangd NOTIF $/progress
09:58:38.763070                             $/progress: backgroundIndexProgress REPORT, 3/27, 11.0%
09:58:38.763070 IDE <-- LS NOTIF $/progress
09:58:38.763070 OUT Elapsed: 0s
09:58:38.763070 IDE <-- LS NOTIF $/progress
09:58:38.763584 OUT Elapsed: 514.1µs
09:58:38.806457 IN Elapsed: 43.3869ms
09:58:38.806974 IDE     LS <-- Clangd NOTIF $/progress
09:58:38.806974                             $/progress: backgroundIndexProgress REPORT, 4/27, 14.0%
09:58:38.806974 IDE <-- LS NOTIF $/progress
09:58:38.807488 OUT Elapsed: 513.9µs
09:58:38.806974 IN Elapsed: 0s
09:58:38.807488 IDE     LS <-- Clangd NOTIF $/progress
09:58:38.807488                             $/progress: backgroundIndexProgress REPORT, 4/27, 14.0%
09:58:38.807488 IDE <-- LS NOTIF $/progress
09:58:38.807488 OUT Elapsed: 0s
09:58:38.907034 IN Elapsed: 99.5459ms
09:58:38.907034 IDE     LS <-- Clangd NOTIF $/progress
09:58:38.907034                             $/progress: backgroundIndexProgress REPORT, 5/27, 18.0%
09:58:38.907034 IN Elapsed: 0s
09:58:38.907034 IDE     LS <-- Clangd NOTIF $/progress
09:58:38.907034                             $/progress: backgroundIndexProgress REPORT, 5/27, 18.0%
09:58:38.912702 IN Elapsed: 5.6683ms
09:58:38.912702 IDE     LS <-- Clangd NOTIF $/progress
09:58:38.912702                             $/progress: backgroundIndexProgress REPORT, 6/27, 22.0%
09:58:38.913205 IN Elapsed: 503.5µs
09:58:38.913205 IDE     LS <-- Clangd NOTIF $/progress
09:58:38.913205                             $/progress: backgroundIndexProgress REPORT, 6/27, 22.0%
09:58:38.919274 IDE <-- LS NOTIF $/progress
09:58:38.919795 OUT Elapsed: 520.8µs
09:58:38.928884 IN Elapsed: 15.6784ms
09:58:38.928884 IDE     LS <-- Clangd NOTIF $/progress
09:58:38.928884                             $/progress: backgroundIndexProgress REPORT, 7/27, 25.0%
09:58:38.928884 IN Elapsed: 0s
09:58:38.928884 IDE     LS <-- Clangd NOTIF $/progress
09:58:38.928884                             $/progress: backgroundIndexProgress REPORT, 7/27, 25.0%
09:58:38.958809 IDE <-- LS NOTIF $/progress
09:58:38.958809 OUT Elapsed: 0s
09:58:39.021690 IN Elapsed: 92.8059ms
09:58:39.021690 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.021690                             $/progress: backgroundIndexProgress REPORT, 8/27, 29.0%
09:58:39.021690 IN Elapsed: 0s
09:58:39.021690 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.021690 IDE <-- LS NOTIF $/progress
09:58:39.021690                             $/progress: backgroundIndexProgress REPORT, 8/27, 29.0%
09:58:39.021690 OUT Elapsed: 0s
09:58:39.021690 IDE <-- LS NOTIF $/progress
09:58:39.022205 OUT Elapsed: 515.1µs
09:58:39.024294 IN Elapsed: 2.6048ms
09:58:39.024294 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.024294                             $/progress: backgroundIndexProgress REPORT, 9/27, 33.0%
09:58:39.024294 IDE <-- LS NOTIF $/progress
09:58:39.024294 IN Elapsed: 0s
09:58:39.024294 OUT Elapsed: 0s
09:58:39.024294 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.024294                             $/progress: backgroundIndexProgress REPORT, 9/27, 33.0%
09:58:39.024294 IDE <-- LS NOTIF $/progress
09:58:39.024807 OUT Elapsed: 512.2µs
09:58:39.054296 IN Elapsed: 30.0016ms
09:58:39.054828 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.054828                             $/progress: backgroundIndexProgress REPORT, 10/27, 37.0%
09:58:39.054828 IDE <-- LS NOTIF $/progress
09:58:39.054828 IN Elapsed: 0s
09:58:39.054828 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.054828                             $/progress: backgroundIndexProgress REPORT, 10/27, 37.0%
09:58:39.054828 OUT Elapsed: 0s
09:58:39.055331 IDE <-- LS NOTIF $/progress
09:58:39.055343 OUT Elapsed: 0s
09:58:39.059023 IN Elapsed: 4.1954ms
09:58:39.059534 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.059534                             $/progress: backgroundIndexProgress REPORT, 11/27, 40.0%
09:58:39.059534 IN Elapsed: 0s
09:58:39.059534 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.059534                             $/progress: backgroundIndexProgress REPORT, 11/27, 40.0%
09:58:39.059534 IDE <-- LS NOTIF $/progress
09:58:39.059534 OUT Elapsed: 0s
09:58:39.076243 IN Elapsed: 16.7087ms
09:58:39.076243 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.076243                             $/progress: backgroundIndexProgress REPORT, 12/27, 44.0%
09:58:39.076243 IN Elapsed: 0s
09:58:39.076243 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.076243 IDE <-- LS NOTIF $/progress
09:58:39.076243 OUT Elapsed: 0s
09:58:39.076243                             $/progress: backgroundIndexProgress REPORT, 12/27, 44.0%
09:58:39.076243 IDE <-- LS NOTIF $/progress
09:58:39.076243 OUT Elapsed: 0s
09:58:39.082461 IN Elapsed: 6.2185ms
09:58:39.082461 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.082461                             $/progress: backgroundIndexProgress REPORT, 13/27, 48.0%
09:58:39.082461 IN Elapsed: 0s
09:58:39.082461 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.082461                             $/progress: backgroundIndexProgress REPORT, 13/27, 48.0%
09:58:39.082461 IDE <-- LS NOTIF $/progress
09:58:39.082972 OUT Elapsed: 0s
09:58:39.082972 IDE <-- LS NOTIF $/progress
09:58:39.082972 OUT Elapsed: 0s
09:58:39.096623 IN Elapsed: 13.651ms
09:58:39.096623 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.096623                             $/progress: backgroundIndexProgress REPORT, 14/27, 51.0%
09:58:39.096623 IDE <-- LS NOTIF $/progress
09:58:39.096623 OUT Elapsed: 0s
09:58:39.096623 IN Elapsed: 0s
09:58:39.096623 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.096623                             $/progress: backgroundIndexProgress REPORT, 14/27, 51.0%
09:58:39.096623 IDE <-- LS NOTIF $/progress
09:58:39.096623 OUT Elapsed: 0s
09:58:39.103781 IN Elapsed: 7.1584ms
09:58:39.103781 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.104295                             $/progress: backgroundIndexProgress REPORT, 15/27, 55.0%
09:58:39.104295 IN Elapsed: 0s
09:58:39.104295 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.104295                             $/progress: backgroundIndexProgress REPORT, 15/27, 55.0%
09:58:39.104295 IDE <-- LS NOTIF $/progress
09:58:39.104295 OUT Elapsed: 0s
09:58:39.104812 IDE <-- LS NOTIF $/progress
09:58:39.104812 OUT Elapsed: 0s
09:58:39.144406 IN Elapsed: 40.111ms
09:58:39.144406 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.144406                             $/progress: backgroundIndexProgress REPORT, 16/27, 59.0%
09:58:39.144406 IDE <-- LS NOTIF $/progress
09:58:39.144406 IN Elapsed: 0s
09:58:39.144406 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.144406                             $/progress: backgroundIndexProgress REPORT, 16/27, 59.0%
09:58:39.144406 OUT Elapsed: 0s
09:58:39.144406 IDE <-- LS NOTIF $/progress
09:58:39.144406 OUT Elapsed: 0s
09:58:39.148687 IN Elapsed: 4.2808ms
09:58:39.148687 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.148687                             $/progress: backgroundIndexProgress REPORT, 17/27, 62.0%
09:58:39.148687 IN Elapsed: 0s
09:58:39.148687 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.148687                             $/progress: backgroundIndexProgress REPORT, 17/27, 62.0%
09:58:39.148687 IDE <-- LS NOTIF $/progress
09:58:39.148687 OUT Elapsed: 0s
09:58:39.148687 IDE <-- LS NOTIF $/progress
09:58:39.148687 OUT Elapsed: 0s
09:58:39.167905 IN Elapsed: 19.218ms
09:58:39.167905 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.167905                             $/progress: backgroundIndexProgress REPORT, 18/27, 66.0%
09:58:39.167905 IN Elapsed: 0s
09:58:39.167905 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.167905 IDE <-- LS NOTIF $/progress
09:58:39.167905 OUT Elapsed: 0s
09:58:39.167905                             $/progress: backgroundIndexProgress REPORT, 18/27, 66.0%
09:58:39.167905 IDE <-- LS NOTIF $/progress
09:58:39.167905 OUT Elapsed: 0s
09:58:39.175771 IN Elapsed: 7.8657ms
09:58:39.175771 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.176284                             $/progress: backgroundIndexProgress REPORT, 19/27, 70.0%
09:58:39.176284 IN Elapsed: 0s
09:58:39.176284 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.176284                             $/progress: backgroundIndexProgress REPORT, 19/27, 70.0%
09:58:39.176284 IDE <-- LS NOTIF $/progress
09:58:39.177308 OUT Elapsed: 511.7µs
09:58:39.178337 IN Elapsed: 2.0528ms
09:58:39.178337 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.178337                             $/progress: backgroundIndexProgress REPORT, 20/27, 74.0%
09:58:39.178337 IN Elapsed: 0s
09:58:39.178337 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.178337                             $/progress: backgroundIndexProgress REPORT, 20/27, 74.0%
09:58:39.178337 IDE <-- LS NOTIF $/progress
09:58:39.178849 OUT Elapsed: 0s
09:58:39.191233 IN Elapsed: 12.896ms
09:58:39.191760 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.191760                             $/progress: backgroundIndexProgress REPORT, 21/27, 77.0%
09:58:39.191760 IN Elapsed: 0s
09:58:39.191760 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.191760                             $/progress: backgroundIndexProgress REPORT, 21/27, 77.0%
09:58:39.191760 IDE <-- LS NOTIF $/progress
09:58:39.191760 OUT Elapsed: 0s
09:58:39.216460 IN Elapsed: 24.6999ms
09:58:39.216460 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.216460                             $/progress: backgroundIndexProgress REPORT, 22/27, 81.0%
09:58:39.216978 IDE <-- LS NOTIF $/progress
09:58:39.216978 OUT Elapsed: 0s
09:58:39.229046 IN Elapsed: 12.5868ms
09:58:39.229046 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.229046                             $/progress: backgroundIndexProgress REPORT, 23/27, 85.0%
09:58:39.229046 IDE <-- LS NOTIF $/progress
09:58:39.229046 OUT Elapsed: 0s
09:58:39.236448 IN Elapsed: 7.4015ms
09:58:39.236448 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.236448                             $/progress: backgroundIndexProgress REPORT, 24/27, 88.0%
09:58:39.236448 IDE <-- LS NOTIF $/progress
09:58:39.236448 OUT Elapsed: 0s
09:58:39.239838 IN Elapsed: 3.3904ms
09:58:39.239838 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.239838                             $/progress: backgroundIndexProgress REPORT, 25/27, 92.0%
09:58:39.239838 IDE <-- LS NOTIF $/progress
09:58:39.239838 OUT Elapsed: 0s
09:58:39.258525 IN Elapsed: 18.6871ms
09:58:39.258525 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.258525                             $/progress: backgroundIndexProgress REPORT, 26/27, 96.0%
09:58:39.258525 IDE <-- LS NOTIF $/progress
09:58:39.258525 OUT Elapsed: 0s
09:58:39.281386 IN Elapsed: 22.8607ms
09:58:39.281386 IDE     LS <-- Clangd NOTIF $/progress
09:58:39.281386                             $/progress: backgroundIndexProgress END 
09:58:39.281386 IDE <-- LS NOTIF $/progress
09:58:39.281386 OUT Elapsed: 0s
09:59:32.958357 IN Elapsed: 54.7201999s
09:59:32.958357 IDE --> LS REQU textDocument/hover 3
09:59:32.958357                 textDocument/hover 3: read-locked
09:59:32.959377                 textDocument/hover 3: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:32.962942                 textDocument/hover 3: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:9:6 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:16:6
09:59:32.962942 IDE     LS --> Clangd REQU textDocument/hover 4
09:59:32.962942 OUT Elapsed: 0s
09:59:32.970962 IN Elapsed: 53.6895762s
09:59:32.970962 IDE     LS <-- Clangd RESP textDocument/hover 4
09:59:32.970962                 textDocument/hover 3: null response
09:59:32.970962                 textDocument/hover 3: read-unlocked
09:59:32.970962 IDE <-- LS RESP textDocument/hover 3
09:59:32.971465 OUT Elapsed: 502.7µs
09:59:33.024609 IN Elapsed: 53.0947ms
09:59:33.024609 IDE --> LS REQU textDocument/documentHighlight 4
09:59:33.024609                 textDocument/documentHighlight 4: read-locked
09:59:33.026178                 textDocument/documentHighlight 4: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:33.029822                 textDocument/documentHighlight 4: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:9:6 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:16:6
09:59:33.029822 IDE     LS --> Clangd REQU textDocument/documentHighlight 5
09:59:33.029822 OUT Elapsed: 0s
09:59:33.030334 IN Elapsed: 59.3719ms
09:59:33.030334 IDE     LS <-- Clangd RESP textDocument/documentHighlight 5
09:59:33.030334                 textDocument/documentHighlight 4: read-unlocked
09:59:33.030334 IDE <-- LS RESP textDocument/documentHighlight 4
09:59:33.030334 OUT Elapsed: 0s
09:59:33.449702 IN Elapsed: 419.3674ms
09:59:33.449702 IDE --> LS REQU textDocument/codeAction 5
09:59:33.449702                 textDocument/codeAction 5: read-locked
09:59:33.449702                 textDocument/codeAction 5: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:9:5)
09:59:33.450805                 textDocument/codeAction 5: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:33.454551                 textDocument/codeAction 5:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:9:5)
09:59:33.454603 IDE     LS --> Clangd REQU textDocument/codeAction 6
09:59:33.454603 OUT Elapsed: 0s
09:59:33.455695 IN Elapsed: 425.3606ms
09:59:33.455695 IDE     LS <-- Clangd RESP textDocument/codeAction 6
09:59:33.455695                 textDocument/codeAction 5: read-unlocked
09:59:33.455695 IDE <-- LS RESP textDocument/codeAction 5
09:59:33.455695 OUT Elapsed: 0s
09:59:52.305724 IN Elapsed: 18.8500292s
09:59:52.305724 IDE --> LS REQU textDocument/documentSymbol 6
09:59:52.305967                 textDocument/documentSymbol 6: read-locked
09:59:52.307005                 textDocument/documentSymbol 6: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:52.307005 IDE     LS --> Clangd REQU textDocument/documentSymbol 7
09:59:52.307005 OUT Elapsed: 0s
09:59:52.311349 IN Elapsed: 18.8556541s
09:59:52.311349 IDE     LS <-- Clangd RESP textDocument/documentSymbol 7
09:59:52.311349                 textDocument/documentSymbol 6: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
09:59:52.311349                 textDocument/documentSymbol 6:   > convert SymbolKind:Variable 4:0-4:12
09:59:52.313393                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:0-4:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-2:12 (.ino)
09:59:52.314476                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
09:59:52.314476                 textDocument/documentSymbol 6: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.314476                 textDocument/documentSymbol 6:   > convert SymbolKind:Variable 6:0-6:18
09:59:52.316103                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
09:59:52.317721                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
09:59:52.317721                 textDocument/documentSymbol 6: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.317721                 textDocument/documentSymbol 6:   > convert SymbolKind:Function 8:0-8:12
09:59:52.319463                 textDocument/documentSymbol 6: Range is in PREPROCESSED section of the sketch
09:59:52.319463                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
09:59:52.319463                 textDocument/documentSymbol 6:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:52.319463                 textDocument/documentSymbol 6:   > convert SymbolKind:Function 10:0-10:11
09:59:52.321073                 textDocument/documentSymbol 6: Range is in PREPROCESSED section of the sketch
09:59:52.321073                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
09:59:52.321073                 textDocument/documentSymbol 6:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:52.321073                 textDocument/documentSymbol 6:   > convert SymbolKind:Function 12:0-12:17
09:59:52.322716                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
09:59:52.323809                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
09:59:52.324312                 textDocument/documentSymbol 6: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.324312                 textDocument/documentSymbol 6:   > convert SymbolKind:Function 13:0-22:1
09:59:52.325447                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
09:59:52.327079                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
09:59:52.327079                 textDocument/documentSymbol 6: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.327079                 textDocument/documentSymbol 6: read-unlocked
09:59:52.327079 IDE <-- LS RESP textDocument/documentSymbol 6
09:59:52.327079 OUT Elapsed: 0s
09:59:52.327582 IN Elapsed: 0s
09:59:52.327611 IDE --> LS NOTIF textDocument/didChange
09:59:52.327611                  textDocument/didChange: write-locked
09:59:52.327611                  textDocument/didChange: didChange(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino@2)
09:59:52.327611                  textDocument/didChange:   > 9:5-9:7 (len=2) -> "1"
09:59:52.328702                  textDocument/didChange: -----Tracked SKETCH file-----

#include "pitches.h"// notes in the melody:
int melody[] = {
NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};
int duration = 500;  // 500 miliseconds 
void setup() {  }
void loop() {
for (int thisNote = 0; thisNote < 12; thisNote++) {
// pin12 output the voice, every scale is 0.5 sencond 
tone(1, melody[thisNote], duration);
delay(100);
// Output the voice after several minutes
delay(100);
} // restart after two seconds 
delay(200);
}

-----------------------------
09:59:52.329763                  textDocument/didChange: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:52.334653 Ino Range: 9:5-9:7 -> Cpp Range:16:5-16:7
09:59:52.334653   > Current sketchmapper content:
09:59:52.334653   0: #include <Arduino.h>                                         | /not-ino:0                                         
09:59:52.335156   1: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:52.335188   2:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:0                          
09:59:52.335188   3: #include "pitches.h"// notes in the melody:                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:1                          
09:59:52.335188   4: int melody[] = {                                             | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:2                          
09:59:52.335188   5: NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:3                          
09:59:52.335188   6: int duration = 500;  // 500 miliseconds                      | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:4                          
09:59:52.335188   7: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:52.335188   8: void setup();                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5
09:59:52.335188   9: #line 7 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:52.335188  10: void loop();                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6
09:59:52.335188  11: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:52.335188  12: void setup() {  }                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5                          
09:59:52.335188  13: void loop() {                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6                          
09:59:52.335188  14: for (int thisNote = 0; thisNote < 12; thisNote++) {          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:7                          
09:59:52.335188  15: // pin12 output the voice, every scale is 0.5 sencond        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:8                          
09:59:52.335188  16: tone(1, melody[thisNote], duration);                         | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:9                          
09:59:52.335188  17: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:10                          
09:59:52.335188  18: // Output the voice after several minutes                    | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:11                          
09:59:52.335188  19: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:12                          
09:59:52.335188  20: } // restart after two seconds                               | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:13                          
09:59:52.335188  21: delay(200);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:14                          
09:59:52.335692  22: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:15                          
09:59:52.335707  23:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:16                          
09:59:52.335707  24:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:17                          
09:59:52.335707                  textDocument/didChange: to Clang: didChange(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp@2)
09:59:52.335707                  textDocument/didChange:             > 16:5-16:7 -> "1"
09:59:52.335707 IDE     LS --> Clangd NOTIF textDocument/didChange
09:59:52.335707 OUT Elapsed: 0s
09:59:52.335707                  textDocument/didChange: write-unlocked
09:59:52.335707 IN Elapsed: 0s
09:59:52.335707 IN Elapsed: 0s
09:59:52.335707 IDE --> LS REQU textDocument/documentSymbol 7
09:59:52.335707                 textDocument/documentSymbol 7: read-locked
09:59:52.336744                 textDocument/documentSymbol 7: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:52.336744 IDE     LS --> Clangd REQU textDocument/documentSymbol 8
09:59:52.337291 OUT Elapsed: 44.5µs
09:59:52.443329 IN Elapsed: 131.9799ms
09:59:52.443329 IDE     LS <-- Clangd RESP textDocument/documentSymbol 8
09:59:52.443329                 textDocument/documentSymbol 7: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
09:59:52.443329                 textDocument/documentSymbol 7:   > convert SymbolKind:Variable 4:0-4:12
09:59:52.444544 IN Elapsed: 1.2152ms
09:59:52.444544 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
09:59:52.444544                             textDocument/publishDiagnostics: Ignored by configuration
09:59:52.445631                 textDocument/documentSymbol 7: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:0-4:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-2:12 (.ino)
09:59:52.447216                 textDocument/documentSymbol 7: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
09:59:52.447246                 textDocument/documentSymbol 7: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.447246                 textDocument/documentSymbol 7:   > convert SymbolKind:Variable 6:0-6:18
09:59:52.448300                 textDocument/documentSymbol 7: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
09:59:52.449899                 textDocument/documentSymbol 7: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
09:59:52.449899                 textDocument/documentSymbol 7: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.449899                 textDocument/documentSymbol 7:   > convert SymbolKind:Function 8:0-8:12
09:59:52.451506                 textDocument/documentSymbol 7: Range is in PREPROCESSED section of the sketch
09:59:52.451506                 textDocument/documentSymbol 7: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
09:59:52.451506                 textDocument/documentSymbol 7:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:52.451506                 textDocument/documentSymbol 7:   > convert SymbolKind:Function 10:0-10:11
09:59:52.453054                 textDocument/documentSymbol 7: Range is in PREPROCESSED section of the sketch
09:59:52.453581                 textDocument/documentSymbol 7: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
09:59:52.453581                 textDocument/documentSymbol 7:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:52.453581                 textDocument/documentSymbol 7:   > convert SymbolKind:Function 12:0-12:17
09:59:52.455149                 textDocument/documentSymbol 7: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
09:59:52.456855                 textDocument/documentSymbol 7: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
09:59:52.456855                 textDocument/documentSymbol 7: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.456855                 textDocument/documentSymbol 7:   > convert SymbolKind:Function 13:0-22:1
09:59:52.458433                 textDocument/documentSymbol 7: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
09:59:52.460491                 textDocument/documentSymbol 7: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
09:59:52.460491                 textDocument/documentSymbol 7: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.460491                 textDocument/documentSymbol 7: read-unlocked
09:59:52.460491 IDE <-- LS RESP textDocument/documentSymbol 7
09:59:52.460491 OUT Elapsed: 0s
09:59:52.463605 IN Elapsed: 3.1138ms
09:59:52.464117 IDE --> LS REQU textDocument/documentSymbol 8
09:59:52.464117                 textDocument/documentSymbol 8: read-locked
09:59:52.465323                 textDocument/documentSymbol 8: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:52.465409 IDE     LS --> Clangd REQU textDocument/documentSymbol 9
09:59:52.465485 OUT Elapsed: 38.9µs
09:59:52.465628 IN Elapsed: 21.0841ms
09:59:52.465628 IDE     LS <-- Clangd RESP textDocument/documentSymbol 9
09:59:52.465628                 textDocument/documentSymbol 8: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
09:59:52.466131                 textDocument/documentSymbol 8:   > convert SymbolKind:Variable 4:0-4:12
09:59:52.467662                 textDocument/documentSymbol 8: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:0-4:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-2:12 (.ino)
09:59:52.468736                 textDocument/documentSymbol 8: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
09:59:52.469246                 textDocument/documentSymbol 8: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.469246                 textDocument/documentSymbol 8:   > convert SymbolKind:Variable 6:0-6:18
09:59:52.470780                 textDocument/documentSymbol 8: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
09:59:52.471844                 textDocument/documentSymbol 8: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
09:59:52.472347                 textDocument/documentSymbol 8: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.472387                 textDocument/documentSymbol 8:   > convert SymbolKind:Function 8:0-8:12
09:59:52.473449                 textDocument/documentSymbol 8: Range is in PREPROCESSED section of the sketch
09:59:52.473449                 textDocument/documentSymbol 8: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
09:59:52.473449                 textDocument/documentSymbol 8:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:52.473449                 textDocument/documentSymbol 8:   > convert SymbolKind:Function 10:0-10:11
09:59:52.475324                 textDocument/documentSymbol 8: Range is in PREPROCESSED section of the sketch
09:59:52.475324                 textDocument/documentSymbol 8: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
09:59:52.475324                 textDocument/documentSymbol 8:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:52.475324                 textDocument/documentSymbol 8:   > convert SymbolKind:Function 12:0-12:17
09:59:52.476904                 textDocument/documentSymbol 8: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
09:59:52.478500                 textDocument/documentSymbol 8: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
09:59:52.478500                 textDocument/documentSymbol 8: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.478500                 textDocument/documentSymbol 8:   > convert SymbolKind:Function 13:0-22:1
09:59:52.480091                 textDocument/documentSymbol 8: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
09:59:52.481713                 textDocument/documentSymbol 8: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
09:59:52.481713                 textDocument/documentSymbol 8: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.481713                 textDocument/documentSymbol 8: read-unlocked
09:59:52.481713 IDE <-- LS RESP textDocument/documentSymbol 8
09:59:52.481713 OUT Elapsed: 0s
09:59:52.481713 IN Elapsed: 0s
09:59:52.481713 IDE --> LS NOTIF textDocument/didChange
09:59:52.481713                  textDocument/didChange: write-locked
09:59:52.481713                  textDocument/didChange: didChange(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino@3)
09:59:52.482216                  textDocument/didChange:   > 9:6-9:6 (len=0) -> "4"
09:59:52.482792                  textDocument/didChange: -----Tracked SKETCH file-----

#include "pitches.h"// notes in the melody:
int melody[] = {
NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};
int duration = 500;  // 500 miliseconds 
void setup() {  }
void loop() {
for (int thisNote = 0; thisNote < 12; thisNote++) {
// pin12 output the voice, every scale is 0.5 sencond 
tone(14, melody[thisNote], duration);
delay(100);
// Output the voice after several minutes
delay(100);
} // restart after two seconds 
delay(200);
}

-----------------------------
09:59:52.483875                  textDocument/didChange: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:52.490099 Ino Range: 9:6-9:6 -> Cpp Range:16:6-16:6
09:59:52.490099   > Current sketchmapper content:
09:59:52.490099   0: #include <Arduino.h>                                         | /not-ino:0                                         
09:59:52.490099   1: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:52.490099   2:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:0                          
09:59:52.490099   3: #include "pitches.h"// notes in the melody:                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:1                          
09:59:52.490099   4: int melody[] = {                                             | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:2                          
09:59:52.490099   5: NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:3                          
09:59:52.490099   6: int duration = 500;  // 500 miliseconds                      | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:4                          
09:59:52.490099   7: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:52.490099   8: void setup();                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5
09:59:52.490099   9: #line 7 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:52.490099  10: void loop();                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6
09:59:52.490099  11: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:52.490099  12: void setup() {  }                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5                          
09:59:52.490099  13: void loop() {                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6                          
09:59:52.490099  14: for (int thisNote = 0; thisNote < 12; thisNote++) {          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:7                          
09:59:52.490099  15: // pin12 output the voice, every scale is 0.5 sencond        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:8                          
09:59:52.490099  16: tone(14, melody[thisNote], duration);                        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:9                          
09:59:52.490099  17: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:10                          
09:59:52.490613  18: // Output the voice after several minutes                    | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:11                          
09:59:52.490613  19: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:12                          
09:59:52.490613  20: } // restart after two seconds                               | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:13                          
09:59:52.490613  21: delay(200);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:14                          
09:59:52.490613  22: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:15                          
09:59:52.490613  23:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:16                          
09:59:52.490613  24:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:17                          
09:59:52.490613                  textDocument/didChange: to Clang: didChange(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp@3)
09:59:52.490613                  textDocument/didChange:             > 16:6-16:6 -> "4"
09:59:52.490613 IDE     LS --> Clangd NOTIF textDocument/didChange
09:59:52.490613 OUT Elapsed: 0s
09:59:52.490613                  textDocument/didChange: write-unlocked
09:59:52.490613 IN Elapsed: 0s
09:59:52.490613 IN Elapsed: 0s
09:59:52.490613 IDE --> LS REQU textDocument/documentSymbol 9
09:59:52.490613                 textDocument/documentSymbol 9: read-locked
09:59:52.491688                 textDocument/documentSymbol 9: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:52.491688 IDE     LS --> Clangd REQU textDocument/documentSymbol 10
09:59:52.492242 OUT Elapsed: 51.3µs
09:59:52.595069 IN Elapsed: 129.4406ms
09:59:52.595069 IDE     LS <-- Clangd RESP textDocument/documentSymbol 10
09:59:52.595069                 textDocument/documentSymbol 9: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
09:59:52.595069                 textDocument/documentSymbol 9:   > convert SymbolKind:Variable 4:0-4:12
09:59:52.596146 IN Elapsed: 1.0774ms
09:59:52.596146 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
09:59:52.596146                             textDocument/publishDiagnostics: Ignored by configuration
09:59:52.597161                 textDocument/documentSymbol 9: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:0-4:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-2:12 (.ino)
09:59:52.598972                 textDocument/documentSymbol 9: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
09:59:52.599475                 textDocument/documentSymbol 9: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.599512                 textDocument/documentSymbol 9:   > convert SymbolKind:Variable 6:0-6:18
09:59:52.601338                 textDocument/documentSymbol 9: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
09:59:52.602490                 textDocument/documentSymbol 9: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
09:59:52.602490                 textDocument/documentSymbol 9: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.602490                 textDocument/documentSymbol 9:   > convert SymbolKind:Function 8:0-8:12
09:59:52.604115                 textDocument/documentSymbol 9: Range is in PREPROCESSED section of the sketch
09:59:52.604115                 textDocument/documentSymbol 9: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
09:59:52.604115                 textDocument/documentSymbol 9:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:52.604115                 textDocument/documentSymbol 9:   > convert SymbolKind:Function 10:0-10:11
09:59:52.605738                 textDocument/documentSymbol 9: Range is in PREPROCESSED section of the sketch
09:59:52.605738                 textDocument/documentSymbol 9: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
09:59:52.605738                 textDocument/documentSymbol 9:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:52.605738                 textDocument/documentSymbol 9:   > convert SymbolKind:Function 12:0-12:17
09:59:52.607348                 textDocument/documentSymbol 9: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
09:59:52.608977                 textDocument/documentSymbol 9: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
09:59:52.608977                 textDocument/documentSymbol 9: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.608977                 textDocument/documentSymbol 9:   > convert SymbolKind:Function 13:0-22:1
09:59:52.610610                 textDocument/documentSymbol 9: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
09:59:52.612253                 textDocument/documentSymbol 9: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
09:59:52.612253                 textDocument/documentSymbol 9: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:52.612253                 textDocument/documentSymbol 9: read-unlocked
09:59:52.612253 IDE <-- LS RESP textDocument/documentSymbol 9
09:59:52.612253 OUT Elapsed: 0s
09:59:52.749020 IN Elapsed: 136.7669ms
09:59:52.749020 IDE --> LS REQU textDocument/codeAction 10
09:59:52.749020                 textDocument/codeAction 10: read-locked
09:59:52.749020                 textDocument/codeAction 10: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:9:7)
09:59:52.760616                 textDocument/codeAction 10: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:52.764803                 textDocument/codeAction 10:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:9:7)
09:59:52.765694 IDE     LS --> Clangd REQU textDocument/codeAction 11
09:59:52.765694 OUT Elapsed: 0s
09:59:52.765694 IN Elapsed: 169.5477ms
09:59:52.766232 IDE     LS <-- Clangd RESP textDocument/codeAction 11
09:59:52.766232                 textDocument/codeAction 10: read-unlocked
09:59:52.766232 IDE <-- LS RESP textDocument/codeAction 10
09:59:52.766232 OUT Elapsed: 0s
09:59:53.477252 IN Elapsed: 711.02ms
09:59:53.477252 IDE --> LS NOTIF textDocument/didSave
09:59:53.477918                  textDocument/didSave: write-locked
09:59:53.477918                  textDocument/didSave: notification is not forwarded to clang
09:59:53.477918                  textDocument/didSave: write-unlocked
09:59:54.486919 SKETCH REBUILD: : Sketch rebuild started
09:59:54.486919 IDE <-- LS REQU window/workDoneProgress/create 2
09:59:54.486919 SKETCH REBUILD: : read-locked
09:59:54.486919 SKETCH REBUILD: : read-unlocked
09:59:54.486919 OUT Elapsed: 0s
09:59:54.487422 IN Elapsed: 1.0090011s
09:59:54.487457 IDE --> LS RESP window/workDoneProgress/create 2
09:59:54.487457 IDE <-- LS NOTIF $/progress
09:59:54.487457 OUT Elapsed: 0s
09:59:54.798904 SKETCH REBUILD: : Running build with: {
  "instance": {
    "id": 1
  },
  "fqbn": "arduino:avr:uno",
  "sketch_path": "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣器等等传感器\\Code\\Lesson 5_Active_buzzer\\5_Active_buzzer",
  "build_path": "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764",
  "verbose": true,
  "create_compilation_database_only": true,
  "source_override": {
    "5_Active_buzzer.ino": "\r\n#include \"pitches.h\"// notes in the melody:\r\nint melody[] = {\r\nNOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};\r\nint duration = 500;  // 500 miliseconds \r\nvoid setup() {  }\r\nvoid loop() {\r\nfor (int thisNote = 0; thisNote \u003c 12; thisNote++) {\r\n// pin12 output the voice, every scale is 0.5 sencond \r\ntone(14, melody[thisNote], duration);\r\ndelay(100);\r\n// Output the voice after several minutes\r\ndelay(100);\r\n} // restart after two seconds \r\ndelay(200);\r\n}\r\n"
  },
  "skip_libraries_discovery": true
}
09:59:55.198557 SKETCH REBUILD: : Compile successful!
09:59:55.226995 SKETCH REBUILD: : write-locked
09:59:55.231399   > Current sketchmapper content:
09:59:55.231399   0: #include <Arduino.h>                                         | /not-ino:0                                         
09:59:55.231399   1: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:55.231399   2:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:0                          
09:59:55.231399   3: #include "pitches.h"// notes in the melody:                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:1                          
09:59:55.231399   4: int melody[] = {                                             | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:2                          
09:59:55.231399   5: NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:3                          
09:59:55.231399   6: int duration = 500;  // 500 miliseconds                      | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:4                          
09:59:55.231399   7: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:55.231399   8: void setup();                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5
09:59:55.231399   9: #line 7 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:55.231399  10: void loop();                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6
09:59:55.231399  11: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:55.231399  12: void setup() {  }                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5                          
09:59:55.231910  13: void loop() {                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6                          
09:59:55.231910  14: for (int thisNote = 0; thisNote < 12; thisNote++) {          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:7                          
09:59:55.231910  15: // pin12 output the voice, every scale is 0.5 sencond        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:8                          
09:59:55.231910  16: tone(14, melody[thisNote], duration);                        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:9                          
09:59:55.231910  17: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:10                          
09:59:55.231910  18: // Output the voice after several minutes                    | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:11                          
09:59:55.231910  19: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:12                          
09:59:55.231910  20: } // restart after two seconds                               | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:13                          
09:59:55.231910  21: delay(200);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:14                          
09:59:55.231910  22: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:15                          
09:59:55.231910  23:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:16                          
09:59:55.231910  24:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:17                          
09:59:55.231910 SKETCH REBUILD: : Sending 'didSave' notification to Clangd
09:59:55.231910 IDE     LS --> Clangd NOTIF textDocument/didSave
09:59:55.231910 OUT Elapsed: 0s
09:59:55.231910 SKETCH REBUILD: : Sending full-text 'didChange' notification to Clangd
09:59:55.231910 IDE     LS --> Clangd NOTIF textDocument/didChange
09:59:55.232414 OUT Elapsed: 503.9µs
09:59:55.232414 SKETCH REBUILD: : write-unlocked
09:59:55.232472 IDE <-- LS NOTIF $/progress
09:59:55.232472 OUT Elapsed: 0s
09:59:56.015585 IN Elapsed: 1.5281281s
09:59:56.015585 IDE --> LS REQU textDocument/documentSymbol 11
09:59:56.015585                 textDocument/documentSymbol 11: read-locked
09:59:56.017160                 textDocument/documentSymbol 11: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:56.017262 IDE     LS --> Clangd REQU textDocument/documentSymbol 12
09:59:56.017262 OUT Elapsed: 0s
09:59:56.017766 IN Elapsed: 3.2515341s
09:59:56.017837 IDE     LS <-- Clangd RESP textDocument/documentSymbol 12
09:59:56.017837                 textDocument/documentSymbol 11: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
09:59:56.017837                 textDocument/documentSymbol 11:   > convert SymbolKind:Variable 4:0-4:12
09:59:56.019496                 textDocument/documentSymbol 11: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:0-4:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-2:12 (.ino)
09:59:56.021088                 textDocument/documentSymbol 11: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
09:59:56.021088                 textDocument/documentSymbol 11: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:56.021088                 textDocument/documentSymbol 11:   > convert SymbolKind:Variable 6:0-6:18
09:59:56.023224                 textDocument/documentSymbol 11: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
09:59:56.024852                 textDocument/documentSymbol 11: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
09:59:56.024852                 textDocument/documentSymbol 11: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:56.024852                 textDocument/documentSymbol 11:   > convert SymbolKind:Function 8:0-8:12
09:59:56.025933                 textDocument/documentSymbol 11: Range is in PREPROCESSED section of the sketch
09:59:56.026436                 textDocument/documentSymbol 11: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
09:59:56.026471                 textDocument/documentSymbol 11:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:56.026471                 textDocument/documentSymbol 11:   > convert SymbolKind:Function 10:0-10:11
09:59:56.027555                 textDocument/documentSymbol 11: Range is in PREPROCESSED section of the sketch
09:59:56.027555                 textDocument/documentSymbol 11: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
09:59:56.027555                 textDocument/documentSymbol 11:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:56.028058                 textDocument/documentSymbol 11:   > convert SymbolKind:Function 12:0-12:17
09:59:56.029181                 textDocument/documentSymbol 11: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
09:59:56.030817                 textDocument/documentSymbol 11: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
09:59:56.030817                 textDocument/documentSymbol 11: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:56.030817                 textDocument/documentSymbol 11:   > convert SymbolKind:Function 13:0-22:1
09:59:56.032554                 textDocument/documentSymbol 11: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
09:59:56.033996                 textDocument/documentSymbol 11: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
09:59:56.033996                 textDocument/documentSymbol 11: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:56.033996                 textDocument/documentSymbol 11: read-unlocked
09:59:56.033996 IDE <-- LS RESP textDocument/documentSymbol 11
09:59:56.034525 OUT Elapsed: 528.8µs
09:59:56.034586 IN Elapsed: 0s
09:59:56.034586 IDE --> LS NOTIF textDocument/didChange
09:59:56.034641                  textDocument/didChange: write-locked
09:59:56.034696                  textDocument/didChange: didChange(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino@4)
09:59:56.034696                  textDocument/didChange:   > 9:5-9:7 (len=2) -> "12"
09:59:56.035469                  textDocument/didChange: -----Tracked SKETCH file-----

#include "pitches.h"// notes in the melody:
int melody[] = {
NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};
int duration = 500;  // 500 miliseconds 
void setup() {  }
void loop() {
for (int thisNote = 0; thisNote < 12; thisNote++) {
// pin12 output the voice, every scale is 0.5 sencond 
tone(12, melody[thisNote], duration);
delay(100);
// Output the voice after several minutes
delay(100);
} // restart after two seconds 
delay(200);
}

-----------------------------
09:59:56.036494                  textDocument/didChange: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:56.041695 Ino Range: 9:5-9:7 -> Cpp Range:16:5-16:7
09:59:56.041695   > Current sketchmapper content:
09:59:56.041695   0: #include <Arduino.h>                                         | /not-ino:0                                         
09:59:56.041695   1: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:56.041695   2:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:0                          
09:59:56.041695   3: #include "pitches.h"// notes in the melody:                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:1                          
09:59:56.041695   4: int melody[] = {                                             | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:2                          
09:59:56.041695   5: NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:3                          
09:59:56.042198   6: int duration = 500;  // 500 miliseconds                      | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:4                          
09:59:56.042198   7: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:56.042246   8: void setup();                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5
09:59:56.042246   9: #line 7 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:56.042246  10: void loop();                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6
09:59:56.042246  11: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:56.042246  12: void setup() {  }                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5                          
09:59:56.042246  13: void loop() {                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6                          
09:59:56.042246  14: for (int thisNote = 0; thisNote < 12; thisNote++) {          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:7                          
09:59:56.042246  15: // pin12 output the voice, every scale is 0.5 sencond        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:8                          
09:59:56.042246  16: tone(12, melody[thisNote], duration);                        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:9                          
09:59:56.042246  17: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:10                          
09:59:56.042246  18: // Output the voice after several minutes                    | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:11                          
09:59:56.042246  19: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:12                          
09:59:56.042246  20: } // restart after two seconds                               | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:13                          
09:59:56.042246  21: delay(200);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:14                          
09:59:56.042246  22: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:15                          
09:59:56.042246  23:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:16                          
09:59:56.042246  24:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:17                          
09:59:56.042246                  textDocument/didChange: to Clang: didChange(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp@5)
09:59:56.042246                  textDocument/didChange:             > 16:5-16:7 -> "12"
09:59:56.042246 IDE     LS --> Clangd NOTIF textDocument/didChange
09:59:56.042246 OUT Elapsed: 0s
09:59:56.042246                  textDocument/didChange: write-unlocked
09:59:56.195470 IN Elapsed: 177.6329ms
09:59:56.195470 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
09:59:56.195470                             textDocument/publishDiagnostics: Ignored by configuration
09:59:56.267667 IN Elapsed: 224.9194ms
09:59:56.267667 IDE --> LS REQU textDocument/codeAction 12
09:59:56.267667                 textDocument/codeAction 12: read-locked
09:59:56.267667                 textDocument/codeAction 12: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:9:5)
09:59:56.269257                 textDocument/codeAction 12: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:56.272887                 textDocument/codeAction 12:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:9:5)
09:59:56.272887 IDE     LS --> Clangd REQU textDocument/codeAction 13
09:59:56.272887 OUT Elapsed: 0s
09:59:56.272887 IN Elapsed: 77.4178ms
09:59:56.273391 IDE     LS <-- Clangd RESP textDocument/codeAction 13
09:59:56.273436                 textDocument/codeAction 12: read-unlocked
09:59:56.273436 IDE <-- LS RESP textDocument/codeAction 12
09:59:56.273436 OUT Elapsed: 0s
09:59:57.016596 IN Elapsed: 743.1603ms
09:59:57.016596 IDE --> LS NOTIF textDocument/didSave
09:59:57.016596                  textDocument/didSave: write-locked
09:59:57.016596                  textDocument/didSave: notification is not forwarded to clang
09:59:57.016596                  textDocument/didSave: write-unlocked
09:59:57.527503 IN Elapsed: 510.9068ms
09:59:57.527503 IDE --> LS REQU textDocument/documentSymbol 13
09:59:57.527503                 textDocument/documentSymbol 13: read-locked
09:59:57.528707                 textDocument/documentSymbol 13: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:57.528842 IDE     LS --> Clangd REQU textDocument/documentSymbol 14
09:59:57.528842 OUT Elapsed: 0s
09:59:57.532516 IN Elapsed: 1.259629s
09:59:57.532516 IDE     LS <-- Clangd RESP textDocument/documentSymbol 14
09:59:57.532516                 textDocument/documentSymbol 13: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
09:59:57.533045                 textDocument/documentSymbol 13:   > convert SymbolKind:Variable 4:0-4:12
09:59:57.534218                 textDocument/documentSymbol 13: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:0-4:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-2:12 (.ino)
09:59:57.535784                 textDocument/documentSymbol 13: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
09:59:57.535784                 textDocument/documentSymbol 13: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:57.535784                 textDocument/documentSymbol 13:   > convert SymbolKind:Variable 6:0-6:18
09:59:57.537352                 textDocument/documentSymbol 13: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
09:59:57.538972                 textDocument/documentSymbol 13: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
09:59:57.538972                 textDocument/documentSymbol 13: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:57.538972                 textDocument/documentSymbol 13:   > convert SymbolKind:Function 8:0-8:12
09:59:57.540062                 textDocument/documentSymbol 13: Range is in PREPROCESSED section of the sketch
09:59:57.540565                 textDocument/documentSymbol 13: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
09:59:57.540565                 textDocument/documentSymbol 13:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:57.540613                 textDocument/documentSymbol 13:   > convert SymbolKind:Function 10:0-10:11
09:59:57.541697                 textDocument/documentSymbol 13: Range is in PREPROCESSED section of the sketch
09:59:57.541697                 textDocument/documentSymbol 13: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
09:59:57.541697                 textDocument/documentSymbol 13:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:57.541697                 textDocument/documentSymbol 13:   > convert SymbolKind:Function 12:0-12:17
09:59:57.543326                 textDocument/documentSymbol 13: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
09:59:57.544921                 textDocument/documentSymbol 13: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
09:59:57.544921                 textDocument/documentSymbol 13: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:57.544921                 textDocument/documentSymbol 13:   > convert SymbolKind:Function 13:0-22:1
09:59:57.546451                 textDocument/documentSymbol 13: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
09:59:57.547996                 textDocument/documentSymbol 13: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
09:59:57.547996                 textDocument/documentSymbol 13: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:57.547996                 textDocument/documentSymbol 13: read-unlocked
09:59:57.547996 IDE <-- LS RESP textDocument/documentSymbol 13
09:59:57.547996 OUT Elapsed: 0s
09:59:57.547996 IN Elapsed: 0s
09:59:57.547996 IDE --> LS NOTIF textDocument/didChange
09:59:57.547996                  textDocument/didChange: write-locked
09:59:57.547996                  textDocument/didChange: didChange(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino@5)
09:59:57.548507                  textDocument/didChange:   > 9:5-9:7 (len=2) -> "1"
09:59:57.549560                  textDocument/didChange: -----Tracked SKETCH file-----

#include "pitches.h"// notes in the melody:
int melody[] = {
NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};
int duration = 500;  // 500 miliseconds 
void setup() {  }
void loop() {
for (int thisNote = 0; thisNote < 12; thisNote++) {
// pin12 output the voice, every scale is 0.5 sencond 
tone(1, melody[thisNote], duration);
delay(100);
// Output the voice after several minutes
delay(100);
} // restart after two seconds 
delay(200);
}

-----------------------------
09:59:57.550095                  textDocument/didChange: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:57.555505 Ino Range: 9:5-9:7 -> Cpp Range:16:5-16:7
09:59:57.555505   > Current sketchmapper content:
09:59:57.555505   0: #include <Arduino.h>                                         | /not-ino:0                                         
09:59:57.555505   1: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:57.556008   2:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:0                          
09:59:57.556121   3: #include "pitches.h"// notes in the melody:                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:1                          
09:59:57.556185   4: int melody[] = {                                             | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:2                          
09:59:57.556185   5: NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:3                          
09:59:57.556185   6: int duration = 500;  // 500 miliseconds                      | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:4                          
09:59:57.556185   7: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:57.556249   8: void setup();                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5
09:59:57.556249   9: #line 7 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:57.556304  10: void loop();                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6
09:59:57.556304  11: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:57.556304  12: void setup() {  }                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5                          
09:59:57.556360  13: void loop() {                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6                          
09:59:57.556360  14: for (int thisNote = 0; thisNote < 12; thisNote++) {          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:7                          
09:59:57.556360  15: // pin12 output the voice, every scale is 0.5 sencond        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:8                          
09:59:57.556422  16: tone(1, melody[thisNote], duration);                         | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:9                          
09:59:57.556422  17: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:10                          
09:59:57.556422  18: // Output the voice after several minutes                    | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:11                          
09:59:57.556478  19: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:12                          
09:59:57.556478  20: } // restart after two seconds                               | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:13                          
09:59:57.556478  21: delay(200);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:14                          
09:59:57.556528  22: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:15                          
09:59:57.556528  23:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:16                          
09:59:57.556528  24:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:17                          
09:59:57.556528                  textDocument/didChange: to Clang: didChange(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp@6)
09:59:57.556604                  textDocument/didChange:             > 16:5-16:7 -> "1"
09:59:57.556604 IDE     LS --> Clangd NOTIF textDocument/didChange
09:59:57.556726 OUT Elapsed: 64.9µs
09:59:57.556757                  textDocument/didChange: write-unlocked
09:59:57.556757 IN Elapsed: 0s
09:59:57.556757 IN Elapsed: 0s
09:59:57.556757 IDE --> LS REQU textDocument/documentSymbol 14
09:59:57.556757                 textDocument/documentSymbol 14: read-locked
09:59:57.557846                 textDocument/documentSymbol 14: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:57.557846 IDE     LS --> Clangd REQU textDocument/documentSymbol 15
09:59:57.557846 OUT Elapsed: 0s
09:59:57.562810 IN Elapsed: 30.2933ms
09:59:57.562810 IDE     LS <-- Clangd REQU window/workDoneProgress/create 1
09:59:57.562810 IDE     LS --> Clangd RESP window/workDoneProgress/create 1
09:59:57.562810 IDE <-- LS REQU window/workDoneProgress/create 3
09:59:57.562810 OUT Elapsed: 0s
09:59:57.562810 OUT Elapsed: 0s
09:59:57.562810 IN Elapsed: 0s
09:59:57.563356 IDE     LS <-- Clangd NOTIF $/progress
09:59:57.563356                             $/progress: backgroundIndexProgress BEGIN indexing, 0.0%
09:59:57.563356 IN Elapsed: 0s
09:59:57.563356 IDE     LS <-- Clangd NOTIF $/progress
09:59:57.563356                             $/progress: backgroundIndexProgress REPORT, 0/1, 0.0%
09:59:57.610371 IN Elapsed: 47.0154ms
09:59:57.610371 IDE     LS <-- Clangd NOTIF $/progress
09:59:57.610371                             $/progress: backgroundIndexProgress REPORT, 0/1, 0.0%
09:59:57.610371 IN Elapsed: 0s
09:59:57.610371 IDE     LS <-- Clangd NOTIF $/progress
09:59:57.610371                             $/progress: backgroundIndexProgress END 
09:59:57.670782 IN Elapsed: 60.4111ms
09:59:57.670782 IDE     LS <-- Clangd RESP textDocument/documentSymbol 15
09:59:57.670782                 textDocument/documentSymbol 14: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
09:59:57.670782                 textDocument/documentSymbol 14:   > convert SymbolKind:Variable 4:0-4:12
09:59:57.671851 IN Elapsed: 1.0685ms
09:59:57.672354 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
09:59:57.672379                             textDocument/publishDiagnostics: Ignored by configuration
09:59:57.672379                 textDocument/documentSymbol 14: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:0-4:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-2:12 (.ino)
09:59:57.673917                 textDocument/documentSymbol 14: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
09:59:57.674420                 textDocument/documentSymbol 14: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:57.674453                 textDocument/documentSymbol 14:   > convert SymbolKind:Variable 6:0-6:18
09:59:57.675532                 textDocument/documentSymbol 14: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
09:59:57.677127                 textDocument/documentSymbol 14: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
09:59:57.677127                 textDocument/documentSymbol 14: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:57.677127                 textDocument/documentSymbol 14:   > convert SymbolKind:Function 8:0-8:12
09:59:57.678702                 textDocument/documentSymbol 14: Range is in PREPROCESSED section of the sketch
09:59:57.678702                 textDocument/documentSymbol 14: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
09:59:57.678702                 textDocument/documentSymbol 14:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:57.678702                 textDocument/documentSymbol 14:   > convert SymbolKind:Function 10:0-10:11
09:59:57.680252                 textDocument/documentSymbol 14: Range is in PREPROCESSED section of the sketch
09:59:57.680252                 textDocument/documentSymbol 14: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
09:59:57.680252                 textDocument/documentSymbol 14:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:57.680252                 textDocument/documentSymbol 14:   > convert SymbolKind:Function 12:0-12:17
09:59:57.681799                 textDocument/documentSymbol 14: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
09:59:57.684092                 textDocument/documentSymbol 14: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
09:59:57.684164                 textDocument/documentSymbol 14: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:57.684164                 textDocument/documentSymbol 14:   > convert SymbolKind:Function 13:0-22:1
09:59:57.685767                 textDocument/documentSymbol 14: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
09:59:57.687370                 textDocument/documentSymbol 14: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
09:59:57.687370                 textDocument/documentSymbol 14: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:57.687370                 textDocument/documentSymbol 14: read-unlocked
09:59:57.687370 IDE <-- LS RESP textDocument/documentSymbol 14
09:59:57.687370 OUT Elapsed: 0s
09:59:57.687370 IN Elapsed: 0s
09:59:57.687370 IDE --> LS RESP window/workDoneProgress/create 3
09:59:57.687370 IDE <-- LS NOTIF $/progress
09:59:57.687881 OUT Elapsed: 511.4µs
09:59:57.687881 IDE <-- LS NOTIF $/progress
09:59:57.687881 OUT Elapsed: 0s
09:59:57.772153 IN Elapsed: 84.7825ms
09:59:57.772153 IDE --> LS REQU textDocument/codeAction 15
09:59:57.772153                 textDocument/codeAction 15: read-locked
09:59:57.772153                 textDocument/codeAction 15: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:9:6)
09:59:57.773216                 textDocument/codeAction 15: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:57.777030                 textDocument/codeAction 15:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:9:6)
09:59:57.777030 IDE     LS --> Clangd REQU textDocument/codeAction 16
09:59:57.777030 OUT Elapsed: 0s
09:59:57.777030 IN Elapsed: 104.6511ms
09:59:57.777542 IDE     LS <-- Clangd RESP textDocument/codeAction 16
09:59:57.777542                 textDocument/codeAction 15: read-unlocked
09:59:57.777542 IDE <-- LS RESP textDocument/codeAction 15
09:59:57.777542 OUT Elapsed: 0s
09:59:57.908920 IN Elapsed: 131.3781ms
09:59:57.908920 IDE --> LS REQU textDocument/documentSymbol 16
09:59:57.909435                 textDocument/documentSymbol 16: read-locked
09:59:57.910563                 textDocument/documentSymbol 16: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:57.910601 IDE     LS --> Clangd REQU textDocument/documentSymbol 17
09:59:57.910646 OUT Elapsed: 0s
09:59:57.910646 IN Elapsed: 133.616ms
09:59:57.911159 IDE     LS <-- Clangd RESP textDocument/documentSymbol 17
09:59:57.911159                 textDocument/documentSymbol 16: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
09:59:57.911159                 textDocument/documentSymbol 16:   > convert SymbolKind:Variable 4:0-4:12
09:59:57.912691                 textDocument/documentSymbol 16: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:0-4:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-2:12 (.ino)
09:59:57.914249                 textDocument/documentSymbol 16: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
09:59:57.914249                 textDocument/documentSymbol 16: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:57.914249                 textDocument/documentSymbol 16:   > convert SymbolKind:Variable 6:0-6:18
09:59:57.915859                 textDocument/documentSymbol 16: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
09:59:57.916941                 textDocument/documentSymbol 16: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
09:59:57.916941                 textDocument/documentSymbol 16: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:57.916941                 textDocument/documentSymbol 16:   > convert SymbolKind:Function 8:0-8:12
09:59:57.919080                 textDocument/documentSymbol 16: Range is in PREPROCESSED section of the sketch
09:59:57.919080                 textDocument/documentSymbol 16: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
09:59:57.919080                 textDocument/documentSymbol 16:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:57.919080                 textDocument/documentSymbol 16:   > convert SymbolKind:Function 10:0-10:11
09:59:57.920649                 textDocument/documentSymbol 16: Range is in PREPROCESSED section of the sketch
09:59:57.920649                 textDocument/documentSymbol 16: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
09:59:57.920649                 textDocument/documentSymbol 16:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:57.920649                 textDocument/documentSymbol 16:   > convert SymbolKind:Function 12:0-12:17
09:59:57.922184                 textDocument/documentSymbol 16: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
09:59:57.924146                 textDocument/documentSymbol 16: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
09:59:57.924146                 textDocument/documentSymbol 16: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:57.924146                 textDocument/documentSymbol 16:   > convert SymbolKind:Function 13:0-22:1
09:59:57.925737                 textDocument/documentSymbol 16: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
09:59:57.926852                 textDocument/documentSymbol 16: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
09:59:57.926852                 textDocument/documentSymbol 16: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:57.926852                 textDocument/documentSymbol 16: read-unlocked
09:59:57.926852 IDE <-- LS RESP textDocument/documentSymbol 16
09:59:57.927355 OUT Elapsed: 502.7µs
09:59:57.927403 IN Elapsed: 48.3µs
09:59:57.927403 IDE --> LS NOTIF textDocument/didChange
09:59:57.927403                  textDocument/didChange: write-locked
09:59:57.927403                  textDocument/didChange: didChange(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino@6)
09:59:57.927403                  textDocument/didChange:   > 9:6-9:6 (len=0) -> "4"
09:59:57.928490                  textDocument/didChange: -----Tracked SKETCH file-----

#include "pitches.h"// notes in the melody:
int melody[] = {
NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};
int duration = 500;  // 500 miliseconds 
void setup() {  }
void loop() {
for (int thisNote = 0; thisNote < 12; thisNote++) {
// pin12 output the voice, every scale is 0.5 sencond 
tone(14, melody[thisNote], duration);
delay(100);
// Output the voice after several minutes
delay(100);
} // restart after two seconds 
delay(200);
}

-----------------------------
09:59:57.929578                  textDocument/didChange: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:57.935073 Ino Range: 9:6-9:6 -> Cpp Range:16:6-16:6
09:59:57.935073   > Current sketchmapper content:
09:59:57.935073   0: #include <Arduino.h>                                         | /not-ino:0                                         
09:59:57.935073   1: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:57.935073   2:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:0                          
09:59:57.935073   3: #include "pitches.h"// notes in the melody:                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:1                          
09:59:57.935073   4: int melody[] = {                                             | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:2                          
09:59:57.935586   5: NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:3                          
09:59:57.935586   6: int duration = 500;  // 500 miliseconds                      | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:4                          
09:59:57.935586   7: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:57.935586   8: void setup();                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5
09:59:57.935586   9: #line 7 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:57.935586  10: void loop();                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6
09:59:57.935586  11: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
09:59:57.935586  12: void setup() {  }                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5                          
09:59:57.935586  13: void loop() {                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6                          
09:59:57.935586  14: for (int thisNote = 0; thisNote < 12; thisNote++) {          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:7                          
09:59:57.935586  15: // pin12 output the voice, every scale is 0.5 sencond        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:8                          
09:59:57.935586  16: tone(14, melody[thisNote], duration);                        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:9                          
09:59:57.935586  17: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:10                          
09:59:57.935586  18: // Output the voice after several minutes                    | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:11                          
09:59:57.935586  19: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:12                          
09:59:57.935586  20: } // restart after two seconds                               | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:13                          
09:59:57.935586  21: delay(200);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:14                          
09:59:57.935586  22: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:15                          
09:59:57.935586  23:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:16                          
09:59:57.935586  24:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:17                          
09:59:57.935586                  textDocument/didChange: to Clang: didChange(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp@7)
09:59:57.935586                  textDocument/didChange:             > 16:6-16:6 -> "4"
09:59:57.935586 IDE     LS --> Clangd NOTIF textDocument/didChange
09:59:57.936098 OUT Elapsed: 511.4µs
09:59:57.936098                  textDocument/didChange: write-unlocked
09:59:57.936098 IN Elapsed: 0s
09:59:57.936098 IN Elapsed: 0s
09:59:57.936098 IDE --> LS REQU textDocument/documentSymbol 17
09:59:57.936098                 textDocument/documentSymbol 17: read-locked
09:59:57.937121                 textDocument/documentSymbol 17: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:57.937121 IDE     LS --> Clangd REQU textDocument/documentSymbol 18
09:59:57.937121 OUT Elapsed: 0s
09:59:58.038965 IN Elapsed: 127.8063ms
09:59:58.039053 IDE     LS <-- Clangd RESP textDocument/documentSymbol 18
09:59:58.039053                 textDocument/documentSymbol 17: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
09:59:58.039053                 textDocument/documentSymbol 17:   > convert SymbolKind:Variable 4:0-4:12
09:59:58.039941 IN Elapsed: 888.3µs
09:59:58.040205 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
09:59:58.040205                             textDocument/publishDiagnostics: Ignored by configuration
09:59:58.041054                 textDocument/documentSymbol 17: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:0-4:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-2:12 (.ino)
09:59:58.042243                 textDocument/documentSymbol 17: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
09:59:58.042243                 textDocument/documentSymbol 17: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:58.042243                 textDocument/documentSymbol 17:   > convert SymbolKind:Variable 6:0-6:18
09:59:58.043890                 textDocument/documentSymbol 17: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
09:59:58.045566                 textDocument/documentSymbol 17: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
09:59:58.045566                 textDocument/documentSymbol 17: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:58.045566                 textDocument/documentSymbol 17:   > convert SymbolKind:Function 8:0-8:12
09:59:58.047194                 textDocument/documentSymbol 17: Range is in PREPROCESSED section of the sketch
09:59:58.047194                 textDocument/documentSymbol 17: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
09:59:58.047194                 textDocument/documentSymbol 17:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:58.047194                 textDocument/documentSymbol 17:   > convert SymbolKind:Function 10:0-10:11
09:59:58.048834                 textDocument/documentSymbol 17: Range is in PREPROCESSED section of the sketch
09:59:58.048834                 textDocument/documentSymbol 17: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
09:59:58.048834                 textDocument/documentSymbol 17:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
09:59:58.048834                 textDocument/documentSymbol 17:   > convert SymbolKind:Function 12:0-12:17
09:59:58.050437                 textDocument/documentSymbol 17: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
09:59:58.051534                 textDocument/documentSymbol 17: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
09:59:58.052037                 textDocument/documentSymbol 17: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:58.052037                 textDocument/documentSymbol 17:   > convert SymbolKind:Function 13:0-22:1
09:59:58.053138                 textDocument/documentSymbol 17: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
09:59:58.054697                 textDocument/documentSymbol 17: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
09:59:58.054697                 textDocument/documentSymbol 17: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
09:59:58.054697                 textDocument/documentSymbol 17: read-unlocked
09:59:58.055200 IDE <-- LS RESP textDocument/documentSymbol 17
09:59:58.055382 OUT Elapsed: 0s
09:59:58.166680 IN Elapsed: 111.2985ms
09:59:58.166680 IDE --> LS REQU textDocument/codeAction 18
09:59:58.166680                 textDocument/codeAction 18: read-locked
09:59:58.166680                 textDocument/codeAction 18: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:9:7)
09:59:58.167765                 textDocument/codeAction 18: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
09:59:58.171522                 textDocument/codeAction 18:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:9:7)
09:59:58.171578 IDE     LS --> Clangd REQU textDocument/codeAction 19
09:59:58.171707 OUT Elapsed: 62.7µs
09:59:58.171707 IN Elapsed: 131.5023ms
09:59:58.171707 IDE     LS <-- Clangd RESP textDocument/codeAction 19
09:59:58.171707                 textDocument/codeAction 18: read-unlocked
09:59:58.171707 IDE <-- LS RESP textDocument/codeAction 18
09:59:58.172211 OUT Elapsed: 503.3µs
09:59:58.913882 IN Elapsed: 741.6443ms
09:59:58.913882 IDE --> LS NOTIF textDocument/didSave
09:59:58.913882                  textDocument/didSave: write-locked
09:59:58.913882                  textDocument/didSave: notification is not forwarded to clang
09:59:58.913882                  textDocument/didSave: write-unlocked
09:59:59.928193 SKETCH REBUILD: : Sketch rebuild started
09:59:59.928316 IDE <-- LS REQU window/workDoneProgress/create 4
09:59:59.928316 SKETCH REBUILD: : read-locked
09:59:59.928316 OUT Elapsed: 0s
09:59:59.928316 SKETCH REBUILD: : read-unlocked
09:59:59.928316 IN Elapsed: 1.0144344s
09:59:59.928316 IDE --> LS RESP window/workDoneProgress/create 4
09:59:59.928820 IDE <-- LS NOTIF $/progress
09:59:59.928867 OUT Elapsed: 0s
10:00:00.240486 SKETCH REBUILD: : Running build with: {
  "instance": {
    "id": 1
  },
  "fqbn": "arduino:avr:uno",
  "sketch_path": "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣器等等传感器\\Code\\Lesson 5_Active_buzzer\\5_Active_buzzer",
  "build_path": "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764",
  "verbose": true,
  "create_compilation_database_only": true,
  "source_override": {
    "5_Active_buzzer.ino": "\r\n#include \"pitches.h\"// notes in the melody:\r\nint melody[] = {\r\nNOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};\r\nint duration = 500;  // 500 miliseconds \r\nvoid setup() {  }\r\nvoid loop() {\r\nfor (int thisNote = 0; thisNote \u003c 12; thisNote++) {\r\n// pin12 output the voice, every scale is 0.5 sencond \r\ntone(14, melody[thisNote], duration);\r\ndelay(100);\r\n// Output the voice after several minutes\r\ndelay(100);\r\n} // restart after two seconds \r\ndelay(200);\r\n}\r\n"
  },
  "skip_libraries_discovery": true
}
10:00:00.628277 SKETCH REBUILD: : Compile successful!
10:00:00.657677 SKETCH REBUILD: : write-locked
10:00:00.661934   > Current sketchmapper content:
10:00:00.661934   0: #include <Arduino.h>                                         | /not-ino:0                                         
10:00:00.661934   1: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:00.661934   2:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:0                          
10:00:00.661934   3: #include "pitches.h"// notes in the melody:                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:1                          
10:00:00.661934   4: int melody[] = {                                             | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:2                          
10:00:00.661934   5: NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:3                          
10:00:00.661934   6: int duration = 500;  // 500 miliseconds                      | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:4                          
10:00:00.661934   7: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:00.661934   8: void setup();                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5
10:00:00.661934   9: #line 7 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:00.661934  10: void loop();                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6
10:00:00.661934  11: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:00.661934  12: void setup() {  }                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5                          
10:00:00.661934  13: void loop() {                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6                          
10:00:00.661934  14: for (int thisNote = 0; thisNote < 12; thisNote++) {          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:7                          
10:00:00.661934  15: // pin12 output the voice, every scale is 0.5 sencond        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:8                          
10:00:00.661934  16: tone(14, melody[thisNote], duration);                        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:9                          
10:00:00.661934  17: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:10                          
10:00:00.661934  18: // Output the voice after several minutes                    | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:11                          
10:00:00.661934  19: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:12                          
10:00:00.661934  20: } // restart after two seconds                               | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:13                          
10:00:00.661934  21: delay(200);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:14                          
10:00:00.661934  22: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:15                          
10:00:00.661934  23:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:16                          
10:00:00.661934  24:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:17                          
10:00:00.661934 SKETCH REBUILD: : Sending 'didSave' notification to Clangd
10:00:00.662931 IDE     LS --> Clangd NOTIF textDocument/didSave
10:00:00.662931 OUT Elapsed: 0s
10:00:00.662931 SKETCH REBUILD: : Sending full-text 'didChange' notification to Clangd
10:00:00.662931 IDE     LS --> Clangd NOTIF textDocument/didChange
10:00:00.662931 OUT Elapsed: 0s
10:00:00.662931 SKETCH REBUILD: : write-unlocked
10:00:00.662931 IDE <-- LS NOTIF $/progress
10:00:00.662931 OUT Elapsed: 0s
10:00:14.741252 IN Elapsed: 14.8129355s
10:00:14.741252 IDE --> LS REQU textDocument/hover 19
10:00:14.741878                 textDocument/hover 19: read-locked
10:00:14.748497                 textDocument/hover 19: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:14.753292                 textDocument/hover 19: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:9:7 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:16:7
10:00:14.753292 IDE     LS --> Clangd REQU textDocument/hover 20
10:00:14.753292 OUT Elapsed: 0s
10:00:14.765640 IN Elapsed: 16.5939329s
10:00:14.765640 IDE     LS <-- Clangd RESP textDocument/hover 20
10:00:14.767265                 textDocument/hover 19: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:16:7-16:8 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:9:7-9:8 (.ino)
10:00:14.767265                 textDocument/hover 19: Hover content: "### function `tone`  \n\n---\n→ `void`  \nParameters:  \n- `uint8_t _pin`\n- `unsigned int frequency`\n- `unsigned long duration = 0`\n\nfrequency (in hertz) and duration (in milliseconds).  \n\n---\n```cpp\nvoid tone(uint8_t _pin, unsigned int frequency, unsigned long duration = 0)\n```"
10:00:14.767265                 textDocument/hover 19: read-unlocked
10:00:14.767265 IDE <-- LS RESP textDocument/hover 19
10:00:14.767265 OUT Elapsed: 0s
10:00:15.043029 IN Elapsed: 275.7637ms
10:00:15.043029 IDE --> LS REQU textDocument/documentHighlight 20
10:00:15.043029                 textDocument/documentHighlight 20: read-locked
10:00:15.044081                 textDocument/documentHighlight 20: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:15.047746                 textDocument/documentHighlight 20: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:9:7 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:16:7
10:00:15.047746 IDE     LS --> Clangd REQU textDocument/documentHighlight 21
10:00:15.047746 OUT Elapsed: 0s
10:00:15.048292 IN Elapsed: 282.6517ms
10:00:15.048850 IDE     LS <-- Clangd RESP textDocument/documentHighlight 21
10:00:15.049956                 textDocument/documentHighlight 20: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:16:0-16:4 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:9:0-9:4 (.ino)
10:00:15.050459                 textDocument/documentHighlight 20: read-unlocked
10:00:15.050492 IDE <-- LS RESP textDocument/documentHighlight 20
10:00:15.050492 OUT Elapsed: 0s
10:00:15.396927 IN Elapsed: 346.4354ms
10:00:15.396927 IDE --> LS REQU textDocument/codeAction 21
10:00:15.396927                 textDocument/codeAction 21: read-locked
10:00:15.396927                 textDocument/codeAction 21: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:9:6)
10:00:15.398276                 textDocument/codeAction 21: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:15.401403                 textDocument/codeAction 21:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:9:6)
10:00:15.401403 IDE     LS --> Clangd REQU textDocument/codeAction 22
10:00:15.401931 OUT Elapsed: 528.5µs
10:00:15.401931 IN Elapsed: 353.1367ms
10:00:15.401931 IDE     LS <-- Clangd RESP textDocument/codeAction 22
10:00:15.401931                 textDocument/codeAction 21: read-unlocked
10:00:15.401931 IDE <-- LS RESP textDocument/codeAction 21
10:00:15.402435 OUT Elapsed: 503.6µs
10:00:15.689927 IN Elapsed: 287.4921ms
10:00:15.689927 IDE --> LS REQU textDocument/hover 22
10:00:15.689927                 textDocument/hover 22: read-locked
10:00:15.690994                 textDocument/hover 22: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:15.694783                 textDocument/hover 22: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:9:5 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:16:5
10:00:15.694783 IDE     LS --> Clangd REQU textDocument/hover 23
10:00:15.694783 OUT Elapsed: 0s
10:00:15.698034 IN Elapsed: 296.1032ms
10:00:15.698034 IDE     LS <-- Clangd RESP textDocument/hover 23
10:00:15.698034                 textDocument/hover 22: null response
10:00:15.698034                 textDocument/hover 22: read-unlocked
10:00:15.698034 IDE <-- LS RESP textDocument/hover 22
10:00:15.698034 OUT Elapsed: 0s
10:00:16.301740 IN Elapsed: 603.7052ms
10:00:16.301740 IDE --> LS REQU textDocument/documentSymbol 23
10:00:16.301740                 textDocument/documentSymbol 23: read-locked
10:00:16.303430                 textDocument/documentSymbol 23: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:16.303430 IDE     LS --> Clangd REQU textDocument/documentSymbol 24
10:00:16.303430 OUT Elapsed: 0s
10:00:16.304014 IN Elapsed: 605.9799ms
10:00:16.304014 IDE     LS <-- Clangd RESP textDocument/documentSymbol 24
10:00:16.304014                 textDocument/documentSymbol 23: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
10:00:16.304014                 textDocument/documentSymbol 23:   > convert SymbolKind:Variable 4:0-4:12
10:00:16.305626                 textDocument/documentSymbol 23: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:0-4:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-2:12 (.ino)
10:00:16.307262                 textDocument/documentSymbol 23: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
10:00:16.307262                 textDocument/documentSymbol 23: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:16.307262                 textDocument/documentSymbol 23:   > convert SymbolKind:Variable 6:0-6:18
10:00:16.308885                 textDocument/documentSymbol 23: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
10:00:16.310033                 textDocument/documentSymbol 23: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
10:00:16.310033                 textDocument/documentSymbol 23: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:16.310536                 textDocument/documentSymbol 23:   > convert SymbolKind:Function 8:0-8:12
10:00:16.311654                 textDocument/documentSymbol 23: Range is in PREPROCESSED section of the sketch
10:00:16.311654                 textDocument/documentSymbol 23: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
10:00:16.311654                 textDocument/documentSymbol 23:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
10:00:16.311654                 textDocument/documentSymbol 23:   > convert SymbolKind:Function 10:0-10:11
10:00:16.313254                 textDocument/documentSymbol 23: Range is in PREPROCESSED section of the sketch
10:00:16.313254                 textDocument/documentSymbol 23: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
10:00:16.313254                 textDocument/documentSymbol 23:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
10:00:16.313254                 textDocument/documentSymbol 23:   > convert SymbolKind:Function 12:0-12:17
10:00:16.314887                 textDocument/documentSymbol 23: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
10:00:16.316528                 textDocument/documentSymbol 23: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
10:00:16.316528                 textDocument/documentSymbol 23: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:16.316528                 textDocument/documentSymbol 23:   > convert SymbolKind:Function 13:0-22:1
10:00:16.317615                 textDocument/documentSymbol 23: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
10:00:16.319260                 textDocument/documentSymbol 23: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
10:00:16.319260                 textDocument/documentSymbol 23: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:16.319260                 textDocument/documentSymbol 23: read-unlocked
10:00:16.319800 IDE <-- LS RESP textDocument/documentSymbol 23
10:00:16.319800 OUT Elapsed: 0s
10:00:16.319800 IN Elapsed: 0s
10:00:16.319800 IDE --> LS NOTIF textDocument/didChange
10:00:16.319800                  textDocument/didChange: write-locked
10:00:16.319800                  textDocument/didChange: didChange(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino@7)
10:00:16.319800                  textDocument/didChange:   > 9:6-9:7 (len=1) -> "2"
10:00:16.320932                  textDocument/didChange: -----Tracked SKETCH file-----

#include "pitches.h"// notes in the melody:
int melody[] = {
NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};
int duration = 500;  // 500 miliseconds 
void setup() {  }
void loop() {
for (int thisNote = 0; thisNote < 12; thisNote++) {
// pin12 output the voice, every scale is 0.5 sencond 
tone(12, melody[thisNote], duration);
delay(100);
// Output the voice after several minutes
delay(100);
} // restart after two seconds 
delay(200);
}

-----------------------------
10:00:16.322093                  textDocument/didChange: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:16.327501 Ino Range: 9:6-9:7 -> Cpp Range:16:6-16:7
10:00:16.327501   > Current sketchmapper content:
10:00:16.327501   0: #include <Arduino.h>                                         | /not-ino:0                                         
10:00:16.327501   1: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:16.327501   2:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:0                          
10:00:16.327501   3: #include "pitches.h"// notes in the melody:                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:1                          
10:00:16.327501   4: int melody[] = {                                             | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:2                          
10:00:16.327501   5: NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:3                          
10:00:16.327501   6: int duration = 500;  // 500 miliseconds                      | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:4                          
10:00:16.327501   7: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:16.327501   8: void setup();                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5
10:00:16.327501   9: #line 7 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:16.327501  10: void loop();                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6
10:00:16.328004  11: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:16.328004  12: void setup() {  }                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5                          
10:00:16.328034  13: void loop() {                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6                          
10:00:16.328034  14: for (int thisNote = 0; thisNote < 12; thisNote++) {          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:7                          
10:00:16.328034  15: // pin12 output the voice, every scale is 0.5 sencond        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:8                          
10:00:16.328034  16: tone(12, melody[thisNote], duration);                        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:9                          
10:00:16.328034  17: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:10                          
10:00:16.328034  18: // Output the voice after several minutes                    | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:11                          
10:00:16.328034  19: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:12                          
10:00:16.328034  20: } // restart after two seconds                               | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:13                          
10:00:16.328034  21: delay(200);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:14                          
10:00:16.328034  22: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:15                          
10:00:16.328034  23:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:16                          
10:00:16.328034  24:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:17                          
10:00:16.328034                  textDocument/didChange: to Clang: didChange(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp@9)
10:00:16.328034                  textDocument/didChange:             > 16:6-16:7 -> "2"
10:00:16.328034 IDE     LS --> Clangd NOTIF textDocument/didChange
10:00:16.328034 OUT Elapsed: 0s
10:00:16.328034                  textDocument/didChange: write-unlocked
10:00:16.328034 IN Elapsed: 0s
10:00:16.328034 IN Elapsed: 0s
10:00:16.328034 IDE --> LS REQU textDocument/documentSymbol 24
10:00:16.328544                 textDocument/documentSymbol 24: read-locked
10:00:16.329081                 textDocument/documentSymbol 24: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:16.329081 IDE     LS --> Clangd REQU textDocument/documentSymbol 25
10:00:16.329598 OUT Elapsed: 0s
10:00:16.333599 IN Elapsed: 29.5846ms
10:00:16.333599 IDE     LS <-- Clangd REQU window/workDoneProgress/create 2
10:00:16.334572 IDE     LS --> Clangd RESP window/workDoneProgress/create 2
10:00:16.334572 OUT Elapsed: 0s
10:00:16.334572 IDE <-- LS REQU window/workDoneProgress/create 5
10:00:16.334572 OUT Elapsed: 0s
10:00:16.334572 IN Elapsed: 0s
10:00:16.334572 IDE     LS <-- Clangd NOTIF $/progress
10:00:16.334572                             $/progress: backgroundIndexProgress BEGIN indexing, 0.0%
10:00:16.334572 IN Elapsed: 0s
10:00:16.334572 IDE     LS <-- Clangd NOTIF $/progress
10:00:16.334572                             $/progress: backgroundIndexProgress REPORT, 0/1, 0.0%
10:00:16.382103 IN Elapsed: 47.5312ms
10:00:16.382103 IDE     LS <-- Clangd NOTIF $/progress
10:00:16.382103                             $/progress: backgroundIndexProgress REPORT, 0/1, 0.0%
10:00:16.382103 IN Elapsed: 0s
10:00:16.382103 IDE     LS <-- Clangd NOTIF $/progress
10:00:16.382103                             $/progress: backgroundIndexProgress END 
10:00:16.436177 IN Elapsed: 54.0737ms
10:00:16.436680 IDE     LS <-- Clangd RESP textDocument/documentSymbol 25
10:00:16.436711                 textDocument/documentSymbol 24: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
10:00:16.436711                 textDocument/documentSymbol 24:   > convert SymbolKind:Variable 4:0-4:12
10:00:16.437246 IN Elapsed: 1.0688ms
10:00:16.437246 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
10:00:16.437813                             textDocument/publishDiagnostics: Ignored by configuration
10:00:16.438458                 textDocument/documentSymbol 24: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:0-4:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-2:12 (.ino)
10:00:16.439971                 textDocument/documentSymbol 24: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
10:00:16.439971                 textDocument/documentSymbol 24: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:16.439971                 textDocument/documentSymbol 24:   > convert SymbolKind:Variable 6:0-6:18
10:00:16.441144                 textDocument/documentSymbol 24: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
10:00:16.442796                 textDocument/documentSymbol 24: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
10:00:16.442796                 textDocument/documentSymbol 24: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:16.442796                 textDocument/documentSymbol 24:   > convert SymbolKind:Function 8:0-8:12
10:00:16.444431                 textDocument/documentSymbol 24: Range is in PREPROCESSED section of the sketch
10:00:16.444431                 textDocument/documentSymbol 24: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
10:00:16.444431                 textDocument/documentSymbol 24:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
10:00:16.444431                 textDocument/documentSymbol 24:   > convert SymbolKind:Function 10:0-10:11
10:00:16.445961                 textDocument/documentSymbol 24: Range is in PREPROCESSED section of the sketch
10:00:16.445961                 textDocument/documentSymbol 24: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
10:00:16.445961                 textDocument/documentSymbol 24:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
10:00:16.445961                 textDocument/documentSymbol 24:   > convert SymbolKind:Function 12:0-12:17
10:00:16.447490                 textDocument/documentSymbol 24: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
10:00:16.449019                 textDocument/documentSymbol 24: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
10:00:16.449019                 textDocument/documentSymbol 24: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:16.449019                 textDocument/documentSymbol 24:   > convert SymbolKind:Function 13:0-22:1
10:00:16.450584                 textDocument/documentSymbol 24: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
10:00:16.452137                 textDocument/documentSymbol 24: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
10:00:16.452137                 textDocument/documentSymbol 24: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:16.452137                 textDocument/documentSymbol 24: read-unlocked
10:00:16.452137 IDE <-- LS RESP textDocument/documentSymbol 24
10:00:16.452137 OUT Elapsed: 0s
10:00:16.452650 IN Elapsed: 513.3µs
10:00:16.452650 IDE --> LS RESP window/workDoneProgress/create 5
10:00:16.452650 IDE <-- LS NOTIF $/progress
10:00:16.452650 OUT Elapsed: 0s
10:00:16.452650 IDE <-- LS NOTIF $/progress
10:00:16.452650 OUT Elapsed: 0s
10:00:16.552241 IN Elapsed: 99.5909ms
10:00:16.552241 IDE --> LS REQU textDocument/codeAction 25
10:00:16.552241                 textDocument/codeAction 25: read-locked
10:00:16.552241                 textDocument/codeAction 25: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:9:7)
10:00:16.553591                 textDocument/codeAction 25: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:16.557276                 textDocument/codeAction 25:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:9:7)
10:00:16.557308 IDE     LS --> Clangd REQU textDocument/codeAction 26
10:00:16.557308 OUT Elapsed: 0s
10:00:16.557308 IN Elapsed: 119.4953ms
10:00:16.557308 IDE     LS <-- Clangd RESP textDocument/codeAction 26
10:00:16.557308                 textDocument/codeAction 25: read-unlocked
10:00:16.557308 IDE <-- LS RESP textDocument/codeAction 25
10:00:16.557843 OUT Elapsed: 534.4µs
10:00:17.303635 IN Elapsed: 745.7925ms
10:00:17.303635 IDE --> LS NOTIF textDocument/didSave
10:00:17.303635                  textDocument/didSave: write-locked
10:00:17.303635                  textDocument/didSave: notification is not forwarded to clang
10:00:17.303635                  textDocument/didSave: write-unlocked
10:00:17.461203 IN Elapsed: 157.5674ms
10:00:17.461203 IDE --> LS REQU textDocument/documentHighlight 26
10:00:17.461203                 textDocument/documentHighlight 26: read-locked
10:00:17.462374                 textDocument/documentHighlight 26: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:17.465995                 textDocument/documentHighlight 26: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:13:19 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:20:19
10:00:17.465995 IDE     LS --> Clangd REQU textDocument/documentHighlight 27
10:00:17.465995 OUT Elapsed: 0s
10:00:17.466507 IN Elapsed: 909.1982ms
10:00:17.466507 IDE     LS <-- Clangd RESP textDocument/documentHighlight 27
10:00:17.466507                 textDocument/documentHighlight 26: read-unlocked
10:00:17.466507 IDE <-- LS RESP textDocument/documentHighlight 26
10:00:17.466507 OUT Elapsed: 0s
10:00:17.714521 IN Elapsed: 248.0145ms
10:00:17.714654 IDE --> LS REQU textDocument/codeAction 27
10:00:17.714654                 textDocument/codeAction 27: read-locked
10:00:17.714654                 textDocument/codeAction 27: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:13:19)
10:00:17.716235                 textDocument/codeAction 27: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:17.719443                 textDocument/codeAction 27:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:19)
10:00:17.719443 IDE     LS --> Clangd REQU textDocument/codeAction 28
10:00:17.719983 OUT Elapsed: 539.8µs
10:00:17.719983 IN Elapsed: 253.4761ms
10:00:17.719983 IDE     LS <-- Clangd RESP textDocument/codeAction 28
10:00:17.719983                 textDocument/codeAction 27: read-unlocked
10:00:17.719983 IDE <-- LS RESP textDocument/codeAction 27
10:00:17.720486 OUT Elapsed: 503.7µs
10:00:18.133948 IN Elapsed: 413.4615ms
10:00:18.133948 IDE --> LS REQU textDocument/definition 28
10:00:18.133948                 textDocument/definition 28: read-locked
10:00:18.135038                 textDocument/definition 28: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:18.138777                 textDocument/definition 28: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:13:19 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:20:19
10:00:18.138777 IDE     LS --> Clangd REQU textDocument/definition 29
10:00:18.138850 OUT Elapsed: 0s
10:00:18.138850 IN Elapsed: 418.8677ms
10:00:18.138850 IDE     LS <-- Clangd RESP textDocument/definition 29
10:00:18.138850                 textDocument/definition 28: read-unlocked
10:00:18.138850 IDE <-- LS RESP textDocument/definition 28
10:00:18.139354 OUT Elapsed: 503.4µs
10:00:18.315090 SKETCH REBUILD: : Sketch rebuild started
10:00:18.315090 SKETCH REBUILD: : read-locked
10:00:18.315090 SKETCH REBUILD: : read-unlocked
10:00:18.315090 IDE <-- LS REQU window/workDoneProgress/create 6
10:00:18.315090 OUT Elapsed: 0s
10:00:18.315595 IN Elapsed: 176.1947ms
10:00:18.315652 IDE --> LS RESP window/workDoneProgress/create 6
10:00:18.315709 IDE <-- LS NOTIF $/progress
10:00:18.315709 OUT Elapsed: 0s
10:00:18.400482 IN Elapsed: 84.7739ms
10:00:18.400482 IDE --> LS REQU textDocument/documentSymbol 29
10:00:18.400482                 textDocument/documentSymbol 29: read-locked
10:00:18.401537                 textDocument/documentSymbol 29: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:18.401537 IDE     LS --> Clangd REQU textDocument/documentSymbol 30
10:00:18.402078 OUT Elapsed: 540.5µs
10:00:18.402078 IN Elapsed: 263.2272ms
10:00:18.402615 IDE     LS <-- Clangd RESP textDocument/documentSymbol 30
10:00:18.402615                 textDocument/documentSymbol 29: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
10:00:18.402615                 textDocument/documentSymbol 29:   > convert SymbolKind:Variable 4:0-4:12
10:00:18.404170                 textDocument/documentSymbol 29: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:0-4:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-2:12 (.ino)
10:00:18.405932                 textDocument/documentSymbol 29: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
10:00:18.405932                 textDocument/documentSymbol 29: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:18.405932                 textDocument/documentSymbol 29:   > convert SymbolKind:Variable 6:0-6:18
10:00:18.407551                 textDocument/documentSymbol 29: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
10:00:18.409960                 textDocument/documentSymbol 29: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
10:00:18.409960                 textDocument/documentSymbol 29: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:18.409960                 textDocument/documentSymbol 29:   > convert SymbolKind:Function 8:0-8:12
10:00:18.411580                 textDocument/documentSymbol 29: Range is in PREPROCESSED section of the sketch
10:00:18.411580                 textDocument/documentSymbol 29: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
10:00:18.411580                 textDocument/documentSymbol 29:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
10:00:18.411580                 textDocument/documentSymbol 29:   > convert SymbolKind:Function 10:0-10:11
10:00:18.412995                 textDocument/documentSymbol 29: Range is in PREPROCESSED section of the sketch
10:00:18.412995                 textDocument/documentSymbol 29: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
10:00:18.412995                 textDocument/documentSymbol 29:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
10:00:18.412995                 textDocument/documentSymbol 29:   > convert SymbolKind:Function 12:0-12:17
10:00:18.414587                 textDocument/documentSymbol 29: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
10:00:18.416207                 textDocument/documentSymbol 29: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
10:00:18.416207                 textDocument/documentSymbol 29: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:18.416207                 textDocument/documentSymbol 29:   > convert SymbolKind:Function 13:0-22:1
10:00:18.417834                 textDocument/documentSymbol 29: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
10:00:18.419546                 textDocument/documentSymbol 29: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
10:00:18.419606                 textDocument/documentSymbol 29: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:18.419606                 textDocument/documentSymbol 29: read-unlocked
10:00:18.419664 IDE <-- LS RESP textDocument/documentSymbol 29
10:00:18.419722 OUT Elapsed: 57.9µs
10:00:18.419794 IN Elapsed: 0s
10:00:18.419794 IDE --> LS NOTIF textDocument/didChange
10:00:18.419850                  textDocument/didChange: write-locked
10:00:18.419910                  textDocument/didChange: didChange(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino@8)
10:00:18.419910                  textDocument/didChange:   > 9:6-9:7 (len=1) -> "4"
10:00:18.421365                  textDocument/didChange: -----Tracked SKETCH file-----

#include "pitches.h"// notes in the melody:
int melody[] = {
NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};
int duration = 500;  // 500 miliseconds 
void setup() {  }
void loop() {
for (int thisNote = 0; thisNote < 12; thisNote++) {
// pin12 output the voice, every scale is 0.5 sencond 
tone(14, melody[thisNote], duration);
delay(100);
// Output the voice after several minutes
delay(100);
} // restart after two seconds 
delay(200);
}

-----------------------------
10:00:18.422443                  textDocument/didChange: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:18.427442 Ino Range: 9:6-9:7 -> Cpp Range:16:6-16:7
10:00:18.427442   > Current sketchmapper content:
10:00:18.428439   0: #include <Arduino.h>                                         | /not-ino:0                                         
10:00:18.428439   1: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:18.428439   2:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:0                          
10:00:18.428439   3: #include "pitches.h"// notes in the melody:                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:1                          
10:00:18.428439   4: int melody[] = {                                             | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:2                          
10:00:18.428439   5: NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:3                          
10:00:18.428439   6: int duration = 500;  // 500 miliseconds                      | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:4                          
10:00:18.428439   7: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:18.428439   8: void setup();                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5
10:00:18.428439   9: #line 7 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:18.428439  10: void loop();                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6
10:00:18.428439  11: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:18.428439  12: void setup() {  }                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5                          
10:00:18.428439  13: void loop() {                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6                          
10:00:18.428439  14: for (int thisNote = 0; thisNote < 12; thisNote++) {          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:7                          
10:00:18.428439  15: // pin12 output the voice, every scale is 0.5 sencond        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:8                          
10:00:18.428439  16: tone(14, melody[thisNote], duration);                        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:9                          
10:00:18.428439  17: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:10                          
10:00:18.428439  18: // Output the voice after several minutes                    | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:11                          
10:00:18.428439  19: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:12                          
10:00:18.428439  20: } // restart after two seconds                               | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:13                          
10:00:18.428439  21: delay(200);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:14                          
10:00:18.428439  22: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:15                          
10:00:18.428439  23:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:16                          
10:00:18.428439  24:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:17                          
10:00:18.428439                  textDocument/didChange: to Clang: didChange(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp@10)
10:00:18.428439                  textDocument/didChange:             > 16:6-16:7 -> "4"
10:00:18.428439 IDE     LS --> Clangd NOTIF textDocument/didChange
10:00:18.428439 OUT Elapsed: 0s
10:00:18.428439                  textDocument/didChange: write-unlocked
10:00:18.592566 IN Elapsed: 164.127ms
10:00:18.593071 IDE --> LS REQU textDocument/documentSymbol 30
10:00:18.593225                 textDocument/documentSymbol 30: read-locked
10:00:18.594262                 textDocument/documentSymbol 30: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:18.594262 IDE     LS --> Clangd REQU textDocument/documentSymbol 31
10:00:18.594262 OUT Elapsed: 0s
10:00:18.597815 IN Elapsed: 195.1996ms
10:00:18.597815 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
10:00:18.597815                             textDocument/publishDiagnostics: Ignored by configuration
10:00:18.598325 IN Elapsed: 510.3µs
10:00:18.598325 IDE     LS <-- Clangd RESP textDocument/documentSymbol 31
10:00:18.598325                 textDocument/documentSymbol 30: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
10:00:18.598325                 textDocument/documentSymbol 30:   > convert SymbolKind:Variable 4:0-4:12
10:00:18.599976                 textDocument/documentSymbol 30: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:0-4:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-2:12 (.ino)
10:00:18.601538                 textDocument/documentSymbol 30: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
10:00:18.601538                 textDocument/documentSymbol 30: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:18.601538                 textDocument/documentSymbol 30:   > convert SymbolKind:Variable 6:0-6:18
10:00:18.603213                 textDocument/documentSymbol 30: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
10:00:18.604819                 textDocument/documentSymbol 30: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
10:00:18.604819                 textDocument/documentSymbol 30: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:18.604819                 textDocument/documentSymbol 30:   > convert SymbolKind:Function 8:0-8:12
10:00:18.606480                 textDocument/documentSymbol 30: Range is in PREPROCESSED section of the sketch
10:00:18.606529                 textDocument/documentSymbol 30: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
10:00:18.606529                 textDocument/documentSymbol 30:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
10:00:18.606529                 textDocument/documentSymbol 30:   > convert SymbolKind:Function 10:0-10:11
10:00:18.607760                 textDocument/documentSymbol 30: Range is in PREPROCESSED section of the sketch
10:00:18.607760                 textDocument/documentSymbol 30: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
10:00:18.607760                 textDocument/documentSymbol 30:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
10:00:18.607760                 textDocument/documentSymbol 30:   > convert SymbolKind:Function 12:0-12:17
10:00:18.609326                 textDocument/documentSymbol 30: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
10:00:18.610967                 textDocument/documentSymbol 30: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
10:00:18.610967                 textDocument/documentSymbol 30: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:18.610967                 textDocument/documentSymbol 30:   > convert SymbolKind:Function 13:0-22:1
10:00:18.612502                 textDocument/documentSymbol 30: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
10:00:18.614035                 textDocument/documentSymbol 30: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
10:00:18.614035                 textDocument/documentSymbol 30: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:00:18.614035                 textDocument/documentSymbol 30: read-unlocked
10:00:18.614035 IDE <-- LS RESP textDocument/documentSymbol 30
10:00:18.614548 OUT Elapsed: 0s
10:00:18.614548 IN Elapsed: 0s
10:00:18.614548 IDE --> LS NOTIF textDocument/didChange
10:00:18.614548                  textDocument/didChange: write-locked
10:00:18.614548                  textDocument/didChange: didChange(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino@9)
10:00:18.614548                  textDocument/didChange:   > 9:5-9:7 (len=2) -> "12"
10:00:18.615576                  textDocument/didChange: -----Tracked SKETCH file-----

#include "pitches.h"// notes in the melody:
int melody[] = {
NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};
int duration = 500;  // 500 miliseconds 
void setup() {  }
void loop() {
for (int thisNote = 0; thisNote < 12; thisNote++) {
// pin12 output the voice, every scale is 0.5 sencond 
tone(12, melody[thisNote], duration);
delay(100);
// Output the voice after several minutes
delay(100);
} // restart after two seconds 
delay(200);
}

-----------------------------
10:00:18.616596                  textDocument/didChange: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:18.622226 Ino Range: 9:5-9:7 -> Cpp Range:16:5-16:7
10:00:18.622226   > Current sketchmapper content:
10:00:18.622226   0: #include <Arduino.h>                                         | /not-ino:0                                         
10:00:18.622226   1: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:18.622226   2:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:0                          
10:00:18.622226   3: #include "pitches.h"// notes in the melody:                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:1                          
10:00:18.622226   4: int melody[] = {                                             | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:2                          
10:00:18.622226   5: NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:3                          
10:00:18.622226   6: int duration = 500;  // 500 miliseconds                      | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:4                          
10:00:18.622226   7: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:18.622226   8: void setup();                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5
10:00:18.622226   9: #line 7 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:18.622226  10: void loop();                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6
10:00:18.622226  11: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:18.622226  12: void setup() {  }                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5                          
10:00:18.622729  13: void loop() {                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6                          
10:00:18.622766  14: for (int thisNote = 0; thisNote < 12; thisNote++) {          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:7                          
10:00:18.622766  15: // pin12 output the voice, every scale is 0.5 sencond        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:8                          
10:00:18.622766  16: tone(12, melody[thisNote], duration);                        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:9                          
10:00:18.622766  17: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:10                          
10:00:18.622766  18: // Output the voice after several minutes                    | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:11                          
10:00:18.622766  19: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:12                          
10:00:18.622766  20: } // restart after two seconds                               | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:13                          
10:00:18.622766  21: delay(200);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:14                          
10:00:18.622766  22: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:15                          
10:00:18.622766  23:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:16                          
10:00:18.622766  24:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:17                          
10:00:18.622766                  textDocument/didChange: to Clang: didChange(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp@11)
10:00:18.623291                  textDocument/didChange:             > 16:5-16:7 -> "12"
10:00:18.623291 IDE     LS --> Clangd NOTIF textDocument/didChange
10:00:18.623291 OUT Elapsed: 0s
10:00:18.623291                  textDocument/didChange: write-unlocked
10:00:18.626554 SKETCH REBUILD: : Running build with: {
  "instance": {
    "id": 1
  },
  "fqbn": "arduino:avr:uno",
  "sketch_path": "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣器等等传感器\\Code\\Lesson 5_Active_buzzer\\5_Active_buzzer",
  "build_path": "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764",
  "verbose": true,
  "create_compilation_database_only": true,
  "source_override": {
    "5_Active_buzzer.ino": "\r\n#include \"pitches.h\"// notes in the melody:\r\nint melody[] = {\r\nNOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};\r\nint duration = 500;  // 500 miliseconds \r\nvoid setup() {  }\r\nvoid loop() {\r\nfor (int thisNote = 0; thisNote \u003c 12; thisNote++) {\r\n// pin12 output the voice, every scale is 0.5 sencond \r\ntone(12, melody[thisNote], duration);\r\ndelay(100);\r\n// Output the voice after several minutes\r\ndelay(100);\r\n} // restart after two seconds \r\ndelay(200);\r\n}\r\n"
  },
  "skip_libraries_discovery": true
}
10:00:18.778589 IN Elapsed: 180.2641ms
10:00:18.778589 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
10:00:18.778589                             textDocument/publishDiagnostics: Ignored by configuration
10:00:18.843667 IN Elapsed: 220.3753ms
10:00:18.843667 IDE --> LS REQU textDocument/codeAction 31
10:00:18.843667                 textDocument/codeAction 31: read-locked
10:00:18.843667                 textDocument/codeAction 31: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:9:5)
10:00:18.844711                 textDocument/codeAction 31: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:00:18.848283                 textDocument/codeAction 31:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:9:5)
10:00:18.848283 IDE     LS --> Clangd REQU textDocument/codeAction 32
10:00:18.848283 OUT Elapsed: 0s
10:00:18.848826 IN Elapsed: 70.2364ms
10:00:18.848826 IDE     LS <-- Clangd RESP textDocument/codeAction 32
10:00:18.848826                 textDocument/codeAction 31: read-unlocked
10:00:18.848826 IDE <-- LS RESP textDocument/codeAction 31
10:00:18.848826 OUT Elapsed: 0s
10:00:19.029003 SKETCH REBUILD: : Compile successful!
10:00:19.058544 SKETCH REBUILD: : write-locked
10:00:19.058544 SKETCH REBUILD: : write-unlocked
10:00:19.058544 SKETCH REBUILD: : Error: context canceled
10:00:19.058544 IDE <-- LS NOTIF $/progress
10:00:19.058544 OUT Elapsed: 0s
10:00:19.612661 IN Elapsed: 763.8351ms
10:00:19.612661 IDE --> LS NOTIF textDocument/didSave
10:00:19.612661                  textDocument/didSave: write-locked
10:00:19.612661                  textDocument/didSave: notification is not forwarded to clang
10:00:19.612661                  textDocument/didSave: write-unlocked
10:00:20.626356 SKETCH REBUILD: : Sketch rebuild started
10:00:20.626356 SKETCH REBUILD: : read-locked
10:00:20.626356 SKETCH REBUILD: : read-unlocked
10:00:20.626356 IDE <-- LS REQU window/workDoneProgress/create 7
10:00:20.626356 OUT Elapsed: 0s
10:00:20.626901 IN Elapsed: 1.0142398s
10:00:20.626901 IDE --> LS RESP window/workDoneProgress/create 7
10:00:20.626901 IDE <-- LS NOTIF $/progress
10:00:20.626901 OUT Elapsed: 0s
10:00:20.937849 SKETCH REBUILD: : Running build with: {
  "instance": {
    "id": 1
  },
  "fqbn": "arduino:avr:uno",
  "sketch_path": "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣器等等传感器\\Code\\Lesson 5_Active_buzzer\\5_Active_buzzer",
  "build_path": "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764",
  "verbose": true,
  "create_compilation_database_only": true,
  "source_override": {
    "5_Active_buzzer.ino": "\r\n#include \"pitches.h\"// notes in the melody:\r\nint melody[] = {\r\nNOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};\r\nint duration = 500;  // 500 miliseconds \r\nvoid setup() {  }\r\nvoid loop() {\r\nfor (int thisNote = 0; thisNote \u003c 12; thisNote++) {\r\n// pin12 output the voice, every scale is 0.5 sencond \r\ntone(12, melody[thisNote], duration);\r\ndelay(100);\r\n// Output the voice after several minutes\r\ndelay(100);\r\n} // restart after two seconds \r\ndelay(200);\r\n}\r\n"
  },
  "skip_libraries_discovery": true
}
10:00:21.324365 SKETCH REBUILD: : Compile successful!
10:00:21.353331 SKETCH REBUILD: : write-locked
10:00:21.356828   > Current sketchmapper content:
10:00:21.356828   0: #include <Arduino.h>                                         | /not-ino:0                                         
10:00:21.356828   1: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:21.356828   2:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:0                          
10:00:21.357825   3: #include "pitches.h"// notes in the melody:                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:1                          
10:00:21.357825   4: int melody[] = {                                             | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:2                          
10:00:21.357825   5: NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:3                          
10:00:21.357825   6: int duration = 500;  // 500 miliseconds                      | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:4                          
10:00:21.357825   7: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:21.357825   8: void setup();                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5
10:00:21.357825   9: #line 7 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:21.357825  10: void loop();                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6
10:00:21.357825  11: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:00:21.357825  12: void setup() {  }                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5                          
10:00:21.357825  13: void loop() {                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6                          
10:00:21.357825  14: for (int thisNote = 0; thisNote < 12; thisNote++) {          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:7                          
10:00:21.357825  15: // pin12 output the voice, every scale is 0.5 sencond        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:8                          
10:00:21.357825  16: tone(12, melody[thisNote], duration);                        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:9                          
10:00:21.357825  17: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:10                          
10:00:21.357825  18: // Output the voice after several minutes                    | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:11                          
10:00:21.357825  19: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:12                          
10:00:21.357825  20: } // restart after two seconds                               | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:13                          
10:00:21.357825  21: delay(200);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:14                          
10:00:21.357825  22: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:15                          
10:00:21.357825  23:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:16                          
10:00:21.357825  24:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:17                          
10:00:21.357825 SKETCH REBUILD: : Sending 'didSave' notification to Clangd
10:00:21.357825 IDE     LS --> Clangd NOTIF textDocument/didSave
10:00:21.357825 OUT Elapsed: 0s
10:00:21.357825 SKETCH REBUILD: : Sending full-text 'didChange' notification to Clangd
10:00:21.357825 IDE     LS --> Clangd NOTIF textDocument/didChange
10:00:21.357825 OUT Elapsed: 0s
10:00:21.357825 SKETCH REBUILD: : write-unlocked
10:00:21.357825 IDE <-- LS NOTIF $/progress
10:00:21.357825 OUT Elapsed: 0s
10:00:21.425406 IN Elapsed: 2.5765805s
10:00:21.425406 IDE     LS <-- Clangd REQU window/workDoneProgress/create 3
10:00:21.425406 IDE     LS --> Clangd RESP window/workDoneProgress/create 3
10:00:21.425406 IDE <-- LS REQU window/workDoneProgress/create 8
10:00:21.425406 OUT Elapsed: 0s
10:00:21.425406 OUT Elapsed: 0s
10:00:21.425406 IN Elapsed: 0s
10:00:21.425406 IDE     LS <-- Clangd NOTIF $/progress
10:00:21.425910                             $/progress: backgroundIndexProgress BEGIN indexing, 0.0%
10:00:21.425910 IN Elapsed: 0s
10:00:21.425910 IDE     LS <-- Clangd NOTIF $/progress
10:00:21.425910 IN Elapsed: 799.009ms
10:00:21.425910                             $/progress: backgroundIndexProgress REPORT, 0/1, 0.0%
10:00:21.425910 IDE --> LS RESP window/workDoneProgress/create 8
10:00:21.425910 IDE <-- LS NOTIF $/progress
10:00:21.425910 OUT Elapsed: 0s
10:00:21.425910 IDE <-- LS NOTIF $/progress
10:00:21.425910 OUT Elapsed: 0s
10:00:21.472084 IN Elapsed: 46.174ms
10:00:21.472084 IDE     LS <-- Clangd NOTIF $/progress
10:00:21.472084                             $/progress: backgroundIndexProgress REPORT, 0/1, 0.0%
10:00:21.472084 IN Elapsed: 0s
10:00:21.472084 IDE     LS <-- Clangd NOTIF $/progress
10:00:21.472084                             $/progress: backgroundIndexProgress END 
10:00:21.472084 IDE <-- LS NOTIF $/progress
10:00:21.472084 OUT Elapsed: 0s
10:00:21.472084 IDE <-- LS NOTIF $/progress
10:00:21.472084 OUT Elapsed: 0s
10:02:07.139168 IN Elapsed: 1m45.7132581s
10:02:07.139168 IDE --> LS REQU textDocument/hover 32
10:02:07.139168                 textDocument/hover 32: read-locked
10:02:07.140258                 textDocument/hover 32: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:02:07.143984                 textDocument/hover 32: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:11 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:12:11
10:02:07.143984 IDE     LS --> Clangd REQU textDocument/hover 33
10:02:07.143984 OUT Elapsed: 0s
10:02:07.150975 IN Elapsed: 1m45.6788911s
10:02:07.150975 IDE     LS <-- Clangd RESP textDocument/hover 33
10:02:07.150975                 textDocument/hover 32: null response
10:02:07.150975                 textDocument/hover 32: read-unlocked
10:02:07.150975 IDE <-- LS RESP textDocument/hover 32
10:02:07.150975 OUT Elapsed: 0s
10:02:08.899107 IN Elapsed: 1.7481322s
10:02:08.899107 IDE --> LS NOTIF ino/didCompleteBuild
10:02:08.899107                  ino/didCompleteBuild: write-locked
10:02:08.900718                  ino/didCompleteBuild: ERROR: updating libraries.cache: open C:\Users\Administrator\AppData\Local\Temp\arduino-sketch-31A9A4270AEAD423CD6B51954EDE7DB3\libraries.cache: The system cannot find the file specified.
10:02:08.900768                  ino/didCompleteBuild: write-unlocked
10:02:09.906292 SKETCH REBUILD: : Sketch rebuild started
10:02:09.906804 IDE <-- LS REQU window/workDoneProgress/create 9
10:02:09.908376 OUT Elapsed: 565.6µs
10:02:09.906804 SKETCH REBUILD: : read-locked
10:02:09.908884 SKETCH REBUILD: : read-unlocked
10:02:09.909774 IN Elapsed: 1.0090051s
10:02:09.909774 IDE --> LS RESP window/workDoneProgress/create 9
10:02:09.909774 IDE <-- LS NOTIF $/progress
10:02:09.909774 OUT Elapsed: 0s
10:02:10.220226 SKETCH REBUILD: : Running build with: {
  "instance": {
    "id": 1
  },
  "fqbn": "arduino:avr:uno",
  "sketch_path": "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣器等等传感器\\Code\\Lesson 5_Active_buzzer\\5_Active_buzzer",
  "build_path": "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764",
  "verbose": true,
  "create_compilation_database_only": true,
  "source_override": {
    "5_Active_buzzer.ino": "\r\n#include \"pitches.h\"// notes in the melody:\r\nint melody[] = {\r\nNOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};\r\nint duration = 500;  // 500 miliseconds \r\nvoid setup() {  }\r\nvoid loop() {\r\nfor (int thisNote = 0; thisNote \u003c 12; thisNote++) {\r\n// pin12 output the voice, every scale is 0.5 sencond \r\ntone(12, melody[thisNote], duration);\r\ndelay(100);\r\n// Output the voice after several minutes\r\ndelay(100);\r\n} // restart after two seconds \r\ndelay(200);\r\n}\r\n"
  },
  "skip_libraries_discovery": true
}
10:02:10.602256 SKETCH REBUILD: : Compile successful!
10:02:10.630556 SKETCH REBUILD: : write-locked
10:02:10.635156   > Current sketchmapper content:
10:02:10.635156   0: #include <Arduino.h>                                         | /not-ino:0                                         
10:02:10.635156   1: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:02:10.635156   2:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:0                          
10:02:10.635156   3: #include "pitches.h"// notes in the melody:                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:1                          
10:02:10.635156   4: int melody[] = {                                             | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:2                          
10:02:10.635156   5: NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:3                          
10:02:10.635156   6: int duration = 500;  // 500 miliseconds                      | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:4                          
10:02:10.635156   7: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:02:10.635156   8: void setup();                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5
10:02:10.635156   9: #line 7 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:02:10.635156  10: void loop();                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6
10:02:10.635156  11: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:02:10.635156  12: void setup() {  }                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5                          
10:02:10.635156  13: void loop() {                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6                          
10:02:10.635156  14: for (int thisNote = 0; thisNote < 12; thisNote++) {          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:7                          
10:02:10.635156  15: // pin12 output the voice, every scale is 0.5 sencond        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:8                          
10:02:10.635156  16: tone(12, melody[thisNote], duration);                        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:9                          
10:02:10.635156  17: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:10                          
10:02:10.635156  18: // Output the voice after several minutes                    | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:11                          
10:02:10.635156  19: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:12                          
10:02:10.635156  20: } // restart after two seconds                               | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:13                          
10:02:10.635156  21: delay(200);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:14                          
10:02:10.635156  22: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:15                          
10:02:10.635156  23:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:16                          
10:02:10.635156  24:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:17                          
10:02:10.635156 SKETCH REBUILD: : Sending 'didSave' notification to Clangd
10:02:10.636153 IDE     LS --> Clangd NOTIF textDocument/didSave
10:02:10.636153 OUT Elapsed: 0s
10:02:10.636153 SKETCH REBUILD: : Sending full-text 'didChange' notification to Clangd
10:02:10.636153 IDE     LS --> Clangd NOTIF textDocument/didChange
10:02:10.636153 OUT Elapsed: 0s
10:02:10.636153 SKETCH REBUILD: : write-unlocked
10:02:10.636153 IDE <-- LS NOTIF $/progress
10:02:10.636153 OUT Elapsed: 0s
10:02:10.700407 IN Elapsed: 3.549432s
10:02:10.700407 IDE     LS <-- Clangd REQU window/workDoneProgress/create 4
10:02:10.700407 IDE     LS --> Clangd RESP window/workDoneProgress/create 4
10:02:10.700407 IDE <-- LS REQU window/workDoneProgress/create 10
10:02:10.700407 OUT Elapsed: 0s
10:02:10.700407 OUT Elapsed: 0s
10:02:10.700407 IN Elapsed: 0s
10:02:10.700407 IDE     LS <-- Clangd NOTIF $/progress
10:02:10.700407                             $/progress: backgroundIndexProgress BEGIN indexing, 0.0%
10:02:10.700407 IN Elapsed: 0s
10:02:10.700910 IDE     LS <-- Clangd NOTIF $/progress
10:02:10.700917                             $/progress: backgroundIndexProgress REPORT, 0/1, 0.0%
10:02:10.700917 IN Elapsed: 791.1435ms
10:02:10.700917 IDE --> LS RESP window/workDoneProgress/create 10
10:02:10.700917 IDE <-- LS NOTIF $/progress
10:02:10.700917 OUT Elapsed: 0s
10:02:10.700917 IDE <-- LS NOTIF $/progress
10:02:10.700917 OUT Elapsed: 0s
10:02:10.746025 IN Elapsed: 45.1084ms
10:02:10.746025 IDE     LS <-- Clangd NOTIF $/progress
10:02:10.746025                             $/progress: backgroundIndexProgress REPORT, 0/1, 0.0%
10:02:10.746025 IN Elapsed: 0s
10:02:10.746025 IDE     LS <-- Clangd NOTIF $/progress
10:02:10.746025                             $/progress: backgroundIndexProgress END 
10:02:10.746025 IDE <-- LS NOTIF $/progress
10:02:10.746025 OUT Elapsed: 0s
10:02:10.746025 IDE <-- LS NOTIF $/progress
10:02:10.746025 OUT Elapsed: 0s
10:02:23.936140 IN Elapsed: 13.2352225s
10:02:23.936140 IDE --> LS NOTIF ino/didCompleteBuild
10:02:23.936140                  ino/didCompleteBuild: write-locked
10:02:23.937782                  ino/didCompleteBuild: ERROR: updating libraries.cache: open C:\Users\Administrator\AppData\Local\Temp\arduino-sketch-31A9A4270AEAD423CD6B51954EDE7DB3\libraries.cache: The system cannot find the file specified.
10:02:23.937782                  ino/didCompleteBuild: write-unlocked
10:02:24.946832 SKETCH REBUILD: : Sketch rebuild started
10:02:24.946832 SKETCH REBUILD: : read-locked
10:02:24.946832 SKETCH REBUILD: : read-unlocked
10:02:24.946832 IDE <-- LS REQU window/workDoneProgress/create 11
10:02:24.946832 OUT Elapsed: 0s
10:02:24.947336 IN Elapsed: 1.009554s
10:02:24.947380 IDE --> LS RESP window/workDoneProgress/create 11
10:02:24.947380 IDE <-- LS NOTIF $/progress
10:02:24.947380 OUT Elapsed: 0s
10:02:25.256323 SKETCH REBUILD: : Running build with: {
  "instance": {
    "id": 1
  },
  "fqbn": "arduino:avr:uno",
  "sketch_path": "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣器等等传感器\\Code\\Lesson 5_Active_buzzer\\5_Active_buzzer",
  "build_path": "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764",
  "verbose": true,
  "create_compilation_database_only": true,
  "source_override": {
    "5_Active_buzzer.ino": "\r\n#include \"pitches.h\"// notes in the melody:\r\nint melody[] = {\r\nNOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};\r\nint duration = 500;  // 500 miliseconds \r\nvoid setup() {  }\r\nvoid loop() {\r\nfor (int thisNote = 0; thisNote \u003c 12; thisNote++) {\r\n// pin12 output the voice, every scale is 0.5 sencond \r\ntone(12, melody[thisNote], duration);\r\ndelay(100);\r\n// Output the voice after several minutes\r\ndelay(100);\r\n} // restart after two seconds \r\ndelay(200);\r\n}\r\n"
  },
  "skip_libraries_discovery": true
}
10:02:25.644113 SKETCH REBUILD: : Compile successful!
10:02:25.673677 SKETCH REBUILD: : write-locked
10:02:25.678136   > Current sketchmapper content:
10:02:25.678136   0: #include <Arduino.h>                                         | /not-ino:0                                         
10:02:25.678136   1: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:02:25.678136   2:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:0                          
10:02:25.678136   3: #include "pitches.h"// notes in the melody:                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:1                          
10:02:25.678136   4: int melody[] = {                                             | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:2                          
10:02:25.678136   5: NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:3                          
10:02:25.678136   6: int duration = 500;  // 500 miliseconds                      | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:4                          
10:02:25.678639   7: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:02:25.678639   8: void setup();                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5
10:02:25.678673   9: #line 7 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:02:25.678673  10: void loop();                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6
10:02:25.678673  11: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:02:25.678673  12: void setup() {  }                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5                          
10:02:25.678673  13: void loop() {                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6                          
10:02:25.678673  14: for (int thisNote = 0; thisNote < 12; thisNote++) {          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:7                          
10:02:25.678673  15: // pin12 output the voice, every scale is 0.5 sencond        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:8                          
10:02:25.678673  16: tone(12, melody[thisNote], duration);                        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:9                          
10:02:25.678673  17: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:10                          
10:02:25.678673  18: // Output the voice after several minutes                    | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:11                          
10:02:25.678673  19: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:12                          
10:02:25.678673  20: } // restart after two seconds                               | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:13                          
10:02:25.678673  21: delay(200);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:14                          
10:02:25.678673  22: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:15                          
10:02:25.678673  23:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:16                          
10:02:25.678673  24:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:17                          
10:02:25.678673 SKETCH REBUILD: : Sending 'didSave' notification to Clangd
10:02:25.678673 IDE     LS --> Clangd NOTIF textDocument/didSave
10:02:25.678673 OUT Elapsed: 0s
10:02:25.678673 SKETCH REBUILD: : Sending full-text 'didChange' notification to Clangd
10:02:25.678673 IDE     LS --> Clangd NOTIF textDocument/didChange
10:02:25.679193 OUT Elapsed: 0s
10:02:25.679193 SKETCH REBUILD: : write-unlocked
10:02:25.679193 IDE <-- LS NOTIF $/progress
10:02:25.679193 OUT Elapsed: 0s
10:02:25.748965 IN Elapsed: 15.0029394s
10:02:25.748965 IDE     LS <-- Clangd REQU window/workDoneProgress/create 5
10:02:25.748965 IDE     LS --> Clangd RESP window/workDoneProgress/create 5
10:02:25.748965 IDE <-- LS REQU window/workDoneProgress/create 12
10:02:25.748965 OUT Elapsed: 0s
10:02:25.748965 OUT Elapsed: 0s
10:02:25.748965 IN Elapsed: 0s
10:02:25.748965 IDE     LS <-- Clangd NOTIF $/progress
10:02:25.748965                             $/progress: backgroundIndexProgress BEGIN indexing, 0.0%
10:02:25.748965 IN Elapsed: 0s
10:02:25.749469 IN Elapsed: 802.0887ms
10:02:25.749502 IDE     LS <-- Clangd NOTIF $/progress
10:02:25.749502 IDE --> LS RESP window/workDoneProgress/create 12
10:02:25.749502 IDE <-- LS NOTIF $/progress
10:02:25.749502                             $/progress: backgroundIndexProgress REPORT, 0/1, 0.0%
10:02:25.749502 OUT Elapsed: 0s
10:02:25.749502 IDE <-- LS NOTIF $/progress
10:02:25.749502 OUT Elapsed: 0s
10:02:25.794086 IN Elapsed: 44.5839ms
10:02:25.794283 IDE     LS <-- Clangd NOTIF $/progress
10:02:25.794283                             $/progress: backgroundIndexProgress REPORT, 0/1, 0.0%
10:02:25.794283 IN Elapsed: 0s
10:02:25.794283 IDE <-- LS NOTIF $/progress
10:02:25.794283 IDE     LS <-- Clangd NOTIF $/progress
10:02:25.794283 OUT Elapsed: 0s
10:02:25.794283                             $/progress: backgroundIndexProgress END 
10:02:25.794283 IDE <-- LS NOTIF $/progress
10:02:25.794283 OUT Elapsed: 0s
10:02:47.649174 IN Elapsed: 21.8996726s
10:02:47.649355 IDE --> LS REQU textDocument/codeAction 33
10:02:47.649413                 textDocument/codeAction 33: read-locked
10:02:47.649463                 textDocument/codeAction 33: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:14:11)
10:02:47.650402                 textDocument/codeAction 33: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:02:47.654167                 textDocument/codeAction 33:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:14:11)
10:02:47.654167 IDE     LS --> Clangd REQU textDocument/codeAction 34
10:02:47.654679 OUT Elapsed: 512.6µs
10:02:47.658633 IN Elapsed: 21.8643504s
10:02:47.658633 IDE     LS <-- Clangd RESP textDocument/codeAction 34
10:02:47.658633                 textDocument/codeAction 33: read-unlocked
10:02:47.658633 IDE <-- LS RESP textDocument/codeAction 33
10:02:47.658633 OUT Elapsed: 0s
10:02:53.267243 IN Elapsed: 5.6086102s
10:02:53.267243 IDE --> LS REQU textDocument/codeAction 34
10:02:53.267243                 textDocument/codeAction 34: read-locked
10:02:53.267243                 textDocument/codeAction 34: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:15:1)
10:02:53.268293                 textDocument/codeAction 34: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:02:53.272008                 textDocument/codeAction 34:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:15:1)
10:02:53.272061 IDE     LS --> Clangd REQU textDocument/codeAction 35
10:02:53.272061 OUT Elapsed: 0s
10:02:53.275665 IN Elapsed: 5.6170319s
10:02:53.275665 IDE     LS <-- Clangd RESP textDocument/codeAction 35
10:02:53.275665                 textDocument/codeAction 34: read-unlocked
10:02:53.275665 IDE <-- LS RESP textDocument/codeAction 34
10:02:53.275665 OUT Elapsed: 0s
10:03:35.471386 IN Elapsed: 42.1957208s
10:03:35.471444 IDE --> LS REQU textDocument/hover 35
10:03:35.471502                 textDocument/hover 35: read-locked
10:03:35.472517                 textDocument/hover 35: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp
10:03:35.475981                 textDocument/hover 35: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:1:34 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp:3:34
10:03:35.475981 IDE     LS --> Clangd REQU textDocument/hover 36
10:03:35.476512 OUT Elapsed: 26µs
10:03:35.483048 IN Elapsed: 42.2073833s
10:03:35.483048 IDE     LS <-- Clangd RESP textDocument/hover 36
10:03:35.483048                 textDocument/hover 35: null response
10:03:35.483048                 textDocument/hover 35: read-unlocked
10:03:35.483048 IDE <-- LS RESP textDocument/hover 35
10:03:35.483048 OUT Elapsed: 0s
10:03:36.651651 IN Elapsed: 1.1686032s
10:03:36.652171 IDE --> LS REQU shutdown 36
10:03:36.652171 IDE     LS --> Clangd REQU shutdown 37
10:03:36.652674 OUT Elapsed: 503.6µs
10:03:36.652922 IN Elapsed: 1.169874s
10:03:36.652922 IDE     LS <-- Clangd RESP shutdown 37
10:03:36.652922 IDE <-- LS RESP shutdown 36
10:03:36.652922 OUT Elapsed: 0s
10:03:36.654609 IN Elapsed: 1.1831ms
10:03:36.654609 IDE --> LS NOTIF exit
10:03:36.654609 IDE     LS --> Clangd NOTIF exit
10:03:36.655170 OUT Elapsed: 56.3µs
10:03:36.655170                  exit: Arduino Language Server is shutting down.







Started logging.
10:03:47.120442 Language server launched with arguments:
10:03:47.120442   arg[0] = d:\Program Files\Arduino IDE\resources\app\node_modules\arduino-ide-extension\build\arduino-language-server.exe
10:03:47.120442   arg[1] = -clangd
10:03:47.120442   arg[2] = d:\Program Files\Arduino IDE\resources\app\node_modules\arduino-ide-extension\build\clangd.exe
10:03:47.120442   arg[3] = -cli-daemon-addr
10:03:47.120442   arg[4] = localhost:57938
10:03:47.120442   arg[5] = -cli-daemon-instance
10:03:47.120442   arg[6] = 1
10:03:47.120442   arg[7] = -fqbn
10:03:47.120442   arg[8] = arduino:avr:uno
10:03:47.120442   arg[9] = -skip-libraries-discovery-on-rebuild
10:03:47.120442   arg[10] = -board-name
10:03:47.120945   arg[11] = "Arduino Uno"
10:03:47.120945   arg[12] = -no-real-time-diagnostics
10:03:47.120980   arg[13] = -log
10:03:47.120980   arg[14] = -logpath
10:03:47.120980   arg[15] = g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer
10:03:47.120980 logging to g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\inols.log
10:03:47.126190 LS: : Initial board configuration: arduino:avr:uno
10:03:47.126190 LS: : Language server build path: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420
10:03:47.126190 LS: : Language server build sketch root: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch
10:03:47.126190 LS: : Language server FULL build path: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server793985706
10:03:47.126728 IN Elapsed: 0s
10:03:47.126728 IDE --> LS REQU initialize 0
10:03:47.127254                 initialize 0: write-locked
10:03:47.129005                 initialize 0: write-unlocked
10:03:47.129005 INIT --- : initializing workbench: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer
10:03:47.129005 INIT --- : read-locked
10:03:47.129005 INIT --- : read-unlocked
10:03:47.129556                 initialize 0: initialization parameters: {"capabilities":{"textDocumentSync":{"openClose":true,"change":2,"save":{"includeText":true}},"completionProvider":{"triggerCharacters":[".","\u003c","\u003e",":","\"","/"],"allCommitCharacters":[" ","\t","(",")","[","]","{","}","\u003c","\u003e",":",";",",","+","-","/","*","%","^","\u0026","#","?",".","=","\"","'","|"],"completionItem":{}},"hoverProvider":{},"signatureHelpProvider":{"triggerCharacters":["(",","]},"definitionProvider":{},"documentHighlightProvider":{},"documentSymbolProvider":{},"codeActionProvider":{"codeActionKinds":["quickfix","refactor","info"]},"documentFormattingProvider":{},"documentRangeFormattingProvider":{},"documentOnTypeFormattingProvider":{"firstTriggerCharacter":"\n"},"renameProvider":{},"executeCommandProvider":{"commands":["clangd.applyFix","clangd.applyTweak"]},"workspaceSymbolProvider":{}},"serverInfo":{"name":"arduino-language-server","version":"0.7.1"}}
10:03:47.129556 IDE <-- LS RESP initialize 0
10:03:47.129556 OUT Elapsed: 0s
10:03:47.132286 listen tcp 127.0.0.1:6060: bind: Only one usage of each socket address (protocol/network address/port) is normally permitted.
10:03:47.133857 IN Elapsed: 4.3014ms
10:03:47.134368 IDE --> LS NOTIF initialized
10:03:47.134368                  initialized: Notification is not propagated to clangd
10:03:47.134368 IN Elapsed: 0s
10:03:47.134368 IDE --> LS NOTIF textDocument/didOpen
10:03:47.134368                  textDocument/didOpen: write-locked
10:03:47.134368                  textDocument/didOpen: (throttled: waiting for clangd)
10:03:47.134368                  textDocument/didOpen: unlocked (waiting clangd)
10:03:47.440867 INIT --- : Running build with: {
  "instance": {
    "id": 1
  },
  "fqbn": "arduino:avr:uno",
  "sketch_path": "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣器等等传感器\\Code\\Lesson 5_Active_buzzer\\5_Active_buzzer",
  "build_path": "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server793985706",
  "verbose": true,
  "create_compilation_database_only": true
}
10:03:49.780621 INIT --- : Compile successful!
10:03:49.784222 INIT --- : Updated 'libraries.cache'. Copied: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server793985706\libraries.cache to C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\libraries.cache
10:03:49.784222 INIT --- : read-locked
10:03:49.784222 INIT --- : read-unlocked
10:03:50.088866 INIT --- : Running build with: {
  "instance": {
    "id": 1
  },
  "fqbn": "arduino:avr:uno",
  "sketch_path": "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣器等等传感器\\Code\\Lesson 5_Active_buzzer\\5_Active_buzzer",
  "build_path": "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420",
  "verbose": true,
  "create_compilation_database_only": true,
  "skip_libraries_discovery": true
}
10:03:50.409871 INIT --- : Compile successful!
10:03:50.747074 INIT --- : Arduino Data Dir -> c:\Users\Administrator\AppData\Local\Arduino15
10:03:50.749738 INIT --- :     Starting clangd: d:\Program Files\Arduino IDE\resources\app\node_modules\arduino-ide-extension\build\clangd.exe -log=verbose --compile-commands-dir=C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420 -query-driver=C:\Users\Administrator\AppData\Local\Arduino15\packages\**
10:03:50.762006 logging to g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\inols-clangd.log
10:03:50.762530 logging to g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\inols-clangd-err.log
10:03:50.762530 IDE     LS --> Clangd REQU initialize 1
10:03:50.762530 OUT Elapsed: 0s
10:03:50.843736 IN Elapsed: 81.2051ms
10:03:50.844506 IDE     LS <-- Clangd RESP initialize 1
10:03:50.844506 INIT --- : clangd successfully started: {"capabilities":{"textDocumentSync":{"openClose":true,"change":2,"save":{}},"completionProvider":{"triggerCharacters":[".","\u003c","\u003e",":","\"","/","*"],"allCommitCharacters":[" ","\t","(",")","[","]","{","}","\u003c","\u003e",":",";",",","+","-","/","*","%","^","\u0026","#","?",".","=","\"","'","|"]},"hoverProvider":{},"signatureHelpProvider":{"triggerCharacters":["(",")","{","}","\u003c","\u003e",","]},"declarationProvider":{},"definitionProvider":{},"typeDefinitionProvider":{},"implementationProvider":{},"referencesProvider":{},"documentHighlightProvider":{},"documentSymbolProvider":{},"codeActionProvider":{"codeActionKinds":["quickfix","refactor","info"]},"documentLinkProvider":{},"documentFormattingProvider":{},"documentRangeFormattingProvider":{},"documentOnTypeFormattingProvider":{"firstTriggerCharacter":"\n"},"renameProvider":{"prepareProvider":true},"executeCommandProvider":{"commands":["clangd.applyFix","clangd.applyTweak"]},"selectionRangeProvider":{},"callHierarchyProvider":{},"semanticTokensProvider":{"legend":{"tokenTypes":["variable","variable","parameter","function","method","function","property","variable","class","interface","enum","enumMember","type","type","unknown","namespace","typeParameter","concept","type","macro","comment"],"tokenModifiers":["declaration","deprecated","deduced","readonly","static","abstract","virtual","dependentName","defaultLibrary","usedAsMutableReference","functionScope","classScope","fileScope","globalScope"]},"range":false,"full":{"delta":true}},"workspaceSymbolProvider":{}},"serverInfo":{"name":"clangd","version":"clangd version 14.0.0 windows x86_64-pc-windows-msvc"}}
10:03:50.844506 IDE     LS --> Clangd NOTIF initialized
10:03:50.844506 OUT Elapsed: 0s
10:03:50.844506 INIT --- : Done initializing workbench
10:03:50.845010                  textDocument/didOpen: locked (waiting clangd)
10:03:50.845723                  textDocument/didOpen: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp
10:03:50.849366                  textDocument/didOpen: Increasing .ino tracked files count to 1
10:03:50.850966 IDE     LS --> Clangd NOTIF textDocument/didOpen
10:03:50.850966 OUT Elapsed: 0s
10:03:50.850966                  textDocument/didOpen: write-unlocked
10:03:50.850966 IN Elapsed: 0s
10:03:50.850966 IDE --> LS NOTIF textDocument/didOpen
10:03:50.851469                  textDocument/didOpen: write-locked
10:03:50.852024                  textDocument/didOpen: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/pitches.h -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/pitches.h
10:03:50.856577 IN Elapsed: 12.8415ms
10:03:50.856577 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
10:03:50.856577                             textDocument/publishDiagnostics: Ignored by configuration
10:03:50.860649 IN Elapsed: 4.0716ms
10:03:50.860649 IDE     LS <-- Clangd REQU window/workDoneProgress/create 0
10:03:50.860649 IDE     LS --> Clangd RESP window/workDoneProgress/create 0
10:03:50.861152 OUT Elapsed: 503µs
10:03:50.861227 IN Elapsed: 74.9µs
10:03:50.861227 IDE     LS <-- Clangd NOTIF $/progress
10:03:50.861227 IDE <-- LS REQU window/workDoneProgress/create 1
10:03:50.861227 OUT Elapsed: 0s
10:03:50.861227                             $/progress: backgroundIndexProgress BEGIN indexing, 0.0%
10:03:50.862461 IDE     LS --> Clangd NOTIF textDocument/didOpen
10:03:50.862461 IN Elapsed: 1.2342ms
10:03:50.862461 IDE     LS <-- Clangd NOTIF $/progress
10:03:50.862965                             $/progress: backgroundIndexProgress REPORT, 0/1, 0.0%
10:03:50.863476 OUT Elapsed: 1.0148ms
10:03:50.863980                  textDocument/didOpen: write-unlocked
10:03:50.864335 IN Elapsed: 355.1µs
10:03:50.864335 IDE --> LS REQU textDocument/codeAction 1
10:03:50.864335                 textDocument/codeAction 1: read-locked
10:03:50.864335                 textDocument/codeAction 1: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/pitches.h:0:0)
10:03:50.865531                 textDocument/codeAction 1: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/pitches.h -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/pitches.h
10:03:50.868064                 textDocument/codeAction 1:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/pitches.h:0:0)
10:03:50.868064 IDE     LS --> Clangd REQU textDocument/codeAction 2
10:03:50.868193 OUT Elapsed: 128.5µs
10:03:50.870755 IN Elapsed: 7.7905ms
10:03:50.870755 IDE     LS <-- Clangd NOTIF $/progress
10:03:50.870755                             $/progress: backgroundIndexProgress REPORT, 0/27, 0.0%
10:03:50.871678 IN Elapsed: 0s
10:03:50.872193 IDE     LS <-- Clangd NOTIF $/progress
10:03:50.872193                             $/progress: backgroundIndexProgress REPORT, 0/27, 0.0%
10:03:50.872193 IN Elapsed: 0s
10:03:50.872193 IDE     LS <-- Clangd NOTIF $/progress
10:03:50.874090                             $/progress: backgroundIndexProgress REPORT, 1/27, 3.0%
10:03:50.874090 IN Elapsed: 0s
10:03:50.874090 IDE     LS <-- Clangd NOTIF $/progress
10:03:50.874090                             $/progress: backgroundIndexProgress REPORT, 1/27, 3.0%
10:03:50.874090 IN Elapsed: 0s
10:03:50.874090 IDE     LS <-- Clangd NOTIF $/progress
10:03:50.874090                             $/progress: backgroundIndexProgress REPORT, 1/27, 3.0%
10:03:50.874090 IN Elapsed: 0s
10:03:50.874090 IDE     LS <-- Clangd NOTIF $/progress
10:03:50.874605                             $/progress: backgroundIndexProgress REPORT, 1/27, 3.0%
10:03:50.874605 IN Elapsed: 0s
10:03:50.874605 IDE     LS <-- Clangd NOTIF $/progress
10:03:50.874605                             $/progress: backgroundIndexProgress REPORT, 1/27, 3.0%
10:03:50.874605 IN Elapsed: 0s
10:03:50.875119 IDE     LS <-- Clangd NOTIF $/progress
10:03:50.875119                             $/progress: backgroundIndexProgress REPORT, 1/27, 3.0%
10:03:51.134849 IN Elapsed: 259.7298ms
10:03:51.134849 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
10:03:51.134849                             textDocument/publishDiagnostics: Ignored by configuration
10:03:51.134849 IN Elapsed: 0s
10:03:51.135362 IDE     LS <-- Clangd RESP textDocument/codeAction 2
10:03:51.135362                 textDocument/codeAction 1: read-unlocked
10:03:51.135362 IDE <-- LS RESP textDocument/codeAction 1
10:03:51.135362 OUT Elapsed: 0s
10:03:51.135362 IN Elapsed: 0s
10:03:51.135362 IDE --> LS REQU textDocument/documentSymbol 2
10:03:51.135362                 textDocument/documentSymbol 2: read-locked
10:03:51.136388                 textDocument/documentSymbol 2: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp
10:03:51.136904 IDE     LS --> Clangd REQU textDocument/documentSymbol 3
10:03:51.136904 OUT Elapsed: 0s
10:03:51.215225 IN Elapsed: 79.8631ms
10:03:51.215225 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
10:03:51.215402                             textDocument/publishDiagnostics: Ignored by configuration
10:03:51.215402 IN Elapsed: 177.4µs
10:03:51.215402 IDE     LS <-- Clangd RESP textDocument/documentSymbol 3
10:03:51.215402                 textDocument/documentSymbol 2: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
10:03:51.215402                 textDocument/documentSymbol 2:   > convert SymbolKind:Variable 4:0-5:71
10:03:51.217462                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:4:0-5:71 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-3:71 (.ino)
10:03:51.219006                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
10:03:51.219006                 textDocument/documentSymbol 2: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:03:51.219006                 textDocument/documentSymbol 2:   > convert SymbolKind:Variable 6:0-6:18
10:03:51.222097                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
10:03:51.224663                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
10:03:51.224663                 textDocument/documentSymbol 2: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:03:51.224663                 textDocument/documentSymbol 2:   > convert SymbolKind:Function 8:0-8:12
10:03:51.227461                 textDocument/documentSymbol 2: Range is in PREPROCESSED section of the sketch
10:03:51.227461                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
10:03:51.227461                 textDocument/documentSymbol 2:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
10:03:51.227461                 textDocument/documentSymbol 2:   > convert SymbolKind:Function 10:0-10:11
10:03:51.229507                 textDocument/documentSymbol 2: Range is in PREPROCESSED section of the sketch
10:03:51.229507                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
10:03:51.229507                 textDocument/documentSymbol 2:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
10:03:51.229507                 textDocument/documentSymbol 2:   > convert SymbolKind:Function 12:0-12:17
10:03:51.231562                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
10:03:51.233095                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
10:03:51.233607                 textDocument/documentSymbol 2: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:03:51.233607                 textDocument/documentSymbol 2:   > convert SymbolKind:Function 13:0-22:1
10:03:51.234631 IN Elapsed: 19.2285ms
10:03:51.235134 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.235144                             $/progress: backgroundIndexProgress REPORT, 2/27, 7.0%
10:03:51.235144 IN Elapsed: 0s
10:03:51.235144 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.235144                             $/progress: backgroundIndexProgress REPORT, 2/27, 7.0%
10:03:51.235144                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
10:03:51.237199                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
10:03:51.237199                 textDocument/documentSymbol 2: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:03:51.237199                 textDocument/documentSymbol 2: read-unlocked
10:03:51.237199 IDE <-- LS RESP textDocument/documentSymbol 2
10:03:51.237199 OUT Elapsed: 0s
10:03:51.237199 IN Elapsed: 0s
10:03:51.237199 IDE --> LS REQU textDocument/hover 3
10:03:51.237199                 textDocument/hover 3: read-locked
10:03:51.238746                 textDocument/hover 3: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp
10:03:51.246971                 textDocument/hover 3: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:10 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:13:10
10:03:51.246971 IDE     LS --> Clangd REQU textDocument/hover 4
10:03:51.247484 OUT Elapsed: 0s
10:03:51.250557 IN Elapsed: 15.4129ms
10:03:51.250557 IDE     LS <-- Clangd RESP textDocument/hover 4
10:03:51.250557                 textDocument/hover 3: null response
10:03:51.250557                 textDocument/hover 3: read-unlocked
10:03:51.251070 IDE <-- LS RESP textDocument/hover 3
10:03:51.251070 OUT Elapsed: 0s
10:03:51.251070 IN Elapsed: 0s
10:03:51.251070 IDE --> LS RESP window/workDoneProgress/create 1
10:03:51.251583 IDE <-- LS NOTIF $/progress
10:03:51.252619 OUT Elapsed: 0s
10:03:51.252619 IDE <-- LS NOTIF $/progress
10:03:51.252619 OUT Elapsed: 0s
10:03:51.535222 IN Elapsed: 284.6646ms
10:03:51.535222 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.535222                             $/progress: backgroundIndexProgress REPORT, 3/27, 11.0%
10:03:51.535222 IN Elapsed: 0s
10:03:51.535222 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.535222                             $/progress: backgroundIndexProgress REPORT, 3/27, 11.0%
10:03:51.535776 IDE <-- LS NOTIF $/progress
10:03:51.535776 OUT Elapsed: 0s
10:03:51.546573 IN Elapsed: 11.3517ms
10:03:51.546573 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.546573                             $/progress: backgroundIndexProgress REPORT, 4/27, 14.0%
10:03:51.546573 IDE <-- LS NOTIF $/progress
10:03:51.546573 OUT Elapsed: 0s
10:03:51.546573 IN Elapsed: 0s
10:03:51.546573 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.547085                             $/progress: backgroundIndexProgress REPORT, 4/27, 14.0%
10:03:51.547085 IDE <-- LS NOTIF $/progress
10:03:51.547085 OUT Elapsed: 0s
10:03:51.626461 IN Elapsed: 79.3762ms
10:03:51.626461 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.626461                             $/progress: backgroundIndexProgress REPORT, 5/27, 18.0%
10:03:51.626461 IN Elapsed: 0s
10:03:51.626461 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.626461                             $/progress: backgroundIndexProgress REPORT, 5/27, 18.0%
10:03:51.626461 IDE <-- LS NOTIF $/progress
10:03:51.626461 OUT Elapsed: 0s
10:03:51.626461 IDE <-- LS NOTIF $/progress
10:03:51.626461 OUT Elapsed: 0s
10:03:51.646375 IN Elapsed: 19.9138ms
10:03:51.646375 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.646375                             $/progress: backgroundIndexProgress REPORT, 6/27, 22.0%
10:03:51.646375 IDE <-- LS NOTIF $/progress
10:03:51.646375 OUT Elapsed: 0s
10:03:51.646375 IN Elapsed: 0s
10:03:51.646375 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.646375                             $/progress: backgroundIndexProgress REPORT, 6/27, 22.0%
10:03:51.646890 IDE <-- LS NOTIF $/progress
10:03:51.646890 OUT Elapsed: 0s
10:03:51.709363 IN Elapsed: 62.4732ms
10:03:51.709867 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.709867                             $/progress: backgroundIndexProgress REPORT, 7/27, 25.0%
10:03:51.710049 IN Elapsed: 0s
10:03:51.710049 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.710049                             $/progress: backgroundIndexProgress REPORT, 7/27, 25.0%
10:03:51.710049 IDE <-- LS NOTIF $/progress
10:03:51.710049 OUT Elapsed: 0s
10:03:51.725960 IN Elapsed: 15.911ms
10:03:51.725960 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.726464                             $/progress: backgroundIndexProgress REPORT, 8/27, 29.0%
10:03:51.726529 IN Elapsed: 64.5µs
10:03:51.726529 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.726529                             $/progress: backgroundIndexProgress REPORT, 8/27, 29.0%
10:03:51.726529 IDE <-- LS NOTIF $/progress
10:03:51.726529 OUT Elapsed: 0s
10:03:51.727043 IDE <-- LS NOTIF $/progress
10:03:51.727043 OUT Elapsed: 0s
10:03:51.728073 IN Elapsed: 1.5446ms
10:03:51.728599 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.728599                             $/progress: backgroundIndexProgress REPORT, 9/27, 33.0%
10:03:51.728599 IN Elapsed: 0s
10:03:51.728599 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.728599                             $/progress: backgroundIndexProgress REPORT, 9/27, 33.0%
10:03:51.728599 IDE <-- LS NOTIF $/progress
10:03:51.728599 OUT Elapsed: 0s
10:03:51.728599 IDE <-- LS NOTIF $/progress
10:03:51.728599 OUT Elapsed: 0s
10:03:51.751745 IN Elapsed: 23.1452ms
10:03:51.751745 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.751745                             $/progress: backgroundIndexProgress REPORT, 10/27, 37.0%
10:03:51.751745 IN Elapsed: 0s
10:03:51.751745 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.751745                             $/progress: backgroundIndexProgress REPORT, 10/27, 37.0%
10:03:51.751745 IDE <-- LS NOTIF $/progress
10:03:51.751745 OUT Elapsed: 0s
10:03:51.751745 IDE <-- LS NOTIF $/progress
10:03:51.751745 OUT Elapsed: 0s
10:03:51.786405 IN Elapsed: 34.6602ms
10:03:51.786405 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.786405                             $/progress: backgroundIndexProgress REPORT, 11/27, 40.0%
10:03:51.786405 IN Elapsed: 0s
10:03:51.786405 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.786405                             $/progress: backgroundIndexProgress REPORT, 11/27, 40.0%
10:03:51.786405 IDE <-- LS NOTIF $/progress
10:03:51.786405 OUT Elapsed: 0s
10:03:51.786405 IDE <-- LS NOTIF $/progress
10:03:51.786405 OUT Elapsed: 0s
10:03:51.820981 IN Elapsed: 34.5762ms
10:03:51.820981 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.821979                             $/progress: backgroundIndexProgress REPORT, 12/27, 44.0%
10:03:51.822081 IDE <-- LS NOTIF $/progress
10:03:51.822081 OUT Elapsed: 0s
10:03:51.822081 IN Elapsed: 0s
10:03:51.822081 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.822081                             $/progress: backgroundIndexProgress REPORT, 12/27, 44.0%
10:03:51.822600 IDE <-- LS NOTIF $/progress
10:03:51.822600 OUT Elapsed: 0s
10:03:51.823117 IN Elapsed: 516.8µs
10:03:51.823117 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.823117                             $/progress: backgroundIndexProgress REPORT, 13/27, 48.0%
10:03:51.823631 IN Elapsed: 514.4µs
10:03:51.823631 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.823631                             $/progress: backgroundIndexProgress REPORT, 13/27, 48.0%
10:03:51.823631 IDE <-- LS NOTIF $/progress
10:03:51.823631 OUT Elapsed: 0s
10:03:51.823631 IDE <-- LS NOTIF $/progress
10:03:51.824150 OUT Elapsed: 0s
10:03:51.833020 IN Elapsed: 9.3889ms
10:03:51.833020 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.833020                             $/progress: backgroundIndexProgress REPORT, 14/27, 51.0%
10:03:51.833537 IDE <-- LS NOTIF $/progress
10:03:51.833537 OUT Elapsed: 0s
10:03:51.833537 IN Elapsed: 0s
10:03:51.833537 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.833537                             $/progress: backgroundIndexProgress REPORT, 14/27, 51.0%
10:03:51.834568 IDE <-- LS NOTIF $/progress
10:03:51.834568 OUT Elapsed: 0s
10:03:51.911945 IN Elapsed: 78.4076ms
10:03:51.911945 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.911945                             $/progress: backgroundIndexProgress REPORT, 15/27, 55.0%
10:03:51.911945 IDE <-- LS NOTIF $/progress
10:03:51.911945 OUT Elapsed: 0s
10:03:51.911945 IN Elapsed: 0s
10:03:51.911945 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.911945                             $/progress: backgroundIndexProgress REPORT, 15/27, 55.0%
10:03:51.912458 IDE <-- LS NOTIF $/progress
10:03:51.912458 OUT Elapsed: 0s
10:03:51.916586 IN Elapsed: 4.6414ms
10:03:51.916586 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.916586                             $/progress: backgroundIndexProgress REPORT, 16/27, 59.0%
10:03:51.916586 IN Elapsed: 0s
10:03:51.916586 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.916586                             $/progress: backgroundIndexProgress REPORT, 16/27, 59.0%
10:03:51.916586 IDE <-- LS NOTIF $/progress
10:03:51.916586 OUT Elapsed: 0s
10:03:51.916586 IDE <-- LS NOTIF $/progress
10:03:51.917100 OUT Elapsed: 0s
10:03:51.933127 IN Elapsed: 16.5408ms
10:03:51.933127 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.933127                             $/progress: backgroundIndexProgress REPORT, 17/27, 62.0%
10:03:51.933127 IDE <-- LS NOTIF $/progress
10:03:51.933644 OUT Elapsed: 517.4µs
10:03:51.933127 IN Elapsed: 0s
10:03:51.933644 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.933644                             $/progress: backgroundIndexProgress REPORT, 17/27, 62.0%
10:03:51.933644 IN Elapsed: 0s
10:03:51.933644 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.933644                             $/progress: backgroundIndexProgress REPORT, 18/27, 66.0%
10:03:51.933644 IN Elapsed: 0s
10:03:51.933644 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.933644                             $/progress: backgroundIndexProgress REPORT, 18/27, 66.0%
10:03:51.933644 IDE <-- LS NOTIF $/progress
10:03:51.934229 OUT Elapsed: 584.6µs
10:03:51.978076 IN Elapsed: 44.4314ms
10:03:51.978076 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.978076                             $/progress: backgroundIndexProgress REPORT, 19/27, 70.0%
10:03:51.978076 IN Elapsed: 0s
10:03:51.978578 IDE     LS <-- Clangd NOTIF $/progress
10:03:51.978591                             $/progress: backgroundIndexProgress REPORT, 19/27, 70.0%
10:03:51.978076 IDE <-- LS NOTIF $/progress
10:03:51.978591 OUT Elapsed: 0s
10:03:51.978591 IDE <-- LS NOTIF $/progress
10:03:51.978591 OUT Elapsed: 0s
10:03:52.008543 IN Elapsed: 29.9522ms
10:03:52.008543 IDE     LS <-- Clangd NOTIF $/progress
10:03:52.008543                             $/progress: backgroundIndexProgress REPORT, 20/27, 74.0%
10:03:52.008543 IN Elapsed: 0s
10:03:52.008543 IDE     LS <-- Clangd NOTIF $/progress
10:03:52.008543                             $/progress: backgroundIndexProgress REPORT, 20/27, 74.0%
10:03:52.008543 IDE <-- LS NOTIF $/progress
10:03:52.008543 OUT Elapsed: 0s
10:03:52.008543 IDE <-- LS NOTIF $/progress
10:03:52.008543 OUT Elapsed: 0s
10:03:52.026046 IN Elapsed: 16.9994ms
10:03:52.026046 IDE     LS <-- Clangd NOTIF $/progress
10:03:52.026118                             $/progress: backgroundIndexProgress REPORT, 21/27, 77.0%
10:03:52.026118 IN Elapsed: 0s
10:03:52.026118 IDE     LS <-- Clangd NOTIF $/progress
10:03:52.026118                             $/progress: backgroundIndexProgress REPORT, 21/27, 77.0%
10:03:52.026118 IDE <-- LS NOTIF $/progress
10:03:52.026118 OUT Elapsed: 0s
10:03:52.026118 IDE <-- LS NOTIF $/progress
10:03:52.026655 OUT Elapsed: 32.9µs
10:03:52.027687 IN Elapsed: 1.5692ms
10:03:52.027687 IDE     LS <-- Clangd NOTIF $/progress
10:03:52.028203                             $/progress: backgroundIndexProgress REPORT, 22/27, 81.0%
10:03:52.028203 IDE <-- LS NOTIF $/progress
10:03:52.028203 OUT Elapsed: 0s
10:03:52.036263 IN Elapsed: 8.06ms
10:03:52.036263 IDE     LS <-- Clangd NOTIF $/progress
10:03:52.036263                             $/progress: backgroundIndexProgress REPORT, 23/27, 85.0%
10:03:52.036263 IDE <-- LS NOTIF $/progress
10:03:52.036263 OUT Elapsed: 0s
10:03:52.061237 IN Elapsed: 24.9746ms
10:03:52.061237 IDE     LS <-- Clangd NOTIF $/progress
10:03:52.061237                             $/progress: backgroundIndexProgress REPORT, 24/27, 88.0%
10:03:52.061237 IDE <-- LS NOTIF $/progress
10:03:52.061237 OUT Elapsed: 0s
10:03:52.089584 IN Elapsed: 28.3469ms
10:03:52.089584 IDE     LS <-- Clangd NOTIF $/progress
10:03:52.089584                             $/progress: backgroundIndexProgress REPORT, 25/27, 92.0%
10:03:52.089584 IDE <-- LS NOTIF $/progress
10:03:52.089584 OUT Elapsed: 0s
10:03:52.112217 IN Elapsed: 22.6331ms
10:03:52.112217 IDE     LS <-- Clangd NOTIF $/progress
10:03:52.112217                             $/progress: backgroundIndexProgress REPORT, 26/27, 96.0%
10:03:52.112217 IDE <-- LS NOTIF $/progress
10:03:52.112217 OUT Elapsed: 0s
10:03:52.172187 IN Elapsed: 59.9694ms
10:03:52.172187 IDE     LS <-- Clangd NOTIF $/progress
10:03:52.172187                             $/progress: backgroundIndexProgress END 
10:03:52.172187 IDE <-- LS NOTIF $/progress
10:03:52.172698 OUT Elapsed: 511.3µs
10:03:52.248848 IN Elapsed: 997.778ms
10:03:52.248848 IDE --> LS NOTIF ino/didCompleteBuild
10:03:52.248848                  ino/didCompleteBuild: write-locked
10:03:52.252522                  ino/didCompleteBuild: Updated 'libraries.cache'. Copied: C:\Users\Administrator\AppData\Local\Temp\arduino-sketch-31A9A4270AEAD423CD6B51954EDE7DB3\libraries.cache to C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\libraries.cache
10:03:52.252522                  ino/didCompleteBuild: write-unlocked
10:03:53.257987 SKETCH REBUILD: : Sketch rebuild started
10:03:53.257987 IDE <-- LS REQU window/workDoneProgress/create 2
10:03:53.257987 SKETCH REBUILD: : read-locked
10:03:53.257987 SKETCH REBUILD: : read-unlocked
10:03:53.257987 OUT Elapsed: 0s
10:03:53.258502 IN Elapsed: 1.0059798s
10:03:53.258502 IDE --> LS RESP window/workDoneProgress/create 2
10:03:53.258502 IDE <-- LS NOTIF $/progress
10:03:53.258502 OUT Elapsed: 0s
10:03:53.568743 SKETCH REBUILD: : Running build with: {
  "instance": {
    "id": 1
  },
  "fqbn": "arduino:avr:uno",
  "sketch_path": "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣器等等传感器\\Code\\Lesson 5_Active_buzzer\\5_Active_buzzer",
  "build_path": "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420",
  "verbose": true,
  "create_compilation_database_only": true,
  "source_override": {
    "5_Active_buzzer.ino": "\r\n#include \"pitches.h\"// notes in the melody:\r\nint melody[] = {\r\nNOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};\r\nint duration = 500;  // 500 miliseconds \r\nvoid setup() {  }\r\nvoid loop() {\r\nfor (int thisNote = 0; thisNote \u003c 12; thisNote++) {\r\n// pin12 output the voice, every scale is 0.5 sencond \r\ntone(12, melody[thisNote], duration);\r\ndelay(100);\r\n// Output the voice after several minutes\r\ndelay(100);\r\n} // restart after two seconds \r\ndelay(200);\r\n}\r\n",
    "pitches.h": "/*************************************************\r\n* Public Constants\r\n*************************************************/\r\n\r\n#define NOTE_B0 31\r\n#define NOTE_C1 33\r\n#define NOTE_CS1 35\r\n#define NOTE_D1 37\r\n#define NOTE_DS1 39\r\n#define NOTE_E1 41\r\n#define NOTE_F1 44\r\n#define NOTE_FS1 46\r\n#define NOTE_G1 49\r\n#define NOTE_GS1 52\r\n#define NOTE_A1 55\r\n#define NOTE_AS1 58\r\n#define NOTE_B1 62\r\n#define NOTE_C2 65\r\n#define NOTE_CS2 69\r\n#define NOTE_D2 73\r\n#define NOTE_DS2 78\r\n#define NOTE_E2 82\r\n#define NOTE_F2 87\r\n#define NOTE_FS2 93\r\n#define NOTE_G2 98\r\n#define NOTE_GS2 104\r\n#define NOTE_A2 110\r\n#define NOTE_AS2 117\r\n#define NOTE_B2 123\r\n#define NOTE_C3 131\r\n#define NOTE_CS3 139\r\n#define NOTE_D3 147\r\n#define NOTE_DS3 156\r\n#define NOTE_E3 165\r\n#define NOTE_F3 175\r\n#define NOTE_FS3 185\r\n#define NOTE_G3 196\r\n#define NOTE_GS3 208\r\n#define NOTE_A3 220\r\n#define NOTE_AS3 233\r\n#define NOTE_B3 247\r\n#define NOTE_C4 262\r\n#define NOTE_CS4 277\r\n#define NOTE_D4 294\r\n#define NOTE_DS4 311\r\n#define NOTE_E4 330\r\n#define NOTE_F4 349\r\n#define NOTE_FS4 370\r\n#define NOTE_G4 392\r\n#define NOTE_GS4 415\r\n#define NOTE_A4 440\r\n#define NOTE_AS4 466\r\n#define NOTE_B4 494\r\n#define NOTE_C5 523\r\n#define NOTE_CS5 554\r\n#define NOTE_D5 587\r\n#define NOTE_DS5 622\r\n#define NOTE_E5 659\r\n#define NOTE_F5 698\r\n#define NOTE_FS5 740\r\n#define NOTE_G5 784\r\n#define NOTE_GS5 831\r\n#define NOTE_A5 880\r\n#define NOTE_AS5 932\r\n#define NOTE_B5 988\r\n#define NOTE_C6 1047\r\n#define NOTE_CS6 1109\r\n#define NOTE_D6 1175\r\n#define NOTE_DS6 1245\r\n#define NOTE_E6 1319\r\n#define NOTE_F6 1397\r\n#define NOTE_FS6 1480\r\n#define NOTE_G6 1568\r\n#define NOTE_GS6 1661\r\n#define NOTE_A6 1760\r\n#define NOTE_AS6 1865\r\n#define NOTE_B6 1976\r\n#define NOTE_C7 2093\r\n#define NOTE_CS7 2217\r\n#define NOTE_D7 2349\r\n#define NOTE_DS7 2489\r\n#define NOTE_E7 2637\r\n#define NOTE_F7 2794\r\n#define NOTE_FS7 2960\r\n#define NOTE_G7 3136\r\n#define NOTE_GS7 3322\r\n#define NOTE_A7 3520\r\n#define NOTE_AS7 3729\r\n#define NOTE_B7 3951\r\n#define NOTE_C8 4186\r\n#define NOTE_CS8 4435\r\n#define NOTE_D8 4699\r\n#define NOTE_DS8 4978\r\n"
  },
  "skip_libraries_discovery": true
}
10:03:53.958482 SKETCH REBUILD: : Compile successful!
10:03:53.993618 SKETCH REBUILD: : write-locked
10:03:53.997927   > Current sketchmapper content:
10:03:53.997927   0: #include <Arduino.h>                                         | /not-ino:0                                         
10:03:53.997927   1: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:03:53.997927   2:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:0                          
10:03:53.997927   3: #include "pitches.h"// notes in the melody:                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:1                          
10:03:53.997927   4: int melody[] = {                                             | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:2                          
10:03:53.997927   5: NOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:3                          
10:03:53.997927   6: int duration = 500;  // 500 miliseconds                      | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:4                          
10:03:53.997927   7: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:03:53.997927   8: void setup();                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5
10:03:53.997927   9: #line 7 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:03:53.997927  10: void loop();                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6
10:03:53.997927  11: #line 6 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:03:53.997927  12: void setup() {  }                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:5                          
10:03:53.997927  13: void loop() {                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:6                          
10:03:53.997927  14: for (int thisNote = 0; thisNote < 12; thisNote++) {          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:7                          
10:03:53.997927  15: // pin12 output the voice, every scale is 0.5 sencond        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:8                          
10:03:53.997927  16: tone(12, melody[thisNote], duration);                        | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:9                          
10:03:53.997927  17: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:10                          
10:03:53.997927  18: // Output the voice after several minutes                    | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:11                          
10:03:53.997927  19: delay(100);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:12                          
10:03:53.997927  20: } // restart after two seconds                               | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:13                          
10:03:53.997927  21: delay(200);                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:14                          
10:03:53.997927  22: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:15                          
10:03:53.997927  23:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:16                          
10:03:53.997927  24:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:17                          
10:03:53.997927 SKETCH REBUILD: : Sending 'didSave' notification to Clangd
10:03:53.997927 IDE     LS --> Clangd NOTIF textDocument/didSave
10:03:53.997927 OUT Elapsed: 0s
10:03:53.997927 SKETCH REBUILD: : Sending full-text 'didChange' notification to Clangd
10:03:53.997927 IDE     LS --> Clangd NOTIF textDocument/didChange
10:03:53.998900 OUT Elapsed: 0s
10:03:53.998900 SKETCH REBUILD: : write-unlocked
10:03:53.998900 IDE <-- LS NOTIF $/progress
10:03:53.998900 OUT Elapsed: 0s
10:03:54.196421 IN Elapsed: 2.0242346s
10:03:54.196421 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
10:03:54.196421                             textDocument/publishDiagnostics: Ignored by configuration
10:04:04.248940 IN Elapsed: 10.9904387s
10:04:04.248940 IDE --> LS REQU textDocument/hover 4
10:04:04.248940                 textDocument/hover 4: read-locked
10:04:04.251691                 textDocument/hover 4: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp
10:04:04.255074                 textDocument/hover 4: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:13 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:13:13
10:04:04.255074 IDE     LS --> Clangd REQU textDocument/hover 5
10:04:04.255074 OUT Elapsed: 0s
10:04:04.261897 IN Elapsed: 10.0654759s
10:04:04.261897 IDE     LS <-- Clangd RESP textDocument/hover 5
10:04:04.262400                 textDocument/hover 4: null response
10:04:04.262417                 textDocument/hover 4: read-unlocked
10:04:04.262417 IDE <-- LS RESP textDocument/hover 4
10:04:04.262417 OUT Elapsed: 0s
10:04:06.231600 IN Elapsed: 1.9690568s
10:04:06.231600 IDE --> LS REQU textDocument/documentSymbol 5
10:04:06.232314                 textDocument/documentSymbol 5: read-locked
10:04:06.237821                 textDocument/documentSymbol 5: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/pitches.h -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/pitches.h
10:04:06.237902 IDE     LS --> Clangd REQU textDocument/documentSymbol 6
10:04:06.238034 OUT Elapsed: 131.8µs
10:04:06.238034 IN Elapsed: 1.9761363s
10:04:06.238034 IDE     LS <-- Clangd RESP textDocument/documentSymbol 6
10:04:06.238034                 textDocument/documentSymbol 5: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/pitches.h (0 document symbols)
10:04:06.238034                 textDocument/documentSymbol 5: read-unlocked
10:04:06.238034 IDE <-- LS RESP textDocument/documentSymbol 5
10:04:06.238034 OUT Elapsed: 0s
10:04:11.460427 IN Elapsed: 5.2223938s
10:04:11.460427 IDE --> LS REQU textDocument/documentSymbol 6
10:04:11.460427                 textDocument/documentSymbol 6: read-locked
10:04:11.462968                 textDocument/documentSymbol 6: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp
10:04:11.462968 IDE     LS --> Clangd REQU textDocument/documentSymbol 7
10:04:11.463471 OUT Elapsed: 503.1µs
10:04:11.467230 IN Elapsed: 5.2291969s
10:04:11.467275 IDE     LS <-- Clangd RESP textDocument/documentSymbol 7
10:04:11.467275                 textDocument/documentSymbol 6: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp (6 document symbols)
10:04:11.467275                 textDocument/documentSymbol 6:   > convert SymbolKind:Variable 4:0-5:71
10:04:11.468978                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:4:0-5:71 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:0-3:71 (.ino)
10:04:11.470541                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:4:4-4:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:2:4-2:10 (.ino)
10:04:11.470541                 textDocument/documentSymbol 6: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:04:11.470541                 textDocument/documentSymbol 6:   > convert SymbolKind:Variable 6:0-6:18
10:04:11.472129                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:6:0-6:18 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:0-4:18 (.ino)
10:04:11.474198                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:6:4-6:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:4:4-4:12 (.ino)
10:04:11.474198                 textDocument/documentSymbol 6: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:04:11.474198                 textDocument/documentSymbol 6:   > convert SymbolKind:Function 8:0-8:12
10:04:11.475728                 textDocument/documentSymbol 6: Range is in PREPROCESSED section of the sketch
10:04:11.475728                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:8:0-8:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:12 (.ino)
10:04:11.475728                 textDocument/documentSymbol 6:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
10:04:11.475728                 textDocument/documentSymbol 6:   > convert SymbolKind:Function 10:0-10:11
10:04:11.477258                 textDocument/documentSymbol 6: Range is in PREPROCESSED section of the sketch
10:04:11.477258                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:10:0-10:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-6:11 (.ino)
10:04:11.477258                 textDocument/documentSymbol 6:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
10:04:11.477258                 textDocument/documentSymbol 6:   > convert SymbolKind:Function 12:0-12:17
10:04:11.478785                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:12:0-12:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:0-5:17 (.ino)
10:04:11.480313                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:12:5-12:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:5-5:10 (.ino)
10:04:11.480313                 textDocument/documentSymbol 6: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:04:11.480313                 textDocument/documentSymbol 6:   > convert SymbolKind:Function 13:0-22:1
10:04:11.481839                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:13:0-22:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:0-15:1 (.ino)
10:04:11.483056                 textDocument/documentSymbol 6: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:13:5-13:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:5-6:9 (.ino)
10:04:11.483056                 textDocument/documentSymbol 6: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp (0 document symbols)
10:04:11.483056                 textDocument/documentSymbol 6: read-unlocked
10:04:11.483056 IDE <-- LS RESP textDocument/documentSymbol 6
10:04:11.483665 OUT Elapsed: 0s
10:04:22.939360 IN Elapsed: 11.4556951s
10:04:22.939360 IDE --> LS REQU textDocument/hover 7
10:04:22.939360                 textDocument/hover 7: read-locked
10:04:22.940684                 textDocument/hover 7: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp
10:04:22.944475                 textDocument/hover 7: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:8:17 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:15:17
10:04:22.944475 IDE     LS --> Clangd REQU textDocument/hover 8
10:04:22.944475 OUT Elapsed: 0s
10:04:22.951400 IN Elapsed: 11.4841248s
10:04:22.951400 IDE     LS <-- Clangd RESP textDocument/hover 8
10:04:22.951400                 textDocument/hover 7: null response
10:04:22.951400                 textDocument/hover 7: read-unlocked
10:04:22.951400 IDE <-- LS RESP textDocument/hover 7
10:04:22.951400 OUT Elapsed: 0s
10:04:23.342252 IN Elapsed: 390.8516ms
10:04:23.342252 IDE --> LS REQU textDocument/hover 8
10:04:23.343596                 textDocument/hover 8: read-locked
10:04:23.348739                 textDocument/hover 8: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp
10:04:23.351993                 textDocument/hover 8: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:7:16 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:14:16
10:04:23.351993 IDE     LS --> Clangd REQU textDocument/hover 9
10:04:23.351993 OUT Elapsed: 0s
10:04:23.355809 IN Elapsed: 404.4086ms
10:04:23.357183 IDE     LS <-- Clangd RESP textDocument/hover 9
10:04:23.358795                 textDocument/hover 8: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:14:9-14:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:7:9-7:17 (.ino)
10:04:23.358795                 textDocument/hover 8: Hover content: "### variable `thisNote`  \n\n---\nType: `int`  \nValue = `0`  \n\n---\n```cpp\n// In loop\nint thisNote = 0\n```"
10:04:23.358795                 textDocument/hover 8: read-unlocked
10:04:23.358795 IDE <-- LS RESP textDocument/hover 8
10:04:23.358795 OUT Elapsed: 0s
10:04:28.288147 IN Elapsed: 4.9293524s
10:04:28.288147 IDE --> LS REQU textDocument/hover 9
10:04:28.288147                 textDocument/hover 9: read-locked
10:04:28.289182                 textDocument/hover 9: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp
10:04:28.292759                 textDocument/hover 9: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:5:14 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:12:14
10:04:28.292759 IDE     LS --> Clangd REQU textDocument/hover 10
10:04:28.292759 OUT Elapsed: 0s
10:04:28.299468 IN Elapsed: 4.9423652s
10:04:28.299468 IDE     LS <-- Clangd RESP textDocument/hover 10
10:04:28.299971                 textDocument/hover 9: null response
10:04:28.299971                 textDocument/hover 9: read-unlocked
10:04:28.299971 IDE <-- LS RESP textDocument/hover 9
10:04:28.300038 OUT Elapsed: 0s
10:07:26.605062 IN Elapsed: 2m58.3050235s
10:07:26.605062 IDE --> LS REQU textDocument/codeAction 10
10:07:26.605062                 textDocument/codeAction 10: read-locked
10:07:26.605062                 textDocument/codeAction 10: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:15:1)
10:07:26.606148                 textDocument/codeAction 10: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp
10:07:26.609857                 textDocument/codeAction 10:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:15:1)
10:07:26.609857 IDE     LS --> Clangd REQU textDocument/codeAction 11
10:07:26.609857 OUT Elapsed: 0s
10:07:26.613953 IN Elapsed: 2m58.3144849s
10:07:26.613953 IDE     LS <-- Clangd RESP textDocument/codeAction 11
10:07:26.613953                 textDocument/codeAction 10: read-unlocked
10:07:26.613953 IDE <-- LS RESP textDocument/codeAction 10
10:07:26.613953 OUT Elapsed: 0s
10:07:52.589668 IN Elapsed: 25.9757147s
10:07:52.589668 IDE --> LS REQU textDocument/codeAction 11
10:07:52.589668                 textDocument/codeAction 11: read-locked
10:07:52.589668                 textDocument/codeAction 11: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:1:0)
10:07:52.590855                 textDocument/codeAction 11: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp
10:07:52.594591                 textDocument/codeAction 11:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:1:0)
10:07:52.594591 IDE     LS --> Clangd REQU textDocument/codeAction 12
10:07:52.594591 OUT Elapsed: 0s
10:07:52.598409 IN Elapsed: 25.9844565s
10:07:52.598409 IDE     LS <-- Clangd RESP textDocument/codeAction 12
10:07:52.598409                 textDocument/codeAction 11: read-unlocked
10:07:52.598409 IDE <-- LS RESP textDocument/codeAction 11
10:07:52.598409 OUT Elapsed: 0s
10:07:53.347165 IN Elapsed: 748.7556ms
10:07:53.347222 IDE --> LS REQU textDocument/hover 12
10:07:53.347269                 textDocument/hover 12: read-locked
10:07:53.348479                 textDocument/hover 12: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp
10:07:53.351792                 textDocument/hover 12: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:7:13 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:14:13
10:07:53.352326 IDE     LS --> Clangd REQU textDocument/hover 13
10:07:53.352326 OUT Elapsed: 0s
10:07:53.356110 IN Elapsed: 757.7005ms
10:07:53.356110 IDE     LS <-- Clangd RESP textDocument/hover 13
10:07:53.357735                 textDocument/hover 12: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:14:9-14:17 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:7:9-7:17 (.ino)
10:07:53.357735                 textDocument/hover 12: Hover content: "### variable `thisNote`  \n\n---\nType: `int`  \nValue = `0`  \n\n---\n```cpp\n// In loop\nint thisNote = 0\n```"
10:07:53.357735                 textDocument/hover 12: read-unlocked
10:07:53.357735 IDE <-- LS RESP textDocument/hover 12
10:07:53.358238 OUT Elapsed: 502.6µs
10:07:53.550709 IN Elapsed: 192.471ms
10:07:53.550709 IDE --> LS REQU textDocument/hover 13
10:07:53.550709                 textDocument/hover 13: read-locked
10:07:53.551740                 textDocument/hover 13: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp
10:07:53.555424                 textDocument/hover 13: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:6:13 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:13:13
10:07:53.555424 IDE     LS --> Clangd REQU textDocument/hover 14
10:07:53.555424 OUT Elapsed: 0s
10:07:53.559054 IN Elapsed: 202.9439ms
10:07:53.559054 IDE     LS <-- Clangd RESP textDocument/hover 14
10:07:53.559054                 textDocument/hover 13: null response
10:07:53.559054                 textDocument/hover 13: read-unlocked
10:07:53.559054 IDE <-- LS RESP textDocument/hover 13
10:07:53.559054 OUT Elapsed: 0s
10:07:54.468978 IN Elapsed: 909.9241ms
10:07:54.468978 IDE --> LS REQU textDocument/definition 14
10:07:54.468978                 textDocument/definition 14: read-locked
10:07:54.470075                 textDocument/definition 14: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp
10:07:54.473966                 textDocument/definition 14: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:8:17 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:15:17
10:07:54.473966 IDE     LS --> Clangd REQU textDocument/definition 15
10:07:54.473966 OUT Elapsed: 0s
10:07:54.473966 IN Elapsed: 914.9126ms
10:07:54.474470 IDE     LS <-- Clangd RESP textDocument/definition 15
10:07:54.474512                 textDocument/definition 14: read-unlocked
10:07:54.474512 IDE <-- LS RESP textDocument/definition 14
10:07:54.474512 OUT Elapsed: 0s
10:07:54.988730 IN Elapsed: 514.2184ms
10:07:54.988852 IDE --> LS REQU textDocument/definition 15
10:07:54.988883                 textDocument/definition 15: read-locked
10:07:54.990170                 textDocument/definition 15: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp
10:07:54.993971                 textDocument/definition 15: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:11:26 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:18:26
10:07:54.993971 IDE     LS --> Clangd REQU textDocument/definition 16
10:07:54.993971 OUT Elapsed: 0s
10:07:54.993971 IN Elapsed: 519.5013ms
10:07:54.993971 IDE     LS <-- Clangd RESP textDocument/definition 16
10:07:54.993971                 textDocument/definition 15: read-unlocked
10:07:54.994483 IDE <-- LS RESP textDocument/definition 15
10:07:54.994483 OUT Elapsed: 0s
10:07:55.676127 IN Elapsed: 681.6442ms
10:07:55.676127 IDE --> LS REQU textDocument/codeAction 16
10:07:55.676127                 textDocument/codeAction 16: read-locked
10:07:55.676127                 textDocument/codeAction 16: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino:14:11)
10:07:55.677219                 textDocument/codeAction 16: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer/5_Active_buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp
10:07:55.680929                 textDocument/codeAction 16:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp:14:11)
10:07:55.680929 IDE     LS --> Clangd REQU textDocument/codeAction 17
10:07:55.680929 OUT Elapsed: 0s
10:07:55.680929 IN Elapsed: 686.9575ms
10:07:55.680929 IDE     LS <-- Clangd RESP textDocument/codeAction 17
10:07:55.680929                 textDocument/codeAction 16: read-unlocked
10:07:55.681432 IDE <-- LS RESP textDocument/codeAction 16
10:07:55.681487 OUT Elapsed: 55.5µs
10:22:57.985461 IN Elapsed: 15m2.3039736s
10:22:57.985461 IDE --> LS REQU shutdown 17
10:22:57.985964 IDE     LS --> Clangd REQU shutdown 18
10:22:57.986594 OUT Elapsed: 503.7µs
10:22:57.987370 IN Elapsed: 15m2.306441s
10:22:57.987370 IDE     LS <-- Clangd RESP shutdown 18
10:22:57.987370 IDE <-- LS RESP shutdown 17
10:22:57.987370 OUT Elapsed: 0s
10:22:57.987957 IN Elapsed: 587.2µs
10:22:57.988460 IDE --> LS NOTIF exit
10:22:57.988460 IDE     LS --> Clangd NOTIF exit
10:22:57.988460 OUT Elapsed: 0s
10:22:57.988460                  exit: Arduino Language Server is shutting down.
