






Started logging.
I[10:51:23.982] clangd version 14.0.0
I[10:51:23.984] Features: windows
I[10:51:23.984] PID: 11336
I[10:51:23.984] Working directory: g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYC0076拍照麦克轮WiFi小车\ZYC0076\4_Arduino_Code\1_Auto_move
I[10:51:23.984] argv[0]: d:\Program Files\Arduino IDE\resources\app\node_modules\arduino-ide-extension\build\clangd.exe
I[10:51:23.984] argv[1]: -log=verbose
I[10:51:23.984] argv[2]: --compile-commands-dir=C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533
I[10:51:23.984] argv[3]: -query-driver=C:\Users\Administrator\AppData\Local\Arduino15\packages\**
V[10:51:23.991] User config file is C:\Users\Administrator\AppData\Local\clangd\config.yaml
I[10:51:23.991] Starting LSP over stdin/stdout
V[10:51:23.991] <<< {"id":"1","jsonrpc":"2.0","method":"initialize","params":{"capabilities":{"textDocument":{"codeAction":{"codeActionLiteralSupport":{"codeActionKind":{"valueSet":["","quickfix","refactor","refactor.extract","refactor.inline","refactor.rewrite","source","source.organizeImports"]}},"dynamicRegistration":true,"isPreferredSupport":true},"codeLens":{"dynamicRegistration":true},"colorProvider":{"dynamicRegistration":true},"completion":{"completionItem":{"commitCharactersSupport":true,"deprecatedSupport":true,"documentationFormat":["markdown","plaintext"],"preselectSupport":true,"snippetSupport":true,"tagSupport":{"valueSet":[1]}},"completionItemKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25]},"contextSupport":true,"dynamicRegistration":true},"declaration":{"dynamicRegistration":true,"linkSupport":true},"definition":{"dynamicRegistration":true,"linkSupport":true},"documentHighlight":{"dynamicRegistration":true},"documentLink":{"dynamicRegistration":true,"tooltipSupport":true},"documentSymbol":{"dynamicRegistration":true,"hierarchicalDocumentSymbolSupport":true,"symbolKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26]}},"foldingRange":{"dynamicRegistration":true,"lineFoldingOnly":true,"rangeLimit":5000},"formatting":{"dynamicRegistration":true},"hover":{"contentFormat":["markdown","plaintext"],"dynamicRegistration":true},"implementation":{"dynamicRegistration":true,"linkSupport":true},"onTypeFormatting":{"dynamicRegistration":true},"publishDiagnostics":{"relatedInformation":true,"tagSupport":{"valueSet":[1,2]}},"rangeFormatting":{"dynamicRegistration":true},"references":{"dynamicRegistration":true},"rename":{"dynamicRegistration":true,"prepareSupport":true},"selectionRange":{"dynamicRegistration":true},"signatureHelp":{"contextSupport":true,"dynamicRegistration":true,"signatureInformation":{"documentationFormat":["markdown","plaintext"],"parameterInformation":{"labelOffsetSupport":true}}},"synchronization":{"didSave":true,"dynamicRegistration":true,"willSave":true,"willSaveWaitUntil":true},"typeDefinition":{"dynamicRegistration":true,"linkSupport":true}},"window":{"workDoneProgress":true},"workspace":{"applyEdit":true,"configuration":true,"didChangeConfiguration":{"dynamicRegistration":true},"didChangeWatchedFiles":{"dynamicRegistration":true},"executeCommand":{"dynamicRegistration":true},"symbol":{"dynamicRegistration":true,"symbolKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26]}},"workspaceEdit":{"documentChanges":true,"failureHandling":"textOnlyTransactional","resourceOperations":["create","rename","delete"]},"workspaceFolders":true}},"clientInfo":{"name":"vscode","version":"1.53.2"},"initializationOptions":{},"processId":512,"rootPath":"C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch","rootUri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch","trace":"off","workspaceFolders":[{"name":"1_Auto_move","uri":"file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYC0076%E6%8B%8D%E7%85%A7%E9%BA%A6%E5%85%8B%E8%BD%AEWiFi%E5%B0%8F%E8%BD%A6/ZYC0076/4_Arduino_Code/1_Auto_move"}]}}

I[10:51:23.991] <-- initialize("1")
I[10:51:24.052] --> reply:initialize("1") 60 ms
V[10:51:24.052] >>> {"id":"1","jsonrpc":"2.0","result":{"capabilities":{"astProvider":true,"callHierarchyProvider":true,"clangdInlayHintsProvider":true,"codeActionProvider":{"codeActionKinds":["quickfix","refactor","info"]},"compilationDatabase":{"automaticReload":true},"completionProvider":{"allCommitCharacters":[" ","\t","(",")","[","]","{","}","<",">",":",";",",","+","-","/","*","%","^","&","#","?",".","=","\"","'","|"],"resolveProvider":false,"triggerCharacters":[".","<",">",":","\"","/","*"]},"declarationProvider":true,"definitionProvider":true,"documentFormattingProvider":true,"documentHighlightProvider":true,"documentLinkProvider":{"resolveProvider":false},"documentOnTypeFormattingProvider":{"firstTriggerCharacter":"\n","moreTriggerCharacter":[]},"documentRangeFormattingProvider":true,"documentSymbolProvider":true,"executeCommandProvider":{"commands":["clangd.applyFix","clangd.applyTweak"]},"hoverProvider":true,"implementationProvider":true,"memoryUsageProvider":true,"referencesProvider":true,"renameProvider":{"prepareProvider":true},"selectionRangeProvider":true,"semanticTokensProvider":{"full":{"delta":true},"legend":{"tokenModifiers":["declaration","deprecated","deduced","readonly","static","abstract","virtual","dependentName","defaultLibrary","usedAsMutableReference","functionScope","classScope","fileScope","globalScope"],"tokenTypes":["variable","variable","parameter","function","method","function","property","variable","class","interface","enum","enumMember","type","type","unknown","namespace","typeParameter","concept","type","macro","comment"]},"range":false},"signatureHelpProvider":{"triggerCharacters":["(",")","{","}","<",">",","]},"textDocumentSync":{"change":2,"openClose":true,"save":true},"typeDefinitionProvider":true,"typeHierarchyProvider":true,"workspaceSymbolProvider":true},"serverInfo":{"name":"clangd","version":"clangd version 14.0.0 windows x86_64-pc-windows-msvc"}}}

V[10:51:24.052] <<< {"jsonrpc":"2.0","method":"initialized","params":{}}

I[10:51:24.052] <-- initialized
V[10:51:24.059] <<< {"jsonrpc":"2.0","method":"textDocument/didOpen","params":{"textDocument":{"languageId":"cpp","text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\n// PWM 控制引脚\n#define PWM1_PIN            5\n#define PWM2_PIN            6      \n// 74HCT595N 芯片引脚\n#define SHCP_PIN            2                               // 位移时钟\n#define EN_PIN              7                               // 使能控制\n#define DATA_PIN            8                               // 串行数据\n#define STCP_PIN            4                               // 存储寄存器时钟          \n\nconst int Forward       = 92;                               // 前进\nconst int Backward      = 163;                              // 后退\nconst int Turn_Left     = 149;                              // 左平移\nconst int Turn_Right    = 106;                              // 右平移\nconst int Top_Left      = 20;                               // 左上移动\nconst int Bottom_Left   = 129;                              // 左下移动\nconst int Top_Right     = 72;                               // 右上移动\nconst int Bottom_Right  = 34;                               // 右下移动\nconst int Stop          = 0;                                // 停止\nconst int Contrarotate  = 172;                              // 逆时针旋转\nconst int Clockwise     = 83;                               // 顺时针旋转\n\n#line 22 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid setup();\n#line 32 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid loop();\n#line 69 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid Motor(int Dir, int Speed);\n#line 22 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid setup()\n{\n    pinMode(SHCP_PIN, OUTPUT);\n    pinMode(EN_PIN, OUTPUT);\n    pinMode(DATA_PIN, OUTPUT);\n    pinMode(STCP_PIN, OUTPUT);\n    pinMode(PWM1_PIN, OUTPUT);\n    pinMode(PWM2_PIN, OUTPUT);\n}\n\nvoid loop()\n{\n    /* 向前 */\n    Motor(Forward, 250);     \n    delay(2000);\n    /* 向后 */\n    Motor(Backward, 250);\n    delay(2000);\n    /* 左平移 */\n    Motor(Turn_Left, 250);\n    delay(2000);\n    /* 右平移 */\n    Motor(Turn_Right, 250);\n    delay(2000);\n    /* 左上移 */\n    Motor(Top_Left, 250);\n    delay(2000);\n    /* 右下移 */\n    Motor(Bottom_Right, 250);\n    delay(2000);\n    /* 左下移 */\n    Motor(Bottom_Left, 250);\n    delay(2000);\n    /* 右上移 */\n    Motor(Top_Right, 250);\n    delay(2000);\n    /* 原地顺时针转 */\n    Motor(Clockwise, 250);\n    delay(2000);\n    /* 原地逆时针转 */\n    Motor(Contrarotate, 250);\n    delay(2000);\n    /* 停止 */\n    Motor(Stop, 250);\n    delay(2000);\n}\n\nvoid Motor(int Dir, int Speed)\n{\n    digitalWrite(EN_PIN, LOW);\n    analogWrite(PWM1_PIN, Speed);\n    analogWrite(PWM2_PIN, Speed);\n\n    digitalWrite(STCP_PIN, LOW);\n    shiftOut(DATA_PIN, SHCP_PIN, MSBFIRST, Dir);\n    digitalWrite(STCP_PIN, HIGH);\n}\n","uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp","version":1}}}

I[10:51:24.059] <-- textDocument/didOpen
V[10:51:24.062] config note at C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\.clangd:1:0: Parsing config fragment
V[10:51:24.063] config note at C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\.clangd:1:0: Parsed 1 fragments from file
V[10:51:24.063] Config fragment: compiling C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\.clangd:1 -> 0x0000019E0E4F7100 (trusted=false)
I[10:51:24.063] --> textDocument/publishDiagnostics
V[10:51:24.063] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/.clangd"}}

V[10:51:24.064] <<< {"id":"2","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":30,"line":37},"start":{"character":30,"line":37}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:51:24.064] <-- textDocument/codeAction("2")
I[10:51:24.064] Loaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\compile_commands.json
V[10:51:24.065] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533
I[10:51:24.068] --> window/workDoneProgress/create(0)
V[10:51:24.068] >>> {"id":0,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[10:51:24.068] Enqueueing 26 commands for indexing
V[10:51:24.068] <<< {"id":0,"jsonrpc":"2.0","result":null}

I[10:51:24.068] <-- reply(0)
I[10:51:24.068] --> $/progress
V[10:51:24.068] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[10:51:24.068] --> $/progress
V[10:51:24.068] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[10:51:24.069] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp
V[10:51:24.069] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp
V[10:51:24.069] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c
V[10:51:24.069] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c
V[10:51:24.069] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp
V[10:51:24.069] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp
V[10:51:24.069] Failed to load shard: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
V[10:51:24.069] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp
V[10:51:24.069] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp
V[10:51:24.070] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp
V[10:51:24.070] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp
V[10:51:24.070] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S
V[10:51:24.070] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp
V[10:51:24.070] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp
V[10:51:24.070] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp
V[10:51:24.070] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp
V[10:51:24.070] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp
V[10:51:24.070] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c
V[10:51:24.070] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp
V[10:51:24.070] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c
V[10:51:24.071] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c
V[10:51:24.071] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp
V[10:51:24.071] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp
V[10:51:24.071] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c
V[10:51:24.071] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp
V[10:51:24.071] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c
I[10:51:24.076] --> $/progress
V[10:51:24.076] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[10:51:24.076] --> $/progress
V[10:51:24.076] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[10:51:24.076] --> $/progress
V[10:51:24.076] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[10:51:24.076] --> $/progress
V[10:51:24.076] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[10:51:24.076] --> $/progress
V[10:51:24.076] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[10:51:24.076] --> $/progress
V[10:51:24.076] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[10:51:24.076] --> $/progress
V[10:51:24.076] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[10:51:24.076] --> $/progress
V[10:51:24.076] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

V[10:51:24.182] System include extraction: target extracted: "avr"
V[10:51:24.182] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:51:24.182] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:51:24.182] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:51:24.182] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
I[10:51:24.183] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp version 1 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch\\1_Auto_move.ino.cpp"
V[10:51:24.186] System include extraction: target extracted: "avr"
V[10:51:24.186] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:51:24.186] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:51:24.186] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:51:24.186] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-gcc.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:51:24.188] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c (digest:=0A36B38756A4F148)
V[10:51:24.190] System include extraction: target extracted: "avr"
V[10:51:24.190] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:51:24.190] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:51:24.190] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:51:24.190] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:51:24.192] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp (digest:=1C31198B0754810E)
V[10:51:24.195] System include extraction: target extracted: "avr"
V[10:51:24.195] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:51:24.195] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:51:24.195] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:51:24.195] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:51:24.197] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp (digest:=81BB1157C290C33B)
V[10:51:24.208] System include extraction: target extracted: "avr"
V[10:51:24.208] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:51:24.208] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:51:24.208] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:51:24.208] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:51:24.210] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp (digest:=487C94A1A1F49B6C)
V[10:51:24.211] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 1_Auto_move.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch\\1_Auto_move.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch\\1_Auto_move.ino.cpp"
V[10:51:24.211] Building first preamble for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp version 1
V[10:51:24.213] System include extraction: target extracted: "avr"
V[10:51:24.213] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:51:24.213] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:51:24.213] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:51:24.213] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:51:24.215] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp (digest:=FDB5BCAAB3E73FCE)
V[10:51:24.233] System include extraction: target extracted: "avr"
V[10:51:24.233] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:51:24.233] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:51:24.233] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:51:24.233] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:51:24.237] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp (digest:=F7D59D2B49112307)
I[10:51:24.280] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c (311 symbols, 2694 refs, 25 files)
V[10:51:24.286] indexed preamble AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp version 1:
  symbol slab: 2505 symbols, 716894 bytes
  ref slab: 0 symbols, 0 refs, 136 bytes
  relations slab: 9 relations, 177 bytes
I[10:51:24.308] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp (600 symbols, 3432 refs, 36 files)
I[10:51:24.310] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp (600 symbols, 3583 refs, 35 files)
V[10:51:24.314] Build dynamic index for header symbols with estimated memory usage of 2164258 bytes
V[10:51:24.316] Built preamble of size 428684 for file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp version 1
I[10:51:24.320] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp (602 symbols, 3499 refs, 37 files)
I[10:51:24.323] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp (613 symbols, 3659 refs, 35 files)
I[10:51:24.350] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp (600 symbols, 3544 refs, 35 files)
V[10:51:24.375] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp version 1:
  symbol slab: 20 symbols, 8864 bytes
  ref slab: 29 symbols, 91 refs, 5240 bytes
  relations slab: 0 relations, 24 bytes
V[10:51:24.375] Build dynamic index for main-file symbols with estimated memory usage of 24216 bytes
I[10:51:24.375] --> textDocument/publishDiagnostics
V[10:51:24.375] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp","version":1}}

V[10:51:24.375] ASTWorker running EnumerateTweaks on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:51:24.375] --> reply:textDocument/codeAction("2") 310 ms
V[10:51:24.375] >>> {"id":"2","jsonrpc":"2.0","result":[]}

V[10:51:24.376] <<< {"id":"3","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:51:24.376] <-- textDocument/documentSymbol("3")
V[10:51:24.376] ASTWorker running DocumentSymbols on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:51:24.377] --> reply:textDocument/documentSymbol("3") 0 ms
V[10:51:24.377] >>> {"id":"3","jsonrpc":"2.0","result":[{"detail":"const int","kind":13,"name":"Forward","range":{"end":{"character":28,"line":11},"start":{"character":0,"line":11}},"selectionRange":{"end":{"character":17,"line":11},"start":{"character":10,"line":11}}},{"detail":"const int","kind":13,"name":"Backward","range":{"end":{"character":29,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":18,"line":12},"start":{"character":10,"line":12}}},{"detail":"const int","kind":13,"name":"Turn_Left","range":{"end":{"character":29,"line":13},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":19,"line":13},"start":{"character":10,"line":13}}},{"detail":"const int","kind":13,"name":"Turn_Right","range":{"end":{"character":29,"line":14},"start":{"character":0,"line":14}},"selectionRange":{"end":{"character":20,"line":14},"start":{"character":10,"line":14}}},{"detail":"const int","kind":13,"name":"Top_Left","range":{"end":{"character":28,"line":15},"start":{"character":0,"line":15}},"selectionRange":{"end":{"character":18,"line":15},"start":{"character":10,"line":15}}},{"detail":"const int","kind":13,"name":"Bottom_Left","range":{"end":{"character":29,"line":16},"start":{"character":0,"line":16}},"selectionRange":{"end":{"character":21,"line":16},"start":{"character":10,"line":16}}},{"detail":"const int","kind":13,"name":"Top_Right","range":{"end":{"character":28,"line":17},"start":{"character":0,"line":17}},"selectionRange":{"end":{"character":19,"line":17},"start":{"character":10,"line":17}}},{"detail":"const int","kind":13,"name":"Bottom_Right","range":{"end":{"character":28,"line":18},"start":{"character":0,"line":18}},"selectionRange":{"end":{"character":22,"line":18},"start":{"character":10,"line":18}}},{"detail":"const int","kind":13,"name":"Stop","range":{"end":{"character":27,"line":19},"start":{"character":0,"line":19}},"selectionRange":{"end":{"character":14,"line":19},"start":{"character":10,"line":19}}},{"detail":"const int","kind":13,"name":"Contrarotate","range":{"end":{"character":29,"line":20},"start":{"character":0,"line":20}},"selectionRange":{"end":{"character":22,"line":20},"start":{"character":10,"line":20}}},{"detail":"const int","kind":13,"name":"Clockwise","range":{"end":{"character":28,"line":21},"start":{"character":0,"line":21}},"selectionRange":{"end":{"character":19,"line":21},"start":{"character":10,"line":21}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":24},"start":{"character":0,"line":24}},"selectionRange":{"end":{"character":10,"line":24},"start":{"character":5,"line":24}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":26},"start":{"character":0,"line":26}},"selectionRange":{"end":{"character":9,"line":26},"start":{"character":5,"line":26}}},{"detail":"void (int, int)","kind":12,"name":"Motor","range":{"end":{"character":30,"line":28},"start":{"character":0,"line":28}},"selectionRange":{"end":{"character":10,"line":28},"start":{"character":5,"line":28}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":1,"line":38},"start":{"character":0,"line":30}},"selectionRange":{"end":{"character":10,"line":30},"start":{"character":5,"line":30}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":75},"start":{"character":0,"line":40}},"selectionRange":{"end":{"character":9,"line":40},"start":{"character":5,"line":40}}},{"detail":"void (int, int)","kind":12,"name":"Motor","range":{"end":{"character":1,"line":86},"start":{"character":0,"line":77}},"selectionRange":{"end":{"character":10,"line":77},"start":{"character":5,"line":77}}}]}

V[10:51:24.432] <<< {"id":"4","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":40,"line":6},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:51:24.432] <-- textDocument/hover("4")
V[10:51:24.432] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:51:24.435] --> reply:textDocument/hover("4") 3 ms
V[10:51:24.435] >>> {"id":"4","jsonrpc":"2.0","result":null}

I[10:51:25.028] --> $/progress
V[10:51:25.028] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"2/27","percentage":7}}}

I[10:51:25.028] --> $/progress
V[10:51:25.028] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"2/27","percentage":7}}}

V[10:51:25.030] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp (digest:=293923F15565174B)
I[10:51:25.113] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp (125 symbols, 2188 refs, 18 files)
I[10:51:25.164] --> $/progress
V[10:51:25.165] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"3/27","percentage":11}}}

I[10:51:25.165] --> $/progress
V[10:51:25.165] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"3/27","percentage":11}}}

V[10:51:25.168] Indexing C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp (digest:=4123CC6579BB460A)
I[10:51:25.170] --> $/progress
V[10:51:25.170] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"4/27","percentage":14}}}

I[10:51:25.170] --> $/progress
V[10:51:25.170] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"4/27","percentage":14}}}

V[10:51:25.175] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp (digest:=313C4893EB7ADBE6)
I[10:51:25.187] --> $/progress
V[10:51:25.187] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"5/27","percentage":18}}}

I[10:51:25.187] --> $/progress
V[10:51:25.187] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"5/27","percentage":18}}}

V[10:51:25.191] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c (digest:=B0774BE9D28D49CB)
V[10:51:25.198] BackgroundIndex: building version 1 after indexing enough files
I[10:51:25.199] --> $/progress
V[10:51:25.199] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"6/27","percentage":22}}}

I[10:51:25.199] --> $/progress
V[10:51:25.199] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"6/27","percentage":22}}}

V[10:51:25.201] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp (digest:=38075D39C713EC91)
I[10:51:25.206] --> $/progress
V[10:51:25.206] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"7/27","percentage":25}}}

I[10:51:25.206] --> $/progress
V[10:51:25.206] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"7/27","percentage":25}}}

V[10:51:25.210] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp (digest:=7D1D0E442CF15FC1)
V[10:51:25.212] BackgroundIndex: serving version 1 (1497454 bytes)
I[10:51:25.213] --> $/progress
V[10:51:25.213] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"8/27","percentage":29}}}

I[10:51:25.213] --> $/progress
V[10:51:25.213] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"8/27","percentage":29}}}

V[10:51:25.216] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp (digest:=E3E9F11672EDD20A)
I[10:51:25.244] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp (46 symbols, 139 refs, 3 files)
I[10:51:25.248] --> $/progress
V[10:51:25.249] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"9/27","percentage":33}}}

I[10:51:25.249] --> $/progress
V[10:51:25.249] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"9/27","percentage":33}}}

V[10:51:25.251] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp (digest:=4A1244E54C0CAC04)
I[10:51:25.256] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c (2 symbols, 2141 refs, 25 files)
I[10:51:25.256] Indexed C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp (14 symbols, 2286 refs, 35 files)
I[10:51:25.263] --> $/progress
V[10:51:25.263] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"10/27","percentage":37}}}

I[10:51:25.263] --> $/progress
V[10:51:25.263] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"10/27","percentage":37}}}

I[10:51:25.264] --> $/progress
V[10:51:25.264] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"11/27","percentage":40}}}

I[10:51:25.264] --> $/progress
V[10:51:25.264] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"11/27","percentage":40}}}

I[10:51:25.265] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp (4 symbols, 2226 refs, 35 files)
V[10:51:25.266] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c (digest:=C16B0ED8B1C5BB9F)
I[10:51:25.272] --> $/progress
V[10:51:25.272] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"12/27","percentage":44}}}

I[10:51:25.272] --> $/progress
V[10:51:25.272] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"12/27","percentage":44}}}

V[10:51:25.275] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp (digest:=3DD4F70FCF8C4FA6)
I[10:51:25.292] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp (2 symbols, 83 refs, 3 files)
V[10:51:25.296] Ignored diagnostic. c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include\avr/wdt.h:464:12:value '64' out of range for constraint 'I'
V[10:51:25.296] Ignored diagnostic. c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include\avr/wdt.h:507:23:value '64' out of range for constraint 'I'
I[10:51:25.297] --> $/progress
V[10:51:25.297] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"13/27","percentage":48}}}

I[10:51:25.297] --> $/progress
V[10:51:25.297] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"13/27","percentage":48}}}

I[10:51:25.300] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c (1 symbols, 1 refs, 1 files)
V[10:51:25.300] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c (digest:=5D6C1534064234DD)
I[10:51:25.301] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp (12 symbols, 2468 refs, 38 files)
I[10:51:25.304] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp (2 symbols, 2307 refs, 37 files)
I[10:51:25.304] Failed to compile C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp, index may be incomplete
I[10:51:25.305] --> $/progress
V[10:51:25.305] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"14/27","percentage":51}}}

I[10:51:25.305] --> $/progress
V[10:51:25.305] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"14/27","percentage":51}}}

V[10:51:25.309] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c (digest:=343A7ACAD5FD2414)
I[10:51:25.317] --> $/progress
V[10:51:25.317] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"15/27","percentage":55}}}

I[10:51:25.317] --> $/progress
V[10:51:25.317] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"15/27","percentage":55}}}

V[10:51:25.320] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp (digest:=55BA50D4FF04E609)
I[10:51:25.325] --> $/progress
V[10:51:25.325] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"16/27","percentage":59}}}

I[10:51:25.325] --> $/progress
V[10:51:25.325] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"16/27","percentage":59}}}

V[10:51:25.327] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp (digest:=6DDB6ED4F4E34E63)
V[10:51:25.335] System include extraction: target extracted: "avr"
V[10:51:25.335] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:51:25.335] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:51:25.335] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:51:25.335] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-gcc.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:51:25.337] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S (digest:=87583F1C920AA889)
I[10:51:25.360] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp (0 symbols, 2251 refs, 37 files)
I[10:51:25.366] --> $/progress
V[10:51:25.366] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"17/27","percentage":62}}}

I[10:51:25.366] --> $/progress
V[10:51:25.366] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"17/27","percentage":62}}}

I[10:51:25.367] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c (8 symbols, 2247 refs, 25 files)
V[10:51:25.369] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp (digest:=F68AA83B5BAAD75D)
I[10:51:25.374] --> $/progress
V[10:51:25.374] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"18/27","percentage":66}}}

I[10:51:25.374] --> $/progress
V[10:51:25.374] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"18/27","percentage":66}}}

V[10:51:25.374] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:54:1:expected identifier or '('
V[10:51:25.374] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:62:23:expected identifier or '('
V[10:51:25.375] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:63:23:expected identifier or '('
V[10:51:25.375] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:64:23:expected identifier or '('
V[10:51:25.375] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:65:23:expected identifier or '('
V[10:51:25.375] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:66:23:expected identifier or '('
V[10:51:25.375] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:67:23:expected identifier or '('
V[10:51:25.375] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:72:37:expected identifier or '('
V[10:51:25.375] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:73:31:expected ';' after top level declarator
V[10:51:25.375] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:79:23:expected identifier or '('
V[10:51:25.375] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:83:32:expected identifier or '('
V[10:51:25.375] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:83:35:expected identifier or '('
V[10:51:25.375] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:84:22:unknown type name 'maxloops'
V[10:51:25.375] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:85:8:expected ';' after top level declarator
V[10:51:25.376] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:85:22:unknown type name 'maxloops'
V[10:51:25.376] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:86:8:expected ';' after top level declarator
V[10:51:25.376] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:86:22:unknown type name 'maxloops'
V[10:51:25.376] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:87:9:expected ';' after top level declarator
V[10:51:25.376] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:87:18:expected identifier or '('
V[10:51:25.376] Ignored diagnostic. too many errors emitted, stopping now
V[10:51:25.377] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp (digest:=365287FBD658A80E)
I[10:51:25.378] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c (4 symbols, 2340 refs, 25 files)
I[10:51:25.379] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S (12 symbols, 937 refs, 9 files)
I[10:51:25.379] Failed to compile C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S, index may be incomplete
I[10:51:25.384] --> $/progress
V[10:51:25.384] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"19/27","percentage":70}}}

I[10:51:25.384] --> $/progress
V[10:51:25.384] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"19/27","percentage":70}}}

I[10:51:25.384] --> $/progress
V[10:51:25.384] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"20/27","percentage":74}}}

I[10:51:25.384] --> $/progress
V[10:51:25.384] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"20/27","percentage":74}}}

V[10:51:25.386] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c (digest:=BC32CF542FD8D605)
V[10:51:25.386] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp (digest:=D7FFC6931C21680C)
I[10:51:25.398] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp (0 symbols, 2222 refs, 36 files)
I[10:51:25.404] --> $/progress
V[10:51:25.405] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"21/27","percentage":77}}}

I[10:51:25.405] --> $/progress
V[10:51:25.405] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"21/27","percentage":77}}}

V[10:51:25.412] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c (digest:=5E8D23E876F6F446)
I[10:51:25.414] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp (20 symbols, 2357 refs, 36 files)
I[10:51:25.420] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp (21 symbols, 150 refs, 5 files)
I[10:51:25.428] --> $/progress
V[10:51:25.428] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"22/27","percentage":81}}}

I[10:51:25.436] --> $/progress
V[10:51:25.436] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"23/27","percentage":85}}}

I[10:51:25.451] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c (4 symbols, 2201 refs, 25 files)
I[10:51:25.455] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp (2 symbols, 2280 refs, 37 files)
I[10:51:25.456] --> $/progress
V[10:51:25.456] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"24/27","percentage":88}}}

I[10:51:25.461] --> $/progress
V[10:51:25.461] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"25/27","percentage":92}}}

I[10:51:25.462] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp (0 symbols, 2251 refs, 37 files)
I[10:51:25.467] --> $/progress
V[10:51:25.467] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"26/27","percentage":96}}}

I[10:51:25.471] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c (2 symbols, 2115 refs, 25 files)
V[10:51:25.477] BackgroundIndex: building version 2 when background indexer is idle
V[10:51:25.488] BackgroundIndex: serving version 2 (1776046 bytes)
I[10:51:25.488] --> $/progress
V[10:51:25.488] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[10:51:27.445] <<< {"id":"5","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":29,"line":8},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:51:27.445] <-- textDocument/hover("5")
V[10:51:27.446] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:51:27.449] --> reply:textDocument/hover("5") 3 ms
V[10:51:27.449] >>> {"id":"5","jsonrpc":"2.0","result":null}

V[10:51:27.650] <<< {"id":"6","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":30,"line":8},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:51:27.650] <-- textDocument/hover("6")
V[10:51:27.650] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:51:27.653] --> reply:textDocument/hover("6") 3 ms
V[10:51:27.654] >>> {"id":"6","jsonrpc":"2.0","result":null}

V[10:51:27.882] <<< {"id":"7","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":30,"line":7},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:51:27.882] <-- textDocument/hover("7")
V[10:51:27.882] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:51:27.885] --> reply:textDocument/hover("7") 3 ms
V[10:51:27.885] >>> {"id":"7","jsonrpc":"2.0","result":null}

V[10:51:44.714] <<< {"id":"8","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":30,"line":7},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:51:44.714] <-- textDocument/hover("8")
V[10:51:44.717] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:51:44.720] --> reply:textDocument/hover("8") 6 ms
V[10:51:44.720] >>> {"id":"8","jsonrpc":"2.0","result":null}

V[10:51:45.314] <<< {"id":"9","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":27,"line":7},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:51:45.314] <-- textDocument/hover("9")
V[10:51:45.314] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:51:45.317] --> reply:textDocument/hover("9") 3 ms
V[10:51:45.317] >>> {"id":"9","jsonrpc":"2.0","result":null}

V[10:51:48.535] <<< {"id":"10","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":16,"line":11},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:51:48.535] <-- textDocument/hover("10")
V[10:51:48.535] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:51:48.539] --> reply:textDocument/hover("10") 3 ms
V[10:51:48.539] >>> {"id":"10","jsonrpc":"2.0","result":{"contents":{"kind":"markdown","value":"### variable `Forward`  \n\n---\nType: `const int`  \nValue = `92 (0x5c)`  \n前进  \n\n---\n```cpp\nconst int Forward = 92\n```"},"range":{"end":{"character":17,"line":11},"start":{"character":10,"line":11}}}}

V[10:51:48.875] <<< {"id":"11","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":59,"line":15},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:51:48.875] <-- textDocument/hover("11")
V[10:51:48.875] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:51:48.879] --> reply:textDocument/hover("11") 3 ms
V[10:51:48.879] >>> {"id":"11","jsonrpc":"2.0","result":null}

V[10:51:49.182] <<< {"id":"12","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":60,"line":16},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:51:49.182] <-- textDocument/hover("12")
V[10:51:49.182] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:51:49.185] --> reply:textDocument/hover("12") 3 ms
V[10:51:49.185] >>> {"id":"12","jsonrpc":"2.0","result":null}

V[10:51:51.960] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:51:51.960] <-- textDocument/didSave
I[10:51:51.960] File version went from 1 to 1
V[10:51:51.960] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\n// PWM 控制引脚\n#define PWM1_PIN            5\n#define PWM2_PIN            6      \n// 74HCT595N 芯片引脚\n#define SHCP_PIN            2                               // 位移时钟\n#define EN_PIN              7                               // 使能控制\n#define DATA_PIN            8                               // 串行数据\n#define STCP_PIN            4                               // 存储寄存器时钟          \n\nconst int Forward       = 92;                               // 前进\nconst int Backward      = 163;                              // 后退\nconst int Turn_Left     = 149;                              // 左平移\nconst int Turn_Right    = 106;                              // 右平移\nconst int Top_Left      = 20;                               // 左上移动\nconst int Bottom_Left   = 129;                              // 左下移动\nconst int Top_Right     = 72;                               // 右上移动\nconst int Bottom_Right  = 34;                               // 右下移动\nconst int Stop          = 0;                                // 停止\nconst int Contrarotate  = 172;                              // 逆时针旋转\nconst int Clockwise     = 83;                               // 顺时针旋转\n\n#line 22 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid setup();\n#line 32 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid loop();\n#line 69 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid Motor(int Dir, int Speed);\n#line 22 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid setup()\n{\n    pinMode(SHCP_PIN, OUTPUT);\n    pinMode(EN_PIN, OUTPUT);\n    pinMode(DATA_PIN, OUTPUT);\n    pinMode(STCP_PIN, OUTPUT);\n    pinMode(PWM1_PIN, OUTPUT);\n    pinMode(PWM2_PIN, OUTPUT);\n}\n\nvoid loop()\n{\n    /* 向前 */\n    Motor(Forward, 250);     \n    delay(2000);\n    /* 向后 */\n    Motor(Backward, 250);\n    delay(2000);\n    /* 左平移 */\n    Motor(Turn_Left, 250);\n    delay(2000);\n    /* 右平移 */\n    Motor(Turn_Right, 250);\n    delay(2000);\n    /* 左上移 */\n    Motor(Top_Left, 250);\n    delay(2000);\n    /* 右下移 */\n    Motor(Bottom_Right, 250);\n    delay(2000);\n    /* 左下移 */\n    Motor(Bottom_Left, 250);\n    delay(2000);\n    /* 右上移 */\n    Motor(Top_Right, 250);\n    delay(2000);\n    /* 原地顺时针转 */\n    Motor(Clockwise, 250);\n    delay(2000);\n    /* 原地逆时针转 */\n    Motor(Contrarotate, 250);\n    delay(2000);\n    /* 停止 */\n    Motor(Stop, 250);\n    delay(2000);\n}\n\nvoid Motor(int Dir, int Speed)\n{\n    digitalWrite(EN_PIN, LOW);\n    analogWrite(PWM1_PIN, Speed);\n    analogWrite(PWM2_PIN, Speed);\n\n    digitalWrite(STCP_PIN, LOW);\n    shiftOut(DATA_PIN, SHCP_PIN, MSBFIRST, Dir);\n    digitalWrite(STCP_PIN, HIGH);\n}\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp","version":2}}}

I[10:51:51.960] <-- textDocument/didChange
V[10:51:51.960] ASTWorker skipping Update (1) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:51:52.035] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\compile_commands.json
V[10:51:52.035] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533
I[10:51:52.035] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp version 2 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch\\1_Auto_move.ino.cpp"
I[10:51:52.038] --> window/workDoneProgress/create(1)
V[10:51:52.038] >>> {"id":1,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[10:51:52.038] Enqueueing 26 commands for indexing
V[10:51:52.038] <<< {"id":1,"jsonrpc":"2.0","result":null}

I[10:51:52.038] <-- reply(1)
I[10:51:52.038] --> $/progress
V[10:51:52.038] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[10:51:52.038] --> $/progress
V[10:51:52.039] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[10:51:52.060] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 1_Auto_move.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch\\1_Auto_move.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch\\1_Auto_move.ino.cpp"
V[10:51:52.063] BackgroundIndex: building version 3 after loading index from disk
V[10:51:52.068] Reusing preamble version 1 for version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
V[10:51:52.074] BackgroundIndex: serving version 3 (1776046 bytes)
I[10:51:52.087] --> $/progress
V[10:51:52.087] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[10:51:52.087] --> $/progress
V[10:51:52.087] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[10:51:59.706] <<< {"id":"13","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":53,"line":20},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:51:59.706] <-- textDocument/hover("13")
V[10:51:59.710] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:51:59.713] --> reply:textDocument/hover("13") 7 ms
V[10:51:59.713] >>> {"id":"13","jsonrpc":"2.0","result":null}

V[10:52:03.151] <<< {"id":"14","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":52,"line":20},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:52:03.151] <-- textDocument/hover("14")
V[10:52:03.151] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:52:03.154] --> reply:textDocument/hover("14") 3 ms
V[10:52:03.154] >>> {"id":"14","jsonrpc":"2.0","result":null}

V[10:52:03.364] <<< {"id":"15","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":53,"line":20},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:52:03.364] <-- textDocument/hover("15")
V[10:52:03.364] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:52:03.367] --> reply:textDocument/hover("15") 3 ms
V[10:52:03.367] >>> {"id":"15","jsonrpc":"2.0","result":null}

V[10:52:11.464] <<< {"id":"16","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":34,"line":21},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:52:11.464] <-- textDocument/hover("16")
V[10:52:11.467] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:52:11.471] --> reply:textDocument/hover("16") 6 ms
V[10:52:11.471] >>> {"id":"16","jsonrpc":"2.0","result":null}

V[10:52:11.784] <<< {"id":"17","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":35,"line":20},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:52:11.784] <-- textDocument/hover("17")
V[10:52:11.784] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:52:11.787] --> reply:textDocument/hover("17") 3 ms
V[10:52:11.787] >>> {"id":"17","jsonrpc":"2.0","result":null}

V[10:52:12.133] <<< {"id":"18","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":39,"line":20},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:52:12.133] <-- textDocument/hover("18")
V[10:52:12.134] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:52:12.137] --> reply:textDocument/hover("18") 3 ms
V[10:52:12.137] >>> {"id":"18","jsonrpc":"2.0","result":null}

V[10:52:12.427] <<< {"id":"19","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":38,"line":20},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:52:12.428] <-- textDocument/hover("19")
V[10:52:12.428] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:52:12.431] --> reply:textDocument/hover("19") 3 ms
V[10:52:12.431] >>> {"id":"19","jsonrpc":"2.0","result":null}

V[10:52:12.644] <<< {"id":"20","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":38,"line":19},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:52:12.644] <-- textDocument/hover("20")
V[10:52:12.644] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:52:12.647] --> reply:textDocument/hover("20") 3 ms
V[10:52:12.647] >>> {"id":"20","jsonrpc":"2.0","result":null}

V[10:52:14.247] <<< {"id":"21","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":38,"line":19},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:52:14.247] <-- textDocument/hover("21")
V[10:52:14.247] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:52:14.251] --> reply:textDocument/hover("21") 3 ms
V[10:52:14.251] >>> {"id":"21","jsonrpc":"2.0","result":null}

V[10:52:16.214] <<< {"id":"22","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":50,"line":19},"start":{"character":49,"line":18}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:52:16.214] <-- textDocument/codeAction("22")
V[10:52:16.214] ASTWorker running EnumerateTweaks on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:52:16.214] --> reply:textDocument/codeAction("22") 0 ms
V[10:52:16.214] >>> {"id":"22","jsonrpc":"2.0","result":[]}

V[10:52:17.390] <<< {"id":"23","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":50,"line":15},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:52:17.390] <-- textDocument/hover("23")
V[10:52:17.394] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:52:17.397] --> reply:textDocument/hover("23") 6 ms
V[10:52:17.397] >>> {"id":"23","jsonrpc":"2.0","result":null}

V[10:52:17.658] <<< {"id":"24","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":49,"line":15},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:52:17.658] <-- textDocument/hover("24")
V[10:52:17.658] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:52:17.661] --> reply:textDocument/hover("24") 3 ms
V[10:52:17.661] >>> {"id":"24","jsonrpc":"2.0","result":null}

V[10:52:17.884] <<< {"id":"25","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":48,"line":16},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:52:17.884] <-- textDocument/hover("25")
V[10:52:17.884] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:52:17.887] --> reply:textDocument/hover("25") 3 ms
V[10:52:17.887] >>> {"id":"25","jsonrpc":"2.0","result":null}

V[10:52:18.334] <<< {"id":"26","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":47,"line":15},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:52:18.334] <-- textDocument/hover("26")
V[10:52:18.335] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:52:18.338] --> reply:textDocument/hover("26") 3 ms
V[10:52:18.338] >>> {"id":"26","jsonrpc":"2.0","result":null}

V[10:52:19.466] <<< {"id":"27","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":43,"line":7},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:52:19.466] <-- textDocument/hover("27")
V[10:52:19.466] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:52:19.469] --> reply:textDocument/hover("27") 3 ms
V[10:52:19.470] >>> {"id":"27","jsonrpc":"2.0","result":null}

V[10:52:19.664] <<< {"id":"28","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":42,"line":7},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:52:19.664] <-- textDocument/hover("28")
V[10:52:19.664] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:52:19.667] --> reply:textDocument/hover("28") 3 ms
V[10:52:19.667] >>> {"id":"28","jsonrpc":"2.0","result":null}

V[10:53:47.710] <<< {"id":"29","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":36,"line":9},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:53:47.710] <-- textDocument/hover("29")
V[10:53:47.714] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:53:47.717] --> reply:textDocument/hover("29") 6 ms
V[10:53:47.717] >>> {"id":"29","jsonrpc":"2.0","result":null}

V[10:53:52.392] <<< {"id":"30","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":27,"line":14},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:53:52.392] <-- textDocument/hover("30")
V[10:53:52.392] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:53:52.395] --> reply:textDocument/hover("30") 3 ms
V[10:53:52.395] >>> {"id":"30","jsonrpc":"2.0","result":null}

V[10:53:52.816] <<< {"id":"31","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":27,"line":13},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:53:52.816] <-- textDocument/hover("31")
V[10:53:52.820] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:53:52.823] --> reply:textDocument/hover("31") 6 ms
V[10:53:52.823] >>> {"id":"31","jsonrpc":"2.0","result":null}

V[10:53:53.447] <<< {"id":"32","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":23,"line":12},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:53:53.447] <-- textDocument/hover("32")
V[10:53:53.447] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:53:53.451] --> reply:textDocument/hover("32") 3 ms
V[10:53:53.451] >>> {"id":"32","jsonrpc":"2.0","result":null}

V[10:53:58.803] <<< {"id":"33","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":38,"line":13},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:53:58.803] <-- textDocument/hover("33")
V[10:53:58.807] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:53:58.811] --> reply:textDocument/hover("33") 7 ms
V[10:53:58.811] >>> {"id":"33","jsonrpc":"2.0","result":null}

V[10:53:59.011] <<< {"id":"34","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":37,"line":12},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:53:59.011] <-- textDocument/hover("34")
V[10:53:59.012] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:53:59.015] --> reply:textDocument/hover("34") 3 ms
V[10:53:59.015] >>> {"id":"34","jsonrpc":"2.0","result":null}

V[10:54:00.183] <<< {"id":"35","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":35,"line":13},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:54:00.183] <-- textDocument/hover("35")
V[10:54:00.183] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:54:00.186] --> reply:textDocument/hover("35") 3 ms
V[10:54:00.186] >>> {"id":"35","jsonrpc":"2.0","result":null}

V[10:54:00.684] <<< {"id":"36","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":35,"line":14},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:54:00.684] <-- textDocument/hover("36")
V[10:54:00.684] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:54:00.687] --> reply:textDocument/hover("36") 3 ms
V[10:54:00.687] >>> {"id":"36","jsonrpc":"2.0","result":null}

V[10:54:01.097] <<< {"id":"37","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":33,"line":15},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:54:01.097] <-- textDocument/hover("37")
V[10:54:01.097] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:54:01.100] --> reply:textDocument/hover("37") 3 ms
V[10:54:01.100] >>> {"id":"37","jsonrpc":"2.0","result":null}

V[10:54:01.494] <<< {"id":"38","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":33,"line":16},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:54:01.494] <-- textDocument/hover("38")
V[10:54:01.494] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:54:01.497] --> reply:textDocument/hover("38") 3 ms
V[10:54:01.497] >>> {"id":"38","jsonrpc":"2.0","result":null}

V[10:55:00.134] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:55:00.134] <-- textDocument/didSave
I[10:55:00.134] File version went from 2 to 2
V[10:55:00.134] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\n// PWM 控制引脚\n#define PWM1_PIN            5\n#define PWM2_PIN            6      \n// 74HCT595N 芯片引脚\n#define SHCP_PIN            2                               // 位移时钟\n#define EN_PIN              7                               // 使能控制\n#define DATA_PIN            8                               // 串行数据\n#define STCP_PIN            4                               // 存储寄存器时钟          \n\nconst int Forward       = 92;                               // 前进\nconst int Backward      = 163;                              // 后退\nconst int Turn_Left     = 149;                              // 左平移\nconst int Turn_Right    = 106;                              // 右平移\nconst int Top_Left      = 20;                               // 左上移动\nconst int Bottom_Left   = 129;                              // 左下移动\nconst int Top_Right     = 72;                               // 右上移动\nconst int Bottom_Right  = 34;                               // 右下移动\nconst int Stop          = 0;                                // 停止\nconst int Contrarotate  = 172;                              // 逆时针旋转\nconst int Clockwise     = 83;                               // 顺时针旋转\n\n#line 22 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid setup();\n#line 32 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid loop();\n#line 69 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid Motor(int Dir, int Speed);\n#line 22 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid setup()\n{\n    pinMode(SHCP_PIN, OUTPUT);\n    pinMode(EN_PIN, OUTPUT);\n    pinMode(DATA_PIN, OUTPUT);\n    pinMode(STCP_PIN, OUTPUT);\n    pinMode(PWM1_PIN, OUTPUT);\n    pinMode(PWM2_PIN, OUTPUT);\n}\n\nvoid loop()\n{\n    /* 向前 */\n    Motor(Forward, 250);     \n    delay(2000);\n    /* 向后 */\n    Motor(Backward, 250);\n    delay(2000);\n    /* 左平移 */\n    Motor(Turn_Left, 250);\n    delay(2000);\n    /* 右平移 */\n    Motor(Turn_Right, 250);\n    delay(2000);\n    /* 左上移 */\n    Motor(Top_Left, 250);\n    delay(2000);\n    /* 右下移 */\n    Motor(Bottom_Right, 250);\n    delay(2000);\n    /* 左下移 */\n    Motor(Bottom_Left, 250);\n    delay(2000);\n    /* 右上移 */\n    Motor(Top_Right, 250);\n    delay(2000);\n    /* 原地顺时针转 */\n    Motor(Clockwise, 250);\n    delay(2000);\n    /* 原地逆时针转 */\n    Motor(Contrarotate, 250);\n    delay(2000);\n    /* 停止 */\n    Motor(Stop, 250);\n    delay(2000);\n}\n\nvoid Motor(int Dir, int Speed)\n{\n    digitalWrite(EN_PIN, LOW);\n    analogWrite(PWM1_PIN, Speed);\n    analogWrite(PWM2_PIN, Speed);\n\n    digitalWrite(STCP_PIN, LOW);\n    shiftOut(DATA_PIN, SHCP_PIN, MSBFIRST, Dir);\n    digitalWrite(STCP_PIN, HIGH);\n}\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp","version":3}}}

I[10:55:00.134] <-- textDocument/didChange
V[10:55:00.134] ASTWorker skipping Update (2) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:55:00.209] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\compile_commands.json
V[10:55:00.209] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533
I[10:55:00.209] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp version 3 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch\\1_Auto_move.ino.cpp"
I[10:55:00.214] --> window/workDoneProgress/create(2)
V[10:55:00.214] >>> {"id":2,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[10:55:00.214] Enqueueing 26 commands for indexing
V[10:55:00.214] <<< {"id":2,"jsonrpc":"2.0","result":null}

I[10:55:00.214] <-- reply(2)
I[10:55:00.214] --> $/progress
V[10:55:00.214] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[10:55:00.214] --> $/progress
V[10:55:00.214] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[10:55:00.238] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 1_Auto_move.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch\\1_Auto_move.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1391305533\\sketch\\1_Auto_move.ino.cpp"
V[10:55:00.239] BackgroundIndex: building version 4 after loading index from disk
V[10:55:00.246] Reusing preamble version 1 for version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
V[10:55:00.251] BackgroundIndex: serving version 4 (1776046 bytes)
I[10:55:00.264] --> $/progress
V[10:55:00.264] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[10:55:00.264] --> $/progress
V[10:55:00.264] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[10:56:30.246] <<< {"id":"39","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":13,"line":54},"start":{"character":13,"line":54}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:56:30.246] <-- textDocument/codeAction("39")
V[10:56:30.249] ASTWorker running EnumerateTweaks on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:56:30.249] --> reply:textDocument/codeAction("39") 3 ms
V[10:56:30.249] >>> {"id":"39","jsonrpc":"2.0","result":[]}

V[10:56:31.135] <<< {"id":"40","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":25,"line":55},"start":{"character":25,"line":55}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:56:31.135] <-- textDocument/codeAction("40")
V[10:56:31.135] ASTWorker running EnumerateTweaks on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:56:31.135] --> reply:textDocument/codeAction("40") 0 ms
V[10:56:31.135] >>> {"id":"40","jsonrpc":"2.0","result":[]}

V[10:56:36.767] <<< {"id":"41","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":53,"line":21},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:56:36.767] <-- textDocument/hover("41")
V[10:56:36.770] ASTWorker running Hover on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:56:36.773] --> reply:textDocument/hover("41") 6 ms
V[10:56:36.773] >>> {"id":"41","jsonrpc":"2.0","result":null}

V[10:56:38.909] <<< {"id":"42","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":53,"line":19},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:56:38.909] <-- textDocument/hover("42")
V[10:56:38.909] ASTWorker running Hover on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:56:38.912] --> reply:textDocument/hover("42") 3 ms
V[10:56:38.912] >>> {"id":"42","jsonrpc":"2.0","result":null}

V[10:58:27.010] <<< {"id":"43","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":13,"line":63},"start":{"character":13,"line":63}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[10:58:27.010] <-- textDocument/codeAction("43")
V[10:58:27.013] ASTWorker running EnumerateTweaks on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[10:58:27.013] --> reply:textDocument/codeAction("43") 3 ms
V[10:58:27.013] >>> {"id":"43","jsonrpc":"2.0","result":[]}

V[13:33:05.225] <<< {"id":"44","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":16,"line":68},"start":{"character":16,"line":68}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[13:33:05.226] <-- textDocument/codeAction("44")
V[13:33:05.231] ASTWorker running EnumerateTweaks on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[13:33:05.232] --> reply:textDocument/codeAction("44") 6 ms
V[13:33:05.232] >>> {"id":"44","jsonrpc":"2.0","result":[]}

V[13:33:19.946] <<< {"id":"45","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":52,"line":20},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[13:33:19.946] <-- textDocument/hover("45")
V[13:33:19.950] ASTWorker running Hover on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[13:33:19.954] --> reply:textDocument/hover("45") 7 ms
V[13:33:19.954] >>> {"id":"45","jsonrpc":"2.0","result":null}

V[13:33:25.234] <<< {"id":"46","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":51,"line":20},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[13:33:25.234] <-- textDocument/hover("46")
V[13:33:25.237] ASTWorker running Hover on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[13:33:25.241] --> reply:textDocument/hover("46") 6 ms
V[13:33:25.241] >>> {"id":"46","jsonrpc":"2.0","result":null}

V[13:33:32.312] <<< {"id":"47","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":47,"line":15},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[13:33:32.312] <-- textDocument/hover("47")
V[13:33:32.316] ASTWorker running Hover on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[13:33:32.319] --> reply:textDocument/hover("47") 6 ms
V[13:33:32.319] >>> {"id":"47","jsonrpc":"2.0","result":null}

V[13:35:41.272] <<< {"id":"48","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":23,"line":9},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[13:35:41.272] <-- textDocument/hover("48")
V[13:35:41.276] ASTWorker running Hover on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[13:35:41.279] --> reply:textDocument/hover("48") 7 ms
V[13:35:41.279] >>> {"id":"48","jsonrpc":"2.0","result":null}

V[13:36:11.328] <<< {"id":"49","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":43,"line":11},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[13:36:11.328] <-- textDocument/hover("49")
V[13:36:11.331] ASTWorker running Hover on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[13:36:11.334] --> reply:textDocument/hover("49") 6 ms
V[13:36:11.334] >>> {"id":"49","jsonrpc":"2.0","result":null}

V[13:36:11.546] <<< {"id":"50","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":42,"line":11},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[13:36:11.546] <-- textDocument/hover("50")
V[13:36:11.546] ASTWorker running Hover on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[13:36:11.549] --> reply:textDocument/hover("50") 3 ms
V[13:36:11.549] >>> {"id":"50","jsonrpc":"2.0","result":null}

V[13:36:16.338] <<< {"id":"51","jsonrpc":"2.0","method":"textDocument/documentHighlight","params":{"position":{"character":66,"line":13},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[13:36:16.338] <-- textDocument/documentHighlight("51")
V[13:36:16.341] ASTWorker running Highlights on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[13:36:16.342] --> reply:textDocument/documentHighlight("51") 3 ms
V[13:36:16.342] >>> {"id":"51","jsonrpc":"2.0","result":[]}

V[13:36:16.576] <<< {"id":"52","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":66,"line":13},"start":{"character":66,"line":13}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1391305533/sketch/1_Auto_move.ino.cpp"}}}

I[13:36:16.576] <-- textDocument/codeAction("52")
V[13:36:16.576] ASTWorker running EnumerateTweaks on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1391305533\sketch\1_Auto_move.ino.cpp
I[13:36:16.576] --> reply:textDocument/codeAction("52") 0 ms
V[13:36:16.576] >>> {"id":"52","jsonrpc":"2.0","result":[]}

V[13:36:18.618] <<< {"id":"53","jsonrpc":"2.0","method":"shutdown","params":null}

I[13:36:18.618] <-- shutdown("53")
I[13:36:18.618] --> reply:shutdown("53") 0 ms
V[13:36:18.618] >>> {"id":"53","jsonrpc":"2.0","result":null}








Started logging.
I[13:38:58.803] clangd version 14.0.0
I[13:38:58.805] Features: windows
I[13:38:58.805] PID: 6908
I[13:38:58.805] Working directory: g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYC0076拍照麦克轮WiFi小车\ZYC0076\4_Arduino_Code\1_Auto_move
I[13:38:58.805] argv[0]: d:\Program Files\Arduino IDE\resources\app\node_modules\arduino-ide-extension\build\clangd.exe
I[13:38:58.805] argv[1]: -log=verbose
I[13:38:58.805] argv[2]: --compile-commands-dir=C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124
I[13:38:58.805] argv[3]: -query-driver=C:\Users\Administrator\AppData\Local\Arduino15\packages\**
V[13:38:58.814] User config file is C:\Users\Administrator\AppData\Local\clangd\config.yaml
I[13:38:58.814] Starting LSP over stdin/stdout
V[13:38:58.814] <<< {"id":"1","jsonrpc":"2.0","method":"initialize","params":{"capabilities":{"textDocument":{"codeAction":{"codeActionLiteralSupport":{"codeActionKind":{"valueSet":["","quickfix","refactor","refactor.extract","refactor.inline","refactor.rewrite","source","source.organizeImports"]}},"dynamicRegistration":true,"isPreferredSupport":true},"codeLens":{"dynamicRegistration":true},"colorProvider":{"dynamicRegistration":true},"completion":{"completionItem":{"commitCharactersSupport":true,"deprecatedSupport":true,"documentationFormat":["markdown","plaintext"],"preselectSupport":true,"snippetSupport":true,"tagSupport":{"valueSet":[1]}},"completionItemKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25]},"contextSupport":true,"dynamicRegistration":true},"declaration":{"dynamicRegistration":true,"linkSupport":true},"definition":{"dynamicRegistration":true,"linkSupport":true},"documentHighlight":{"dynamicRegistration":true},"documentLink":{"dynamicRegistration":true,"tooltipSupport":true},"documentSymbol":{"dynamicRegistration":true,"hierarchicalDocumentSymbolSupport":true,"symbolKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26]}},"foldingRange":{"dynamicRegistration":true,"lineFoldingOnly":true,"rangeLimit":5000},"formatting":{"dynamicRegistration":true},"hover":{"contentFormat":["markdown","plaintext"],"dynamicRegistration":true},"implementation":{"dynamicRegistration":true,"linkSupport":true},"onTypeFormatting":{"dynamicRegistration":true},"publishDiagnostics":{"relatedInformation":true,"tagSupport":{"valueSet":[1,2]}},"rangeFormatting":{"dynamicRegistration":true},"references":{"dynamicRegistration":true},"rename":{"dynamicRegistration":true,"prepareSupport":true},"selectionRange":{"dynamicRegistration":true},"signatureHelp":{"contextSupport":true,"dynamicRegistration":true,"signatureInformation":{"documentationFormat":["markdown","plaintext"],"parameterInformation":{"labelOffsetSupport":true}}},"synchronization":{"didSave":true,"dynamicRegistration":true,"willSave":true,"willSaveWaitUntil":true},"typeDefinition":{"dynamicRegistration":true,"linkSupport":true}},"window":{"workDoneProgress":true},"workspace":{"applyEdit":true,"configuration":true,"didChangeConfiguration":{"dynamicRegistration":true},"didChangeWatchedFiles":{"dynamicRegistration":true},"executeCommand":{"dynamicRegistration":true},"symbol":{"dynamicRegistration":true,"symbolKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26]}},"workspaceEdit":{"documentChanges":true,"failureHandling":"textOnlyTransactional","resourceOperations":["create","rename","delete"]},"workspaceFolders":true}},"clientInfo":{"name":"vscode","version":"1.53.2"},"initializationOptions":{},"processId":11856,"rootPath":"C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch","rootUri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch","trace":"off","workspaceFolders":[{"name":"1_Auto_move","uri":"file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYC0076%E6%8B%8D%E7%85%A7%E9%BA%A6%E5%85%8B%E8%BD%AEWiFi%E5%B0%8F%E8%BD%A6/ZYC0076/4_Arduino_Code/1_Auto_move"}]}}

I[13:38:58.815] <-- initialize("1")
I[13:38:58.872] --> reply:initialize("1") 57 ms
V[13:38:58.872] >>> {"id":"1","jsonrpc":"2.0","result":{"capabilities":{"astProvider":true,"callHierarchyProvider":true,"clangdInlayHintsProvider":true,"codeActionProvider":{"codeActionKinds":["quickfix","refactor","info"]},"compilationDatabase":{"automaticReload":true},"completionProvider":{"allCommitCharacters":[" ","\t","(",")","[","]","{","}","<",">",":",";",",","+","-","/","*","%","^","&","#","?",".","=","\"","'","|"],"resolveProvider":false,"triggerCharacters":[".","<",">",":","\"","/","*"]},"declarationProvider":true,"definitionProvider":true,"documentFormattingProvider":true,"documentHighlightProvider":true,"documentLinkProvider":{"resolveProvider":false},"documentOnTypeFormattingProvider":{"firstTriggerCharacter":"\n","moreTriggerCharacter":[]},"documentRangeFormattingProvider":true,"documentSymbolProvider":true,"executeCommandProvider":{"commands":["clangd.applyFix","clangd.applyTweak"]},"hoverProvider":true,"implementationProvider":true,"memoryUsageProvider":true,"referencesProvider":true,"renameProvider":{"prepareProvider":true},"selectionRangeProvider":true,"semanticTokensProvider":{"full":{"delta":true},"legend":{"tokenModifiers":["declaration","deprecated","deduced","readonly","static","abstract","virtual","dependentName","defaultLibrary","usedAsMutableReference","functionScope","classScope","fileScope","globalScope"],"tokenTypes":["variable","variable","parameter","function","method","function","property","variable","class","interface","enum","enumMember","type","type","unknown","namespace","typeParameter","concept","type","macro","comment"]},"range":false},"signatureHelpProvider":{"triggerCharacters":["(",")","{","}","<",">",","]},"textDocumentSync":{"change":2,"openClose":true,"save":true},"typeDefinitionProvider":true,"typeHierarchyProvider":true,"workspaceSymbolProvider":true},"serverInfo":{"name":"clangd","version":"clangd version 14.0.0 windows x86_64-pc-windows-msvc"}}}

V[13:38:58.873] <<< {"jsonrpc":"2.0","method":"initialized","params":{}}

I[13:38:58.873] <-- initialized
V[13:38:58.879] <<< {"jsonrpc":"2.0","method":"textDocument/didOpen","params":{"textDocument":{"languageId":"cpp","text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\n// PWM 控制引脚\n#define PWM1_PIN            5\n#define PWM2_PIN            6      \n// 74HCT595N 芯片引脚\n#define SHCP_PIN            2                               // 位移时钟\n#define EN_PIN              7                               // 使能控制\n#define DATA_PIN            8                               // 串行数据\n#define STCP_PIN            4                               // 存储寄存器时钟          \n\nconst int Forward       = 92;                               // 前进\nconst int Backward      = 163;                              // 后退\nconst int Turn_Left     = 149;                              // 左平移\nconst int Turn_Right    = 106;                              // 右平移\nconst int Top_Left      = 20;                               // 左上移动\nconst int Bottom_Left   = 129;                              // 左下移动\nconst int Top_Right     = 72;                               // 右上移动\nconst int Bottom_Right  = 34;                               // 右下移动\nconst int Stop          = 0;                                // 停止\nconst int Contrarotate  = 172;                              // 逆时针旋转\nconst int Clockwise     = 83;                               // 顺时针旋转\n\n#line 22 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid setup();\n#line 32 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid loop();\n#line 69 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid Motor(int Dir, int Speed);\n#line 22 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\nvoid setup()\n{\n    pinMode(SHCP_PIN, OUTPUT);\n    pinMode(EN_PIN, OUTPUT);\n    pinMode(DATA_PIN, OUTPUT);\n    pinMode(STCP_PIN, OUTPUT);\n    pinMode(PWM1_PIN, OUTPUT);\n    pinMode(PWM2_PIN, OUTPUT);\n}\n\nvoid loop()\n{\n    /* 向前 */\n    Motor(Forward, 250);     \n    delay(2000);\n    /* 向后 */\n    Motor(Backward, 250);\n    delay(2000);\n    /* 左平移 */\n    Motor(Turn_Left, 250);\n    delay(2000);\n    /* 右平移 */\n    Motor(Turn_Right, 250);\n    delay(2000);\n    /* 左上移 */\n    Motor(Top_Left, 250);\n    delay(2000);\n    /* 右下移 */\n    Motor(Bottom_Right, 250);\n    delay(2000);\n    /* 左下移 */\n    Motor(Bottom_Left, 250);\n    delay(2000);\n    /* 右上移 */\n    Motor(Top_Right, 250);\n    delay(2000);\n    /* 原地顺时针转 */\n    Motor(Clockwise, 250);\n    delay(2000);\n    /* 原地逆时针转 */\n    Motor(Contrarotate, 250);\n    delay(2000);\n    /* 停止 */\n    Motor(Stop, 250);\n    delay(2000);\n}\n\nvoid Motor(int Dir, int Speed)\n{\n    digitalWrite(EN_PIN, LOW);\n    analogWrite(PWM1_PIN, Speed);\n    analogWrite(PWM2_PIN, Speed);\n\n    digitalWrite(STCP_PIN, LOW);\n    shiftOut(DATA_PIN, SHCP_PIN, MSBFIRST, Dir);\n    digitalWrite(STCP_PIN, HIGH);\n}\n","uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":1}}}

I[13:38:58.879] <-- textDocument/didOpen
V[13:38:58.883] config note at C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\.clangd:1:0: Parsing config fragment
V[13:38:58.883] config note at C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\.clangd:1:0: Parsed 1 fragments from file
V[13:38:58.883] Config fragment: compiling C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\.clangd:1 -> 0x000001F2D1F1A620 (trusted=false)
I[13:38:58.884] --> textDocument/publishDiagnostics
V[13:38:58.884] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/.clangd"}}

V[13:38:58.884] <<< {"id":"2","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":66,"line":13},"start":{"character":66,"line":13}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:38:58.884] <-- textDocument/codeAction("2")
I[13:38:58.885] Loaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\compile_commands.json
V[13:38:58.885] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124
I[13:38:58.888] --> window/workDoneProgress/create(0)
V[13:38:58.888] >>> {"id":0,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[13:38:58.888] Enqueueing 26 commands for indexing
V[13:38:58.888] <<< {"id":0,"jsonrpc":"2.0","result":null}

I[13:38:58.888] <-- reply(0)
I[13:38:58.888] --> $/progress
V[13:38:58.888] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[13:38:58.888] --> $/progress
V[13:38:58.888] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[13:38:58.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp
V[13:38:58.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp
V[13:38:58.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c
V[13:38:58.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c
V[13:38:58.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp
V[13:38:58.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp
V[13:38:58.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp
V[13:38:58.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp
V[13:38:58.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp
V[13:38:58.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp
V[13:38:58.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S
V[13:38:58.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp
V[13:38:58.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp
V[13:38:58.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c
V[13:38:58.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp
V[13:38:58.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp
V[13:38:58.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp
V[13:38:58.891] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp
V[13:38:58.891] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c
V[13:38:58.891] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c
V[13:38:58.891] Failed to load shard: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
V[13:38:58.891] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp
V[13:38:58.891] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp
V[13:38:58.891] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c
V[13:38:58.891] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp
V[13:38:58.891] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c
I[13:38:58.897] --> $/progress
V[13:38:58.897] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[13:38:58.897] --> $/progress
V[13:38:58.897] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[13:38:58.897] --> $/progress
V[13:38:58.897] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[13:38:58.897] --> $/progress
V[13:38:58.897] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[13:38:58.897] --> $/progress
V[13:38:58.897] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[13:38:58.897] --> $/progress
V[13:38:58.897] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[13:38:58.897] --> $/progress
V[13:38:58.897] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[13:38:58.897] --> $/progress
V[13:38:58.897] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

V[13:38:59.008] System include extraction: target extracted: "avr"
V[13:38:59.008] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[13:38:59.008] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[13:38:59.008] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[13:38:59.008] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
I[13:38:59.009] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 1 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:38:59.040] System include extraction: target extracted: "avr"
V[13:38:59.040] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[13:38:59.040] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[13:38:59.040] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[13:38:59.040] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[13:38:59.054] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp (digest:=7D1D0E442CF15FC1)
V[13:38:59.055] System include extraction: target extracted: "avr"
V[13:38:59.055] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[13:38:59.055] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[13:38:59.055] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[13:38:59.055] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[13:38:59.057] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp (digest:=E3E9F11672EDD20A)
V[13:38:59.058] System include extraction: target extracted: "avr"
V[13:38:59.058] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[13:38:59.058] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[13:38:59.058] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[13:38:59.058] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[13:38:59.059] System include extraction: target extracted: "avr"
V[13:38:59.059] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[13:38:59.065] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[13:38:59.065] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[13:38:59.065] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-gcc.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[13:38:59.064] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp (digest:=1C31198B0754810E)
V[13:38:59.065] System include extraction: target extracted: "avr"
V[13:38:59.065] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[13:38:59.065] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[13:38:59.065] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[13:38:59.065] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[13:38:59.066] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 1_Auto_move.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:38:59.066] Building first preamble for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 1
V[13:38:59.069] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp (digest:=F7D59D2B49112307)
V[13:38:59.071] System include extraction: target extracted: "avr"
V[13:38:59.071] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[13:38:59.071] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[13:38:59.071] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[13:38:59.071] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[13:38:59.072] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c (digest:=5E8D23E876F6F446)
V[13:38:59.074] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp (digest:=55BA50D4FF04E609)
V[13:38:59.147] indexed preamble AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 1:
  symbol slab: 2505 symbols, 716894 bytes
  ref slab: 0 symbols, 0 refs, 136 bytes
  relations slab: 9 relations, 177 bytes
V[13:38:59.177] Build dynamic index for header symbols with estimated memory usage of 2164258 bytes
V[13:38:59.180] Built preamble of size 428684 for file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 1
I[13:38:59.183] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c (309 symbols, 2643 refs, 25 files)
V[13:38:59.198] Ignored diagnostic. c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include\avr/wdt.h:464:12:value '64' out of range for constraint 'I'
V[13:38:59.199] Ignored diagnostic. c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include\avr/wdt.h:507:23:value '64' out of range for constraint 'I'
I[13:38:59.212] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp (602 symbols, 3517 refs, 37 files)
I[13:38:59.212] Failed to compile C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp, index may be incomplete
I[13:38:59.220] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp (600 symbols, 3432 refs, 36 files)
I[13:38:59.227] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp (604 symbols, 3716 refs, 38 files)
I[13:38:59.227] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp (600 symbols, 3544 refs, 35 files)
V[13:38:59.239] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 1:
  symbol slab: 20 symbols, 8864 bytes
  ref slab: 29 symbols, 91 refs, 5240 bytes
  relations slab: 0 relations, 24 bytes
V[13:38:59.239] Build dynamic index for main-file symbols with estimated memory usage of 24216 bytes
I[13:38:59.239] --> textDocument/publishDiagnostics
V[13:38:59.239] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":1}}

V[13:38:59.240] ASTWorker running EnumerateTweaks on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:38:59.240] --> reply:textDocument/codeAction("2") 355 ms
V[13:38:59.240] >>> {"id":"2","jsonrpc":"2.0","result":[]}

V[13:38:59.241] <<< {"id":"3","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:38:59.241] <-- textDocument/documentSymbol("3")
V[13:38:59.241] ASTWorker running DocumentSymbols on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:38:59.242] --> reply:textDocument/documentSymbol("3") 0 ms
V[13:38:59.242] >>> {"id":"3","jsonrpc":"2.0","result":[{"detail":"const int","kind":13,"name":"Forward","range":{"end":{"character":28,"line":11},"start":{"character":0,"line":11}},"selectionRange":{"end":{"character":17,"line":11},"start":{"character":10,"line":11}}},{"detail":"const int","kind":13,"name":"Backward","range":{"end":{"character":29,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":18,"line":12},"start":{"character":10,"line":12}}},{"detail":"const int","kind":13,"name":"Turn_Left","range":{"end":{"character":29,"line":13},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":19,"line":13},"start":{"character":10,"line":13}}},{"detail":"const int","kind":13,"name":"Turn_Right","range":{"end":{"character":29,"line":14},"start":{"character":0,"line":14}},"selectionRange":{"end":{"character":20,"line":14},"start":{"character":10,"line":14}}},{"detail":"const int","kind":13,"name":"Top_Left","range":{"end":{"character":28,"line":15},"start":{"character":0,"line":15}},"selectionRange":{"end":{"character":18,"line":15},"start":{"character":10,"line":15}}},{"detail":"const int","kind":13,"name":"Bottom_Left","range":{"end":{"character":29,"line":16},"start":{"character":0,"line":16}},"selectionRange":{"end":{"character":21,"line":16},"start":{"character":10,"line":16}}},{"detail":"const int","kind":13,"name":"Top_Right","range":{"end":{"character":28,"line":17},"start":{"character":0,"line":17}},"selectionRange":{"end":{"character":19,"line":17},"start":{"character":10,"line":17}}},{"detail":"const int","kind":13,"name":"Bottom_Right","range":{"end":{"character":28,"line":18},"start":{"character":0,"line":18}},"selectionRange":{"end":{"character":22,"line":18},"start":{"character":10,"line":18}}},{"detail":"const int","kind":13,"name":"Stop","range":{"end":{"character":27,"line":19},"start":{"character":0,"line":19}},"selectionRange":{"end":{"character":14,"line":19},"start":{"character":10,"line":19}}},{"detail":"const int","kind":13,"name":"Contrarotate","range":{"end":{"character":29,"line":20},"start":{"character":0,"line":20}},"selectionRange":{"end":{"character":22,"line":20},"start":{"character":10,"line":20}}},{"detail":"const int","kind":13,"name":"Clockwise","range":{"end":{"character":28,"line":21},"start":{"character":0,"line":21}},"selectionRange":{"end":{"character":19,"line":21},"start":{"character":10,"line":21}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":24},"start":{"character":0,"line":24}},"selectionRange":{"end":{"character":10,"line":24},"start":{"character":5,"line":24}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":26},"start":{"character":0,"line":26}},"selectionRange":{"end":{"character":9,"line":26},"start":{"character":5,"line":26}}},{"detail":"void (int, int)","kind":12,"name":"Motor","range":{"end":{"character":30,"line":28},"start":{"character":0,"line":28}},"selectionRange":{"end":{"character":10,"line":28},"start":{"character":5,"line":28}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":1,"line":38},"start":{"character":0,"line":30}},"selectionRange":{"end":{"character":10,"line":30},"start":{"character":5,"line":30}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":75},"start":{"character":0,"line":40}},"selectionRange":{"end":{"character":9,"line":40},"start":{"character":5,"line":40}}},{"detail":"void (int, int)","kind":12,"name":"Motor","range":{"end":{"character":1,"line":86},"start":{"character":0,"line":77}},"selectionRange":{"end":{"character":10,"line":77},"start":{"character":5,"line":77}}}]}

I[13:38:59.252] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp (613 symbols, 3659 refs, 35 files)
I[13:38:59.830] --> $/progress
V[13:38:59.830] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"2/27","percentage":7}}}

I[13:38:59.830] --> $/progress
V[13:38:59.830] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"2/27","percentage":7}}}

V[13:38:59.832] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp (digest:=F68AA83B5BAAD75D)
I[13:38:59.924] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp (22 symbols, 151 refs, 5 files)
I[13:39:00.070] --> $/progress
V[13:39:00.070] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"3/27","percentage":11}}}

I[13:39:00.070] --> $/progress
V[13:39:00.070] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"3/27","percentage":11}}}

V[13:39:00.074] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c (digest:=343A7ACAD5FD2414)
V[13:39:00.082] <<< {"id":"4","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":40,"line":18},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:00.082] <-- textDocument/hover("4")
V[13:39:00.082] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:00.085] --> reply:textDocument/hover("4") 3 ms
V[13:39:00.085] >>> {"id":"4","jsonrpc":"2.0","result":null}

I[13:39:00.131] --> $/progress
V[13:39:00.131] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"4/27","percentage":14}}}

I[13:39:00.131] --> $/progress
V[13:39:00.131] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"4/27","percentage":14}}}

V[13:39:00.134] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c (digest:=5D6C1534064234DD)
I[13:39:00.145] --> $/progress
V[13:39:00.145] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"5/27","percentage":18}}}

I[13:39:00.145] --> $/progress
V[13:39:00.145] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"5/27","percentage":18}}}

V[13:39:00.148] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp (digest:=D7FFC6931C21680C)
I[13:39:00.149] --> $/progress
V[13:39:00.149] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"6/27","percentage":22}}}

I[13:39:00.149] --> $/progress
V[13:39:00.149] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"6/27","percentage":22}}}

V[13:39:00.149] BackgroundIndex: building version 1 after indexing enough files
V[13:39:00.153] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp (digest:=81BB1157C290C33B)
I[13:39:00.158] --> $/progress
V[13:39:00.158] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"7/27","percentage":25}}}

I[13:39:00.159] --> $/progress
V[13:39:00.159] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"7/27","percentage":25}}}

V[13:39:00.160] BackgroundIndex: serving version 1 (1468902 bytes)
I[13:39:00.161] --> $/progress
V[13:39:00.161] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"8/27","percentage":29}}}

I[13:39:00.161] --> $/progress
V[13:39:00.161] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"8/27","percentage":29}}}

V[13:39:00.164] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp (digest:=293923F15565174B)
V[13:39:00.165] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp (digest:=487C94A1A1F49B6C)
I[13:39:00.168] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c (266 symbols, 2773 refs, 25 files)
I[13:39:00.216] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c (310 symbols, 2769 refs, 25 files)
I[13:39:00.254] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp (299 symbols, 2470 refs, 18 files)
I[13:39:00.260] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp (596 symbols, 3444 refs, 37 files)
I[13:39:00.266] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp (598 symbols, 3578 refs, 35 files)
I[13:39:00.269] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp (600 symbols, 3461 refs, 37 files)
I[13:39:00.363] --> $/progress
V[13:39:00.363] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"9/27","percentage":33}}}

I[13:39:00.363] --> $/progress
V[13:39:00.363] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"9/27","percentage":33}}}

V[13:39:00.435] System include extraction: target extracted: "avr"
V[13:39:00.435] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[13:39:00.435] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[13:39:00.435] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[13:39:00.435] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-gcc.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[13:39:00.436] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S (digest:=87583F1C920AA889)
V[13:39:00.507] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:54:1:expected identifier or '('
V[13:39:00.508] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:62:23:expected identifier or '('
V[13:39:00.508] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:63:23:expected identifier or '('
V[13:39:00.508] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:64:23:expected identifier or '('
V[13:39:00.508] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:65:23:expected identifier or '('
V[13:39:00.508] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:66:23:expected identifier or '('
V[13:39:00.508] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:67:23:expected identifier or '('
V[13:39:00.508] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:72:37:expected identifier or '('
V[13:39:00.508] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:73:31:expected ';' after top level declarator
V[13:39:00.508] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:79:23:expected identifier or '('
V[13:39:00.509] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:83:32:expected identifier or '('
V[13:39:00.509] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:83:35:expected identifier or '('
V[13:39:00.509] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:84:22:unknown type name 'maxloops'
V[13:39:00.509] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:85:8:expected ';' after top level declarator
V[13:39:00.510] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:85:22:unknown type name 'maxloops'
V[13:39:00.510] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:86:8:expected ';' after top level declarator
V[13:39:00.510] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:86:22:unknown type name 'maxloops'
V[13:39:00.510] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:87:9:expected ';' after top level declarator
V[13:39:00.510] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:87:18:expected identifier or '('
V[13:39:00.510] Ignored diagnostic. too many errors emitted, stopping now
I[13:39:00.516] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S (12 symbols, 937 refs, 9 files)
I[13:39:00.516] Failed to compile C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S, index may be incomplete
I[13:39:00.587] --> $/progress
V[13:39:00.587] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"10/27","percentage":37}}}

I[13:39:00.587] --> $/progress
V[13:39:00.587] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"10/27","percentage":37}}}

V[13:39:00.599] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp (digest:=3DD4F70FCF8C4FA6)
I[13:39:00.708] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp (600 symbols, 3461 refs, 37 files)
I[13:39:00.783] --> $/progress
V[13:39:00.783] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"11/27","percentage":40}}}

I[13:39:00.783] --> $/progress
V[13:39:00.783] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"11/27","percentage":40}}}

I[13:39:00.787] --> $/progress
V[13:39:00.787] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"12/27","percentage":44}}}

I[13:39:00.787] --> $/progress
V[13:39:00.787] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"12/27","percentage":44}}}

V[13:39:00.788] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp (digest:=4A1244E54C0CAC04)
V[13:39:00.796] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c (digest:=B0774BE9D28D49CB)
I[13:39:00.835] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp (42 symbols, 134 refs, 3 files)
I[13:39:00.872] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c (307 symbols, 2663 refs, 25 files)
I[13:39:00.947] --> $/progress
V[13:39:00.947] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"13/27","percentage":48}}}

I[13:39:00.947] --> $/progress
V[13:39:00.947] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"13/27","percentage":48}}}

V[13:39:00.952] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c (digest:=BC32CF542FD8D605)
I[13:39:01.024] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c (308 symbols, 2723 refs, 25 files)
I[13:39:01.199] --> $/progress
V[13:39:01.199] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"14/27","percentage":51}}}

I[13:39:01.199] --> $/progress
V[13:39:01.200] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"14/27","percentage":51}}}

V[13:39:01.201] Indexing C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp (digest:=4123CC6579BB460A)
I[13:39:01.253] --> $/progress
V[13:39:01.253] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"15/27","percentage":55}}}

I[13:39:01.253] --> $/progress
V[13:39:01.253] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"15/27","percentage":55}}}

V[13:39:01.256] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp (digest:=313C4893EB7ADBE6)
I[13:39:01.257] --> $/progress
V[13:39:01.257] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"16/27","percentage":59}}}

I[13:39:01.257] --> $/progress
V[13:39:01.257] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"16/27","percentage":59}}}

V[13:39:01.258] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp (digest:=FDB5BCAAB3E73FCE)
I[13:39:01.309] Indexed C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp (612 symbols, 3496 refs, 35 files)
I[13:39:01.349] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp (602 symbols, 3436 refs, 35 files)
I[13:39:01.351] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp (600 symbols, 3432 refs, 36 files)
I[13:39:01.368] --> $/progress
V[13:39:01.368] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"17/27","percentage":62}}}

I[13:39:01.368] --> $/progress
V[13:39:01.368] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"17/27","percentage":62}}}

V[13:39:01.369] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c (digest:=0A36B38756A4F148)
I[13:39:01.432] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c (309 symbols, 2688 refs, 25 files)
I[13:39:01.473] --> $/progress
V[13:39:01.473] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"18/27","percentage":66}}}

I[13:39:01.473] --> $/progress
V[13:39:01.473] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"18/27","percentage":66}}}

V[13:39:01.479] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp (digest:=365287FBD658A80E)
I[13:39:01.504] --> $/progress
V[13:39:01.504] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"19/27","percentage":70}}}

I[13:39:01.504] --> $/progress
V[13:39:01.504] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"19/27","percentage":70}}}

V[13:39:01.507] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp (digest:=6DDB6ED4F4E34E63)
I[13:39:01.572] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp (601 symbols, 3490 refs, 37 files)
I[13:39:01.595] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp (620 symbols, 3567 refs, 36 files)
I[13:39:01.924] --> $/progress
V[13:39:01.924] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"20/27","percentage":74}}}

I[13:39:01.924] --> $/progress
V[13:39:01.924] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"20/27","percentage":74}}}

V[13:39:01.928] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c (digest:=C16B0ED8B1C5BB9F)
I[13:39:01.970] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c (1 symbols, 1 refs, 1 files)
I[13:39:01.980] --> $/progress
V[13:39:01.980] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"21/27","percentage":77}}}

I[13:39:01.980] --> $/progress
V[13:39:01.980] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"21/27","percentage":77}}}

I[13:39:01.980] --> $/progress
V[13:39:01.980] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"22/27","percentage":81}}}

V[13:39:01.982] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp (digest:=38075D39C713EC91)
I[13:39:02.008] --> $/progress
V[13:39:02.008] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"23/27","percentage":85}}}

I[13:39:02.009] --> $/progress
V[13:39:02.009] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"24/27","percentage":88}}}

I[13:39:02.017] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp (46 symbols, 139 refs, 3 files)
I[13:39:02.100] --> $/progress
V[13:39:02.100] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"25/27","percentage":92}}}

I[13:39:02.158] --> $/progress
V[13:39:02.158] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"26/27","percentage":96}}}

V[13:39:02.178] BackgroundIndex: building version 2 when background indexer is idle
V[13:39:02.189] BackgroundIndex: serving version 2 (1776382 bytes)
I[13:39:02.190] --> $/progress
V[13:39:02.190] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[13:39:10.355] <<< {"id":"5","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":48,"line":15},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:10.355] <-- textDocument/hover("5")
V[13:39:10.358] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:10.361] --> reply:textDocument/hover("5") 6 ms
V[13:39:10.361] >>> {"id":"5","jsonrpc":"2.0","result":null}

V[13:39:27.552] <<< {"id":"6","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":64,"line":7},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:27.552] <-- textDocument/hover("6")
V[13:39:27.555] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:27.558] --> reply:textDocument/hover("6") 6 ms
V[13:39:27.558] >>> {"id":"6","jsonrpc":"2.0","result":null}

V[13:39:27.862] <<< {"id":"7","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":63,"line":6},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:27.862] <-- textDocument/hover("7")
V[13:39:27.862] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:27.865] --> reply:textDocument/hover("7") 3 ms
V[13:39:27.865] >>> {"id":"7","jsonrpc":"2.0","result":null}

V[13:39:28.172] <<< {"id":"8","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":63,"line":6},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:28.172] <-- textDocument/hover("8")
V[13:39:28.172] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:28.175] --> reply:textDocument/hover("8") 3 ms
V[13:39:28.175] >>> {"id":"8","jsonrpc":"2.0","result":null}

V[13:39:28.546] <<< {"id":"9","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":62,"line":6},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:28.546] <-- textDocument/hover("9")
V[13:39:28.546] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:28.549] --> reply:textDocument/hover("9") 3 ms
V[13:39:28.549] >>> {"id":"9","jsonrpc":"2.0","result":null}

V[13:39:29.159] <<< {"id":"10","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":62,"line":6},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:29.159] <-- textDocument/hover("10")
V[13:39:29.159] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:29.163] --> reply:textDocument/hover("10") 3 ms
V[13:39:29.163] >>> {"id":"10","jsonrpc":"2.0","result":null}

V[13:39:29.627] <<< {"id":"11","jsonrpc":"2.0","method":"textDocument/documentHighlight","params":{"position":{"character":63,"line":6},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:29.627] <-- textDocument/documentHighlight("11")
V[13:39:29.627] ASTWorker running Highlights on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:29.627] --> reply:textDocument/documentHighlight("11") 0 ms
V[13:39:29.627] >>> {"id":"11","jsonrpc":"2.0","result":[]}

V[13:39:29.880] <<< {"id":"12","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":63,"line":6},"start":{"character":63,"line":6}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:29.880] <-- textDocument/codeAction("12")
V[13:39:29.880] ASTWorker running EnumerateTweaks on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:29.880] --> reply:textDocument/codeAction("12") 0 ms
V[13:39:29.880] >>> {"id":"12","jsonrpc":"2.0","result":[]}

V[13:39:30.337] <<< {"id":"13","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":63,"line":6},"start":{"character":63,"line":6}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:30.337] <-- textDocument/codeAction("13")
V[13:39:30.337] ASTWorker running EnumerateTweaks on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:30.337] --> reply:textDocument/codeAction("13") 0 ms
V[13:39:30.337] >>> {"id":"13","jsonrpc":"2.0","result":[]}

V[13:39:30.619] <<< {"id":"14","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":63,"line":6},"start":{"character":63,"line":6}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:30.619] <-- textDocument/codeAction("14")
V[13:39:30.619] ASTWorker running EnumerateTweaks on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:30.619] --> reply:textDocument/codeAction("14") 0 ms
V[13:39:30.619] >>> {"id":"14","jsonrpc":"2.0","result":[]}

V[13:39:30.920] <<< {"id":"15","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":63,"line":6},"start":{"character":63,"line":6}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:30.920] <-- textDocument/codeAction("15")
V[13:39:30.920] ASTWorker running EnumerateTweaks on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:30.920] --> reply:textDocument/codeAction("15") 0 ms
V[13:39:30.920] >>> {"id":"15","jsonrpc":"2.0","result":[]}

V[13:39:32.671] <<< {"id":"16","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":67,"line":6},"start":{"character":63,"line":6}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:32.671] <-- textDocument/codeAction("16")
V[13:39:32.675] ASTWorker running EnumerateTweaks on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:32.675] --> reply:textDocument/codeAction("16") 3 ms
V[13:39:32.675] >>> {"id":"16","jsonrpc":"2.0","result":[]}

V[13:39:33.019] <<< {"id":"17","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":70,"line":9},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:33.019] <-- textDocument/hover("17")
V[13:39:33.019] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:33.022] --> reply:textDocument/hover("17") 3 ms
V[13:39:33.022] >>> {"id":"17","jsonrpc":"2.0","result":null}

V[13:39:33.191] <<< {"id":"18","jsonrpc":"2.0","method":"textDocument/definition","params":{"position":{"character":70,"line":9},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:33.191] <-- textDocument/definition("18")
V[13:39:33.192] ASTWorker running Definitions on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:33.192] --> reply:textDocument/definition("18") 0 ms
V[13:39:33.192] >>> {"id":"18","jsonrpc":"2.0","result":[]}

V[13:39:33.414] <<< {"id":"19","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":69,"line":9},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:33.414] <-- textDocument/hover("19")
V[13:39:33.414] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:33.417] --> reply:textDocument/hover("19") 3 ms
V[13:39:33.417] >>> {"id":"19","jsonrpc":"2.0","result":null}

V[13:39:33.695] <<< {"id":"20","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:33.695] <-- textDocument/documentSymbol("20")
V[13:39:33.695] ASTWorker running DocumentSymbols on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:33.696] --> reply:textDocument/documentSymbol("20") 0 ms
V[13:39:33.696] >>> {"id":"20","jsonrpc":"2.0","result":[{"detail":"const int","kind":13,"name":"Forward","range":{"end":{"character":28,"line":11},"start":{"character":0,"line":11}},"selectionRange":{"end":{"character":17,"line":11},"start":{"character":10,"line":11}}},{"detail":"const int","kind":13,"name":"Backward","range":{"end":{"character":29,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":18,"line":12},"start":{"character":10,"line":12}}},{"detail":"const int","kind":13,"name":"Turn_Left","range":{"end":{"character":29,"line":13},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":19,"line":13},"start":{"character":10,"line":13}}},{"detail":"const int","kind":13,"name":"Turn_Right","range":{"end":{"character":29,"line":14},"start":{"character":0,"line":14}},"selectionRange":{"end":{"character":20,"line":14},"start":{"character":10,"line":14}}},{"detail":"const int","kind":13,"name":"Top_Left","range":{"end":{"character":28,"line":15},"start":{"character":0,"line":15}},"selectionRange":{"end":{"character":18,"line":15},"start":{"character":10,"line":15}}},{"detail":"const int","kind":13,"name":"Bottom_Left","range":{"end":{"character":29,"line":16},"start":{"character":0,"line":16}},"selectionRange":{"end":{"character":21,"line":16},"start":{"character":10,"line":16}}},{"detail":"const int","kind":13,"name":"Top_Right","range":{"end":{"character":28,"line":17},"start":{"character":0,"line":17}},"selectionRange":{"end":{"character":19,"line":17},"start":{"character":10,"line":17}}},{"detail":"const int","kind":13,"name":"Bottom_Right","range":{"end":{"character":28,"line":18},"start":{"character":0,"line":18}},"selectionRange":{"end":{"character":22,"line":18},"start":{"character":10,"line":18}}},{"detail":"const int","kind":13,"name":"Stop","range":{"end":{"character":27,"line":19},"start":{"character":0,"line":19}},"selectionRange":{"end":{"character":14,"line":19},"start":{"character":10,"line":19}}},{"detail":"const int","kind":13,"name":"Contrarotate","range":{"end":{"character":29,"line":20},"start":{"character":0,"line":20}},"selectionRange":{"end":{"character":22,"line":20},"start":{"character":10,"line":20}}},{"detail":"const int","kind":13,"name":"Clockwise","range":{"end":{"character":28,"line":21},"start":{"character":0,"line":21}},"selectionRange":{"end":{"character":19,"line":21},"start":{"character":10,"line":21}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":24},"start":{"character":0,"line":24}},"selectionRange":{"end":{"character":10,"line":24},"start":{"character":5,"line":24}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":26},"start":{"character":0,"line":26}},"selectionRange":{"end":{"character":9,"line":26},"start":{"character":5,"line":26}}},{"detail":"void (int, int)","kind":12,"name":"Motor","range":{"end":{"character":30,"line":28},"start":{"character":0,"line":28}},"selectionRange":{"end":{"character":10,"line":28},"start":{"character":5,"line":28}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":1,"line":38},"start":{"character":0,"line":30}},"selectionRange":{"end":{"character":10,"line":30},"start":{"character":5,"line":30}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":75},"start":{"character":0,"line":40}},"selectionRange":{"end":{"character":9,"line":40},"start":{"character":5,"line":40}}},{"detail":"void (int, int)","kind":12,"name":"Motor","range":{"end":{"character":1,"line":86},"start":{"character":0,"line":77}},"selectionRange":{"end":{"character":10,"line":77},"start":{"character":5,"line":77}}}]}

V[13:39:33.773] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"range":{"end":{"character":70,"line":9},"start":{"character":63,"line":9}},"text":"Memory register clock        "},{"range":{"end":{"character":67,"line":8},"start":{"character":63,"line":8}},"text":"Serial data"},{"range":{"end":{"character":67,"line":7},"start":{"character":63,"line":7}},"text":"Can make control"},{"range":{"end":{"character":67,"line":6},"start":{"character":63,"line":6}},"text":"The displacement of the clock"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":5}}}

I[13:39:33.773] <-- textDocument/didChange
V[13:39:33.775] <<< {"id":"21","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:33.775] <-- textDocument/documentSymbol("21")
I[13:39:33.776] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 5 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:39:33.800] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 1_Auto_move.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:39:33.802] Rebuilding invalidated preamble for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 5 (previous was version 1)
V[13:39:33.825] ASTWorker rebuilding evicted AST to run DocumentSymbols: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 5
V[13:39:33.870] indexed preamble AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 5:
  symbol slab: 2505 symbols, 716894 bytes
  ref slab: 0 symbols, 0 refs, 136 bytes
  relations slab: 9 relations, 177 bytes
V[13:39:33.871] ASTWorker running DocumentSymbols on version 5 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:33.871] --> reply:textDocument/documentSymbol("21") 96 ms
V[13:39:33.872] >>> {"id":"21","jsonrpc":"2.0","result":[{"detail":"const int","kind":13,"name":"Forward","range":{"end":{"character":28,"line":11},"start":{"character":0,"line":11}},"selectionRange":{"end":{"character":17,"line":11},"start":{"character":10,"line":11}}},{"detail":"const int","kind":13,"name":"Backward","range":{"end":{"character":29,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":18,"line":12},"start":{"character":10,"line":12}}},{"detail":"const int","kind":13,"name":"Turn_Left","range":{"end":{"character":29,"line":13},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":19,"line":13},"start":{"character":10,"line":13}}},{"detail":"const int","kind":13,"name":"Turn_Right","range":{"end":{"character":29,"line":14},"start":{"character":0,"line":14}},"selectionRange":{"end":{"character":20,"line":14},"start":{"character":10,"line":14}}},{"detail":"const int","kind":13,"name":"Top_Left","range":{"end":{"character":28,"line":15},"start":{"character":0,"line":15}},"selectionRange":{"end":{"character":18,"line":15},"start":{"character":10,"line":15}}},{"detail":"const int","kind":13,"name":"Bottom_Left","range":{"end":{"character":29,"line":16},"start":{"character":0,"line":16}},"selectionRange":{"end":{"character":21,"line":16},"start":{"character":10,"line":16}}},{"detail":"const int","kind":13,"name":"Top_Right","range":{"end":{"character":28,"line":17},"start":{"character":0,"line":17}},"selectionRange":{"end":{"character":19,"line":17},"start":{"character":10,"line":17}}},{"detail":"const int","kind":13,"name":"Bottom_Right","range":{"end":{"character":28,"line":18},"start":{"character":0,"line":18}},"selectionRange":{"end":{"character":22,"line":18},"start":{"character":10,"line":18}}},{"detail":"const int","kind":13,"name":"Stop","range":{"end":{"character":27,"line":19},"start":{"character":0,"line":19}},"selectionRange":{"end":{"character":14,"line":19},"start":{"character":10,"line":19}}},{"detail":"const int","kind":13,"name":"Contrarotate","range":{"end":{"character":29,"line":20},"start":{"character":0,"line":20}},"selectionRange":{"end":{"character":22,"line":20},"start":{"character":10,"line":20}}},{"detail":"const int","kind":13,"name":"Clockwise","range":{"end":{"character":28,"line":21},"start":{"character":0,"line":21}},"selectionRange":{"end":{"character":19,"line":21},"start":{"character":10,"line":21}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":24},"start":{"character":0,"line":24}},"selectionRange":{"end":{"character":10,"line":24},"start":{"character":5,"line":24}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":26},"start":{"character":0,"line":26}},"selectionRange":{"end":{"character":9,"line":26},"start":{"character":5,"line":26}}},{"detail":"void (int, int)","kind":12,"name":"Motor","range":{"end":{"character":30,"line":28},"start":{"character":0,"line":28}},"selectionRange":{"end":{"character":10,"line":28},"start":{"character":5,"line":28}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":1,"line":38},"start":{"character":0,"line":30}},"selectionRange":{"end":{"character":10,"line":30},"start":{"character":5,"line":30}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":75},"start":{"character":0,"line":40}},"selectionRange":{"end":{"character":9,"line":40},"start":{"character":5,"line":40}}},{"detail":"void (int, int)","kind":12,"name":"Motor","range":{"end":{"character":1,"line":86},"start":{"character":0,"line":77}},"selectionRange":{"end":{"character":10,"line":77},"start":{"character":5,"line":77}}}]}

V[13:39:33.898] Build dynamic index for header symbols with estimated memory usage of 2164194 bytes
V[13:39:33.900] Built preamble of size 428728 for file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 5
V[13:39:33.937] <<< {"id":"22","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":92,"line":6},"start":{"character":92,"line":6}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:33.937] <-- textDocument/codeAction("22")
V[13:39:33.955] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 5:
  symbol slab: 20 symbols, 8864 bytes
  ref slab: 29 symbols, 91 refs, 5240 bytes
  relations slab: 0 relations, 24 bytes
V[13:39:33.955] Build dynamic index for main-file symbols with estimated memory usage of 24216 bytes
I[13:39:33.955] --> textDocument/publishDiagnostics
V[13:39:33.955] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":5}}

V[13:39:33.956] ASTWorker running EnumerateTweaks on version 5 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:33.956] --> reply:textDocument/codeAction("22") 18 ms
V[13:39:33.956] >>> {"id":"22","jsonrpc":"2.0","result":[]}

V[13:39:36.442] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:36.442] <-- textDocument/didSave
I[13:39:36.442] File version went from 5 to 5
V[13:39:36.442] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\n// PWM 控制引脚\n#define PWM1_PIN            5\n#define PWM2_PIN            6      \n// 74HCT595N 芯片引脚\n#define SHCP_PIN            2                               // The displacement of the clock\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":6}}}

I[13:39:36.442] <-- textDocument/didChange
V[13:39:36.442] ASTWorker skipping Update (5) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:36.503] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 6 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:39:36.526] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 1_Auto_move.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:39:36.527] Rebuilding invalidated preamble for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 6 (previous was version 5)
V[13:39:36.593] indexed preamble AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 6:
  symbol slab: 2502 symbols, 716198 bytes
  ref slab: 0 symbols, 0 refs, 136 bytes
  relations slab: 9 relations, 177 bytes
V[13:39:36.621] Build dynamic index for header symbols with estimated memory usage of 2163590 bytes
V[13:39:36.623] Built preamble of size 428228 for file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 6
V[13:39:36.672] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 6:
  symbol slab: 3 symbols, 4920 bytes
  ref slab: 3 symbols, 3 refs, 4304 bytes
  relations slab: 0 relations, 24 bytes
V[13:39:36.672] Build dynamic index for main-file symbols with estimated memory usage of 12576 bytes
I[13:39:36.672] --> textDocument/publishDiagnostics
V[13:39:36.672] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":6}}

V[13:39:51.859] <<< {"id":"23","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:51.859] <-- textDocument/documentSymbol("23")
V[13:39:51.863] ASTWorker running DocumentSymbols on version 6 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:51.863] --> reply:textDocument/documentSymbol("23") 4 ms
V[13:39:51.863] >>> {"id":"23","jsonrpc":"2.0","result":[]}

V[13:39:51.866] <<< {"id":"24","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:51.866] <-- textDocument/documentSymbol("24")
V[13:39:51.866] ASTWorker running DocumentSymbols on version 6 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:51.866] --> reply:textDocument/documentSymbol("24") 0 ms
V[13:39:51.866] >>> {"id":"24","jsonrpc":"2.0","result":[]}

V[13:39:53.379] <<< {"id":"25","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:53.379] <-- textDocument/documentSymbol("25")
V[13:39:53.379] ASTWorker running DocumentSymbols on version 6 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:53.379] --> reply:textDocument/documentSymbol("25") 0 ms
V[13:39:53.379] >>> {"id":"25","jsonrpc":"2.0","result":[]}

V[13:39:54.597] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:54.597] <-- textDocument/didSave
I[13:39:54.597] File version went from 6 to 6
V[13:39:54.597] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\n// PWM 控制引脚\n#define PWM1_PIN            5\n#define PWM2_PIN            6      \n// 74HCT595N 芯片引脚\n#define SHCP_PIN            2                               // The displacement of the clock\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":7}}}

I[13:39:54.597] <-- textDocument/didChange
V[13:39:54.597] ASTWorker skipping Update (6) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:54.659] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\compile_commands.json
V[13:39:54.659] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124
I[13:39:54.659] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 7 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
I[13:39:54.663] --> window/workDoneProgress/create(1)
V[13:39:54.663] >>> {"id":1,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[13:39:54.663] Enqueueing 26 commands for indexing
V[13:39:54.663] <<< {"id":1,"jsonrpc":"2.0","result":null}

I[13:39:54.663] <-- reply(1)
I[13:39:54.663] --> $/progress
V[13:39:54.663] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[13:39:54.663] --> $/progress
V[13:39:54.663] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[13:39:54.687] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 1_Auto_move.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:39:54.688] BackgroundIndex: building version 3 after loading index from disk
V[13:39:54.694] Reusing preamble version 6 for version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
V[13:39:54.698] BackgroundIndex: serving version 3 (1772786 bytes)
I[13:39:54.711] --> $/progress
V[13:39:54.711] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[13:39:54.711] --> $/progress
V[13:39:54.711] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[13:39:58.192] <<< {"id":"26","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:39:58.192] <-- textDocument/documentSymbol("26")
V[13:39:58.195] ASTWorker running DocumentSymbols on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:39:58.195] --> reply:textDocument/documentSymbol("26") 3 ms
V[13:39:58.195] >>> {"id":"26","jsonrpc":"2.0","result":[]}

V[13:40:08.445] <<< {"id":"27","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":10,"line":2},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:08.445] <-- textDocument/hover("27")
V[13:40:08.448] ASTWorker running Hover on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:08.451] --> reply:textDocument/hover("27") 6 ms
V[13:40:08.451] >>> {"id":"27","jsonrpc":"2.0","result":null}

V[13:40:08.777] <<< {"id":"28","jsonrpc":"2.0","method":"textDocument/documentHighlight","params":{"position":{"character":11,"line":2},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:08.777] <-- textDocument/documentHighlight("28")
V[13:40:08.777] ASTWorker running Highlights on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:08.777] --> reply:textDocument/documentHighlight("28") 0 ms
V[13:40:08.777] >>> {"id":"28","jsonrpc":"2.0","result":[]}

V[13:40:08.779] <<< {"id":"29","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:08.779] <-- textDocument/documentSymbol("29")
V[13:40:08.779] ASTWorker running DocumentSymbols on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:08.779] --> reply:textDocument/documentSymbol("29") 0 ms
V[13:40:08.779] >>> {"id":"29","jsonrpc":"2.0","result":[]}

V[13:40:08.836] <<< {"id":"30","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:08.836] <-- textDocument/documentSymbol("30")
V[13:40:08.836] ASTWorker running DocumentSymbols on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:08.836] --> reply:textDocument/documentSymbol("30") 0 ms
V[13:40:08.836] >>> {"id":"30","jsonrpc":"2.0","result":[]}

V[13:40:08.902] <<< {"id":"31","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:08.902] <-- textDocument/documentSymbol("31")
V[13:40:08.902] ASTWorker running DocumentSymbols on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:08.902] --> reply:textDocument/documentSymbol("31") 0 ms
V[13:40:08.902] >>> {"id":"31","jsonrpc":"2.0","result":[]}

V[13:40:09.054] <<< {"id":"32","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:09.054] <-- textDocument/documentSymbol("32")
V[13:40:09.054] ASTWorker running DocumentSymbols on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:09.054] --> reply:textDocument/documentSymbol("32") 0 ms
V[13:40:09.054] >>> {"id":"32","jsonrpc":"2.0","result":[]}

V[13:40:09.151] <<< {"id":"33","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:09.151] <-- textDocument/documentSymbol("33")
V[13:40:09.151] ASTWorker running DocumentSymbols on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:09.151] --> reply:textDocument/documentSymbol("33") 0 ms
V[13:40:09.151] >>> {"id":"33","jsonrpc":"2.0","result":[]}

V[13:40:09.408] <<< {"id":"34","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":11,"line":2},"start":{"character":7,"line":2}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:09.408] <-- textDocument/codeAction("34")
V[13:40:09.408] ASTWorker running EnumerateTweaks on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:09.408] --> reply:textDocument/codeAction("34") 0 ms
V[13:40:09.408] >>> {"id":"34","jsonrpc":"2.0","result":[]}

V[13:40:09.532] <<< {"id":"35","jsonrpc":"2.0","method":"textDocument/definition","params":{"position":{"character":7,"line":2},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:09.532] <-- textDocument/definition("35")
V[13:40:09.532] ASTWorker running Definitions on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:09.532] --> reply:textDocument/definition("35") 0 ms
V[13:40:09.532] >>> {"id":"35","jsonrpc":"2.0","result":[]}

V[13:40:09.701] <<< {"id":"36","jsonrpc":"2.0","method":"textDocument/definition","params":{"position":{"character":15,"line":4},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:09.701] <-- textDocument/definition("36")
V[13:40:09.701] ASTWorker running Definitions on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:09.701] --> reply:textDocument/definition("36") 0 ms
V[13:40:09.701] >>> {"id":"36","jsonrpc":"2.0","result":[{"range":{"end":{"character":16,"line":4},"start":{"character":8,"line":4}},"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}]}

V[13:40:09.901] <<< {"id":"37","jsonrpc":"2.0","method":"textDocument/definition","params":{"position":{"character":28,"line":7},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:09.901] <-- textDocument/definition("37")
V[13:40:09.901] ASTWorker running Definitions on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
E[13:40:09.901] locateSymbolAt failed to convert position to source location: utf-16 offset 28 is invalid for line 7
I[13:40:09.901] --> reply:textDocument/definition("37") 0 ms
V[13:40:09.901] >>> {"id":"37","jsonrpc":"2.0","result":[]}

V[13:40:10.282] <<< {"id":"38","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:10.282] <-- textDocument/documentSymbol("38")
V[13:40:10.282] ASTWorker running DocumentSymbols on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:10.282] --> reply:textDocument/documentSymbol("38") 0 ms
V[13:40:10.282] >>> {"id":"38","jsonrpc":"2.0","result":[]}

V[13:40:10.290] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"range":{"end":{"character":11,"line":2},"start":{"character":7,"line":2}},"text":"control pin"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":8}}}

I[13:40:10.290] <-- textDocument/didChange
V[13:40:10.291] <<< {"id":"39","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:10.291] <-- textDocument/documentSymbol("39")
I[13:40:10.292] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 8 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:40:10.316] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 1_Auto_move.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:40:10.317] Rebuilding invalidated preamble for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 8 (previous was version 6)
V[13:40:10.341] ASTWorker rebuilding evicted AST to run DocumentSymbols: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 8
V[13:40:10.386] indexed preamble AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 8:
  symbol slab: 2502 symbols, 712102 bytes
  ref slab: 0 symbols, 0 refs, 136 bytes
  relations slab: 9 relations, 177 bytes
V[13:40:10.387] ASTWorker running DocumentSymbols on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:10.387] --> reply:textDocument/documentSymbol("39") 95 ms
V[13:40:10.387] >>> {"id":"39","jsonrpc":"2.0","result":[]}

V[13:40:10.413] Build dynamic index for header symbols with estimated memory usage of 2163462 bytes
V[13:40:10.415] Built preamble of size 428224 for file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 8
V[13:40:10.467] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 8:
  symbol slab: 3 symbols, 4920 bytes
  ref slab: 3 symbols, 3 refs, 4304 bytes
  relations slab: 0 relations, 24 bytes
V[13:40:10.467] Build dynamic index for main-file symbols with estimated memory usage of 12576 bytes
I[13:40:10.467] --> textDocument/publishDiagnostics
V[13:40:10.467] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":8}}

V[13:40:10.530] <<< {"id":"40","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":18,"line":2},"start":{"character":18,"line":2}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:10.530] <-- textDocument/codeAction("40")
V[13:40:10.530] ASTWorker running EnumerateTweaks on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:10.530] --> reply:textDocument/codeAction("40") 0 ms
V[13:40:10.530] >>> {"id":"40","jsonrpc":"2.0","result":[]}

V[13:40:13.772] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:13.772] <-- textDocument/didSave
I[13:40:13.772] File version went from 8 to 8
V[13:40:13.772] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\n// PWM control pin\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":9}}}

I[13:40:13.772] <-- textDocument/didChange
V[13:40:13.772] ASTWorker skipping Update (8) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:13.834] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 9 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:40:13.857] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 1_Auto_move.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:40:13.858] Rebuilding invalidated preamble for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 9 (previous was version 8)
V[13:40:13.925] indexed preamble AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 9:
  symbol slab: 2499 symbols, 711406 bytes
  ref slab: 0 symbols, 0 refs, 136 bytes
  relations slab: 9 relations, 177 bytes
V[13:40:13.953] Build dynamic index for header symbols with estimated memory usage of 2163494 bytes
V[13:40:13.956] Built preamble of size 427792 for file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 9
V[13:40:14.005] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 9:
  symbol slab: 0 symbols, 128 bytes
  ref slab: 0 symbols, 0 refs, 136 bytes
  relations slab: 0 relations, 24 bytes
V[13:40:14.005] Build dynamic index for main-file symbols with estimated memory usage of 264 bytes
I[13:40:14.006] --> textDocument/publishDiagnostics
V[13:40:14.006] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":9}}

V[13:40:16.520] <<< {"id":"41","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:16.520] <-- textDocument/documentSymbol("41")
V[13:40:16.520] ASTWorker running DocumentSymbols on version 9 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:16.520] --> reply:textDocument/documentSymbol("41") 0 ms
V[13:40:16.520] >>> {"id":"41","jsonrpc":"2.0","result":[]}

V[13:40:16.552] <<< {"id":"42","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:16.552] <-- textDocument/documentSymbol("42")
V[13:40:16.552] ASTWorker running DocumentSymbols on version 9 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:16.552] --> reply:textDocument/documentSymbol("42") 0 ms
V[13:40:16.552] >>> {"id":"42","jsonrpc":"2.0","result":[]}

V[13:40:16.651] <<< {"id":"43","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:16.651] <-- textDocument/documentSymbol("43")
V[13:40:16.651] ASTWorker running DocumentSymbols on version 9 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:16.651] --> reply:textDocument/documentSymbol("43") 0 ms
V[13:40:16.651] >>> {"id":"43","jsonrpc":"2.0","result":[]}

V[13:40:16.753] <<< {"id":"44","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:16.753] <-- textDocument/documentSymbol("44")
V[13:40:16.753] ASTWorker running DocumentSymbols on version 9 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:16.753] --> reply:textDocument/documentSymbol("44") 0 ms
V[13:40:16.753] >>> {"id":"44","jsonrpc":"2.0","result":[]}

V[13:40:16.869] <<< {"id":"45","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:16.869] <-- textDocument/documentSymbol("45")
V[13:40:16.869] ASTWorker running DocumentSymbols on version 9 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:16.869] --> reply:textDocument/documentSymbol("45") 0 ms
V[13:40:16.869] >>> {"id":"45","jsonrpc":"2.0","result":[]}

V[13:40:17.260] <<< {"id":"46","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:17.260] <-- textDocument/documentSymbol("46")
V[13:40:17.260] ASTWorker running DocumentSymbols on version 9 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:17.260] --> reply:textDocument/documentSymbol("46") 0 ms
V[13:40:17.260] >>> {"id":"46","jsonrpc":"2.0","result":[]}

V[13:40:17.263] <<< {"id":"47","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:17.263] <-- textDocument/documentSymbol("47")
V[13:40:17.263] ASTWorker running DocumentSymbols on version 9 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:17.263] --> reply:textDocument/documentSymbol("47") 0 ms
V[13:40:17.263] >>> {"id":"47","jsonrpc":"2.0","result":[]}

V[13:40:17.734] <<< {"id":"48","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:17.734] <-- textDocument/documentSymbol("48")
V[13:40:17.734] ASTWorker running DocumentSymbols on version 9 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:17.734] --> reply:textDocument/documentSymbol("48") 0 ms
V[13:40:17.734] >>> {"id":"48","jsonrpc":"2.0","result":[]}

V[13:40:20.022] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:40:20.022] <-- textDocument/didSave
I[13:40:20.022] File version went from 9 to 9
V[13:40:20.022] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\n// PWM control pin\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":10}}}

I[13:40:20.022] <-- textDocument/didChange
V[13:40:20.022] ASTWorker skipping Update (9) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:40:20.081] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\compile_commands.json
V[13:40:20.081] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124
I[13:40:20.081] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 10 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
I[13:40:20.085] --> window/workDoneProgress/create(2)
V[13:40:20.085] >>> {"id":2,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[13:40:20.085] Enqueueing 26 commands for indexing
V[13:40:20.085] <<< {"id":2,"jsonrpc":"2.0","result":null}

I[13:40:20.085] <-- reply(2)
I[13:40:20.085] --> $/progress
V[13:40:20.085] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[13:40:20.085] --> $/progress
V[13:40:20.085] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[13:40:20.106] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 1_Auto_move.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:40:20.108] BackgroundIndex: building version 4 after loading index from disk
V[13:40:20.114] Reusing preamble version 9 for version 10 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
V[13:40:20.119] BackgroundIndex: serving version 4 (1772786 bytes)
I[13:40:20.132] --> $/progress
V[13:40:20.132] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[13:40:20.132] --> $/progress
V[13:40:20.132] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[13:44:53.402] <<< {"id":"49","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:44:53.403] <-- textDocument/documentSymbol("49")
V[13:44:53.406] ASTWorker running DocumentSymbols on version 10 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:44:53.406] --> reply:textDocument/documentSymbol("49") 3 ms
V[13:44:53.406] >>> {"id":"49","jsonrpc":"2.0","result":[]}

V[13:44:54.018] <<< {"id":"50","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:44:54.018] <-- textDocument/documentSymbol("50")
V[13:44:54.018] ASTWorker running DocumentSymbols on version 10 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:44:54.018] --> reply:textDocument/documentSymbol("50") 0 ms
V[13:44:54.018] >>> {"id":"50","jsonrpc":"2.0","result":[]}

V[13:44:54.665] <<< {"id":"51","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:44:54.665] <-- textDocument/documentSymbol("51")
V[13:44:54.665] ASTWorker running DocumentSymbols on version 10 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:44:54.665] --> reply:textDocument/documentSymbol("51") 0 ms
V[13:44:54.665] >>> {"id":"51","jsonrpc":"2.0","result":[]}

V[13:44:54.668] <<< {"id":"52","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:44:54.668] <-- textDocument/documentSymbol("52")
V[13:44:54.668] ASTWorker running DocumentSymbols on version 10 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:44:54.668] --> reply:textDocument/documentSymbol("52") 0 ms
V[13:44:54.668] >>> {"id":"52","jsonrpc":"2.0","result":[]}

V[13:44:58.162] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:44:58.162] <-- textDocument/didSave
I[13:44:58.163] File version went from 10 to 10
V[13:44:58.163] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\n// PWM control pin\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":11}}}

I[13:44:58.163] <-- textDocument/didChange
V[13:44:58.163] ASTWorker skipping Update (10) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:44:58.226] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\compile_commands.json
V[13:44:58.226] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124
I[13:44:58.226] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 11 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
I[13:44:58.229] --> window/workDoneProgress/create(3)
V[13:44:58.229] >>> {"id":3,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[13:44:58.229] Enqueueing 26 commands for indexing
V[13:44:58.229] <<< {"id":3,"jsonrpc":"2.0","result":null}

I[13:44:58.229] <-- reply(3)
I[13:44:58.229] --> $/progress
V[13:44:58.229] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[13:44:58.229] --> $/progress
V[13:44:58.229] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[13:44:58.251] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 1_Auto_move.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:44:58.253] BackgroundIndex: building version 5 after loading index from disk
V[13:44:58.258] Reusing preamble version 9 for version 11 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
V[13:44:58.264] BackgroundIndex: serving version 5 (1772786 bytes)
I[13:44:58.275] --> $/progress
V[13:44:58.276] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[13:44:58.276] --> $/progress
V[13:44:58.276] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[13:46:23.879] <<< {"id":"53","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:46:23.879] <-- textDocument/documentSymbol("53")
V[13:46:23.883] ASTWorker running DocumentSymbols on version 11 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:46:23.883] --> reply:textDocument/documentSymbol("53") 3 ms
V[13:46:23.883] >>> {"id":"53","jsonrpc":"2.0","result":[]}

V[13:46:26.262] <<< {"id":"54","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:46:26.262] <-- textDocument/documentSymbol("54")
V[13:46:26.262] ASTWorker running DocumentSymbols on version 11 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:46:26.262] --> reply:textDocument/documentSymbol("54") 0 ms
V[13:46:26.262] >>> {"id":"54","jsonrpc":"2.0","result":[]}

V[13:46:27.375] <<< {"id":"55","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:46:27.375] <-- textDocument/documentSymbol("55")
V[13:46:27.375] ASTWorker running DocumentSymbols on version 11 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:46:27.375] --> reply:textDocument/documentSymbol("55") 0 ms
V[13:46:27.375] >>> {"id":"55","jsonrpc":"2.0","result":[]}

V[13:46:27.379] <<< {"id":"56","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:46:27.379] <-- textDocument/documentSymbol("56")
V[13:46:27.379] ASTWorker running DocumentSymbols on version 11 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:46:27.379] --> reply:textDocument/documentSymbol("56") 0 ms
V[13:46:27.379] >>> {"id":"56","jsonrpc":"2.0","result":[]}

V[13:46:30.868] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:46:30.868] <-- textDocument/didSave
I[13:46:30.868] File version went from 11 to 11
V[13:46:30.868] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\n// PWM control pin\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":12}}}

I[13:46:30.868] <-- textDocument/didChange
V[13:46:30.868] ASTWorker skipping Update (11) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:46:30.937] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\compile_commands.json
V[13:46:30.937] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124
I[13:46:30.937] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 12 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
I[13:46:30.940] --> window/workDoneProgress/create(4)
V[13:46:30.940] >>> {"id":4,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[13:46:30.940] Enqueueing 26 commands for indexing
V[13:46:30.941] <<< {"id":4,"jsonrpc":"2.0","result":null}

I[13:46:30.941] <-- reply(4)
I[13:46:30.941] --> $/progress
V[13:46:30.941] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[13:46:30.941] --> $/progress
V[13:46:30.941] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[13:46:30.963] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 1_Auto_move.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:46:30.965] BackgroundIndex: building version 6 after loading index from disk
V[13:46:30.971] Reusing preamble version 9 for version 12 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
V[13:46:30.976] BackgroundIndex: serving version 6 (1772786 bytes)
I[13:46:30.988] --> $/progress
V[13:46:30.988] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[13:46:30.988] --> $/progress
V[13:46:30.988] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[13:46:33.986] <<< {"id":"57","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:46:33.986] <-- textDocument/documentSymbol("57")
V[13:46:33.987] ASTWorker running DocumentSymbols on version 12 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:46:33.987] --> reply:textDocument/documentSymbol("57") 0 ms
V[13:46:33.987] >>> {"id":"57","jsonrpc":"2.0","result":[]}

V[13:46:36.635] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:46:36.635] <-- textDocument/didSave
I[13:46:36.635] File version went from 12 to 12
V[13:46:36.635] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\n// PWM control pin\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":13}}}

I[13:46:36.635] <-- textDocument/didChange
V[13:46:36.635] ASTWorker skipping Update (12) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:46:36.703] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\compile_commands.json
V[13:46:36.703] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124
I[13:46:36.703] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 13 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
I[13:46:36.706] --> window/workDoneProgress/create(5)
V[13:46:36.706] >>> {"id":5,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[13:46:36.706] Enqueueing 26 commands for indexing
V[13:46:36.706] <<< {"id":5,"jsonrpc":"2.0","result":null}

I[13:46:36.706] <-- reply(5)
I[13:46:36.706] --> $/progress
V[13:46:36.706] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[13:46:36.706] --> $/progress
V[13:46:36.706] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[13:46:36.728] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 1_Auto_move.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:46:36.729] BackgroundIndex: building version 7 after loading index from disk
V[13:46:36.735] Reusing preamble version 9 for version 13 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
V[13:46:36.740] BackgroundIndex: serving version 7 (1772786 bytes)
I[13:46:36.752] --> $/progress
V[13:46:36.752] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[13:46:36.752] --> $/progress
V[13:46:36.752] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[13:47:02.246] <<< {"id":"58","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:47:02.246] <-- textDocument/documentSymbol("58")
V[13:47:02.250] ASTWorker running DocumentSymbols on version 13 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:47:02.250] --> reply:textDocument/documentSymbol("58") 3 ms
V[13:47:02.250] >>> {"id":"58","jsonrpc":"2.0","result":[]}

V[13:47:11.109] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:47:11.109] <-- textDocument/didSave
I[13:47:11.109] File version went from 13 to 13
V[13:47:11.110] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\n// PWM control pin\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":14}}}

I[13:47:11.110] <-- textDocument/didChange
V[13:47:11.110] ASTWorker skipping Update (13) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:47:11.175] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\compile_commands.json
V[13:47:11.175] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124
I[13:47:11.175] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 14 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
I[13:47:11.179] --> window/workDoneProgress/create(6)
V[13:47:11.179] >>> {"id":6,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[13:47:11.179] Enqueueing 26 commands for indexing
V[13:47:11.179] <<< {"id":6,"jsonrpc":"2.0","result":null}

I[13:47:11.179] <-- reply(6)
I[13:47:11.179] --> $/progress
V[13:47:11.179] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[13:47:11.179] --> $/progress
V[13:47:11.179] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[13:47:11.200] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 1_Auto_move.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:47:11.202] BackgroundIndex: building version 8 after loading index from disk
V[13:47:11.208] Reusing preamble version 9 for version 14 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
V[13:47:11.213] BackgroundIndex: serving version 8 (1772786 bytes)
I[13:47:11.225] --> $/progress
V[13:47:11.225] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[13:47:11.225] --> $/progress
V[13:47:11.225] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[13:51:31.203] <<< {"id":"59","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:51:31.203] <-- textDocument/documentSymbol("59")
V[13:51:31.206] ASTWorker running DocumentSymbols on version 14 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:51:31.206] --> reply:textDocument/documentSymbol("59") 3 ms
V[13:51:31.206] >>> {"id":"59","jsonrpc":"2.0","result":[]}

V[13:51:33.856] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:51:33.856] <-- textDocument/didSave
I[13:51:33.856] File version went from 14 to 14
V[13:51:33.856] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\1_Auto_move\\\\1_Auto_move.ino\"\n// PWM control pin\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp","version":15}}}

I[13:51:33.857] <-- textDocument/didChange
V[13:51:33.857] ASTWorker skipping Update (14) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:51:33.918] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\compile_commands.json
V[13:51:33.918] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124
I[13:51:33.918] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp version 15 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
I[13:51:33.921] --> window/workDoneProgress/create(7)
V[13:51:33.921] >>> {"id":7,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[13:51:33.921] Enqueueing 26 commands for indexing
V[13:51:33.921] <<< {"id":7,"jsonrpc":"2.0","result":null}

I[13:51:33.921] <-- reply(7)
I[13:51:33.921] --> $/progress
V[13:51:33.921] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[13:51:33.921] --> $/progress
V[13:51:33.921] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[13:51:33.943] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 1_Auto_move.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server1832620124\\sketch\\1_Auto_move.ino.cpp"
V[13:51:33.945] BackgroundIndex: building version 9 after loading index from disk
V[13:51:33.951] Reusing preamble version 9 for version 15 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
V[13:51:33.956] BackgroundIndex: serving version 9 (1772786 bytes)
I[13:51:33.968] --> $/progress
V[13:51:33.968] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[13:51:33.969] --> $/progress
V[13:51:33.969] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[13:55:40.696] <<< {"id":"60","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server1832620124/sketch/1_Auto_move.ino.cpp"}}}

I[13:55:40.696] <-- textDocument/documentSymbol("60")
V[13:55:40.700] ASTWorker running DocumentSymbols on version 15 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server1832620124\sketch\1_Auto_move.ino.cpp
I[13:55:40.700] --> reply:textDocument/documentSymbol("60") 3 ms
V[13:55:40.700] >>> {"id":"60","jsonrpc":"2.0","result":[]}

V[13:55:44.008] <<< {"id":"61","jsonrpc":"2.0","method":"shutdown","params":null}

I[13:55:44.008] <-- shutdown("61")
I[13:55:44.008] --> reply:shutdown("61") 0 ms
V[13:55:44.008] >>> {"id":"61","jsonrpc":"2.0","result":null}

