






Started logging.
I[15:25:09.679] clangd version 14.0.0
I[15:25:09.681] Features: windows
I[15:25:09.681] PID: 2212
I[15:25:09.681] Working directory: g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYC0076拍照麦克轮WiFi小车\ZYC0076\4_Arduino_Code\2_servo_Angle
I[15:25:09.681] argv[0]: d:\Program Files\Arduino IDE\resources\app\node_modules\arduino-ide-extension\build\clangd.exe
I[15:25:09.681] argv[1]: -log=verbose
I[15:25:09.681] argv[2]: --compile-commands-dir=C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482
I[15:25:09.681] argv[3]: -query-driver=C:\Users\Administrator\AppData\Local\Arduino15\packages\**
V[15:25:09.688] User config file is C:\Users\Administrator\AppData\Local\clangd\config.yaml
I[15:25:09.689] Starting LSP over stdin/stdout
V[15:25:09.689] <<< {"id":"1","jsonrpc":"2.0","method":"initialize","params":{"capabilities":{"textDocument":{"codeAction":{"codeActionLiteralSupport":{"codeActionKind":{"valueSet":["","quickfix","refactor","refactor.extract","refactor.inline","refactor.rewrite","source","source.organizeImports"]}},"dynamicRegistration":true,"isPreferredSupport":true},"codeLens":{"dynamicRegistration":true},"colorProvider":{"dynamicRegistration":true},"completion":{"completionItem":{"commitCharactersSupport":true,"deprecatedSupport":true,"documentationFormat":["markdown","plaintext"],"preselectSupport":true,"snippetSupport":true,"tagSupport":{"valueSet":[1]}},"completionItemKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25]},"contextSupport":true,"dynamicRegistration":true},"declaration":{"dynamicRegistration":true,"linkSupport":true},"definition":{"dynamicRegistration":true,"linkSupport":true},"documentHighlight":{"dynamicRegistration":true},"documentLink":{"dynamicRegistration":true,"tooltipSupport":true},"documentSymbol":{"dynamicRegistration":true,"hierarchicalDocumentSymbolSupport":true,"symbolKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26]}},"foldingRange":{"dynamicRegistration":true,"lineFoldingOnly":true,"rangeLimit":5000},"formatting":{"dynamicRegistration":true},"hover":{"contentFormat":["markdown","plaintext"],"dynamicRegistration":true},"implementation":{"dynamicRegistration":true,"linkSupport":true},"onTypeFormatting":{"dynamicRegistration":true},"publishDiagnostics":{"relatedInformation":true,"tagSupport":{"valueSet":[1,2]}},"rangeFormatting":{"dynamicRegistration":true},"references":{"dynamicRegistration":true},"rename":{"dynamicRegistration":true,"prepareSupport":true},"selectionRange":{"dynamicRegistration":true},"signatureHelp":{"contextSupport":true,"dynamicRegistration":true,"signatureInformation":{"documentationFormat":["markdown","plaintext"],"parameterInformation":{"labelOffsetSupport":true}}},"synchronization":{"didSave":true,"dynamicRegistration":true,"willSave":true,"willSaveWaitUntil":true},"typeDefinition":{"dynamicRegistration":true,"linkSupport":true}},"window":{"workDoneProgress":true},"workspace":{"applyEdit":true,"configuration":true,"didChangeConfiguration":{"dynamicRegistration":true},"didChangeWatchedFiles":{"dynamicRegistration":true},"executeCommand":{"dynamicRegistration":true},"symbol":{"dynamicRegistration":true,"symbolKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26]}},"workspaceEdit":{"documentChanges":true,"failureHandling":"textOnlyTransactional","resourceOperations":["create","rename","delete"]},"workspaceFolders":true}},"clientInfo":{"name":"vscode","version":"1.53.2"},"initializationOptions":{},"processId":3280,"rootPath":"C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch","rootUri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch","trace":"off","workspaceFolders":[{"name":"2_servo_Angle","uri":"file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYC0076%E6%8B%8D%E7%85%A7%E9%BA%A6%E5%85%8B%E8%BD%AEWiFi%E5%B0%8F%E8%BD%A6/ZYC0076/4_Arduino_Code/2_servo_Angle"}]}}

I[15:25:09.689] <-- initialize("1")
I[15:25:09.753] --> reply:initialize("1") 64 ms
V[15:25:09.753] >>> {"id":"1","jsonrpc":"2.0","result":{"capabilities":{"astProvider":true,"callHierarchyProvider":true,"clangdInlayHintsProvider":true,"codeActionProvider":{"codeActionKinds":["quickfix","refactor","info"]},"compilationDatabase":{"automaticReload":true},"completionProvider":{"allCommitCharacters":[" ","\t","(",")","[","]","{","}","<",">",":",";",",","+","-","/","*","%","^","&","#","?",".","=","\"","'","|"],"resolveProvider":false,"triggerCharacters":[".","<",">",":","\"","/","*"]},"declarationProvider":true,"definitionProvider":true,"documentFormattingProvider":true,"documentHighlightProvider":true,"documentLinkProvider":{"resolveProvider":false},"documentOnTypeFormattingProvider":{"firstTriggerCharacter":"\n","moreTriggerCharacter":[]},"documentRangeFormattingProvider":true,"documentSymbolProvider":true,"executeCommandProvider":{"commands":["clangd.applyFix","clangd.applyTweak"]},"hoverProvider":true,"implementationProvider":true,"memoryUsageProvider":true,"referencesProvider":true,"renameProvider":{"prepareProvider":true},"selectionRangeProvider":true,"semanticTokensProvider":{"full":{"delta":true},"legend":{"tokenModifiers":["declaration","deprecated","deduced","readonly","static","abstract","virtual","dependentName","defaultLibrary","usedAsMutableReference","functionScope","classScope","fileScope","globalScope"],"tokenTypes":["variable","variable","parameter","function","method","function","property","variable","class","interface","enum","enumMember","type","type","unknown","namespace","typeParameter","concept","type","macro","comment"]},"range":false},"signatureHelpProvider":{"triggerCharacters":["(",")","{","}","<",">",","]},"textDocumentSync":{"change":2,"openClose":true,"save":true},"typeDefinitionProvider":true,"typeHierarchyProvider":true,"workspaceSymbolProvider":true},"serverInfo":{"name":"clangd","version":"clangd version 14.0.0 windows x86_64-pc-windows-msvc"}}}

V[15:25:09.753] <<< {"jsonrpc":"2.0","method":"initialized","params":{}}

I[15:25:09.754] <-- initialized
V[15:25:09.760] <<< {"jsonrpc":"2.0","method":"textDocument/didOpen","params":{"textDocument":{"languageId":"cpp","text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\n#include    <Servo.h>\n\n#define servo_PIN    9\n\nServo myservo;\n\nint pos = 0;\n\n#line 9 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid setup();\n#line 15 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid loop();\n#line 9 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid setup()\n{\n    myservo.attach(servo_PIN);\n    myservo.write(90);\n}\n\nvoid loop()\n{\n    for (pos = 170; pos >= 10; pos -= 1) \n    { \n        clawservo.write(pos);    \n        delay(15);\n    } \n    for (pos = 10; pos <= 170; pos += 1) \n    { \n        clawservo.write(pos);            \n        delay(15);                     \n    }\n}\n\n","uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp","version":1}}}

I[15:25:09.760] <-- textDocument/didOpen
V[15:25:09.761] <<< {"id":"2","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:25:09.761] <-- textDocument/documentSymbol("2")
V[15:25:09.763] config note at C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\.clangd:1:0: Parsing config fragment
V[15:25:09.763] config note at C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\.clangd:1:0: Parsed 1 fragments from file
V[15:25:09.763] Config fragment: compiling C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\.clangd:1 -> 0x00000178EFC11030 (trusted=false)
I[15:25:09.764] --> textDocument/publishDiagnostics
V[15:25:09.764] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/.clangd"}}

I[15:25:09.765] Loaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\compile_commands.json
V[15:25:09.765] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482
I[15:25:09.768] --> window/workDoneProgress/create(0)
V[15:25:09.768] >>> {"id":0,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[15:25:09.768] Enqueueing 26 commands for indexing
V[15:25:09.769] <<< {"id":0,"jsonrpc":"2.0","result":null}

I[15:25:09.769] <-- reply(0)
I[15:25:09.769] --> $/progress
V[15:25:09.769] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[15:25:09.769] --> $/progress
V[15:25:09.769] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[15:25:09.770] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp
V[15:25:09.770] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp
V[15:25:09.770] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c
V[15:25:09.770] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c
V[15:25:09.770] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp
V[15:25:09.771] Failed to load shard: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
V[15:25:09.771] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp
V[15:25:09.771] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp
V[15:25:09.771] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp
V[15:25:09.771] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp
V[15:25:09.771] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp
V[15:25:09.771] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S
V[15:25:09.771] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp
V[15:25:09.771] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp
V[15:25:09.771] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp
V[15:25:09.772] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp
V[15:25:09.772] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp
V[15:25:09.772] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c
V[15:25:09.772] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp
V[15:25:09.772] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c
V[15:25:09.772] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c
V[15:25:09.772] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp
V[15:25:09.772] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp
V[15:25:09.772] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c
V[15:25:09.773] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp
V[15:25:09.773] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c
I[15:25:09.778] --> $/progress
V[15:25:09.778] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[15:25:09.778] --> $/progress
V[15:25:09.778] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[15:25:09.778] --> $/progress
V[15:25:09.778] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[15:25:09.778] --> $/progress
V[15:25:09.778] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[15:25:09.778] --> $/progress
V[15:25:09.778] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[15:25:09.778] --> $/progress
V[15:25:09.778] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[15:25:09.778] --> $/progress
V[15:25:09.778] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[15:25:09.778] --> $/progress
V[15:25:09.778] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

V[15:25:09.893] System include extraction: target extracted: "avr"
V[15:25:09.893] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[15:25:09.893] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[15:25:09.893] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[15:25:09.893] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
I[15:25:09.894] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp version 1 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" "-ID:\\Program Files\\Arduino\\libraries\\Servo\\src" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp"
V[15:25:09.898] System include extraction: target extracted: "avr"
V[15:25:09.898] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[15:25:09.898] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[15:25:09.898] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[15:25:09.898] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-gcc.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[15:25:09.900] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c (digest:=BC32CF542FD8D605)
V[15:25:09.907] System include extraction: target extracted: "avr"
V[15:25:09.907] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[15:25:09.907] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[15:25:09.907] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[15:25:09.907] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[15:25:09.908] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp (digest:=6DDB6ED4F4E34E63)
V[15:25:09.912] System include extraction: target extracted: "avr"
V[15:25:09.912] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[15:25:09.912] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[15:25:09.912] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[15:25:09.912] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[15:25:09.913] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp (digest:=F7D59D2B49112307)
V[15:25:09.923] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 2_servo_Angle.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -I "D:\\Program Files\\Arduino\\libraries\\Servo\\src" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp"
V[15:25:09.923] Building first preamble for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp version 1
V[15:25:09.926] System include extraction: target extracted: "avr"
V[15:25:09.926] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[15:25:09.926] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[15:25:09.926] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[15:25:09.926] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[15:25:09.928] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp (digest:=7D1D0E442CF15FC1)
V[15:25:09.933] System include extraction: target extracted: "avr"
V[15:25:09.933] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[15:25:09.933] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[15:25:09.933] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[15:25:09.933] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-gcc.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[15:25:09.936] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c (digest:=B0774BE9D28D49CB)
V[15:25:09.936] System include extraction: target extracted: "avr"
V[15:25:09.936] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[15:25:09.936] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[15:25:09.936] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[15:25:09.936] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[15:25:09.938] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp (digest:=E3E9F11672EDD20A)
V[15:25:10.002] indexed preamble AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp version 1:
  symbol slab: 2530 symbols, 718598 bytes
  ref slab: 0 symbols, 0 refs, 136 bytes
  relations slab: 9 relations, 177 bytes
I[15:25:10.002] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c (310 symbols, 2729 refs, 25 files)
I[15:25:10.026] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c (309 symbols, 2669 refs, 25 files)
I[15:25:10.028] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp (600 symbols, 3544 refs, 35 files)
V[15:25:10.031] Build dynamic index for header symbols with estimated memory usage of 2181510 bytes
I[15:25:10.032] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp (620 symbols, 3567 refs, 36 files)
V[15:25:10.032] Built preamble of size 432340 for file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp version 1
V[15:25:10.035] Ignored diagnostic. c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include\avr/wdt.h:464:12:value '64' out of range for constraint 'I'
V[15:25:10.035] Ignored diagnostic. c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include\avr/wdt.h:507:23:value '64' out of range for constraint 'I'
I[15:25:10.037] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp (604 symbols, 3716 refs, 38 files)
I[15:25:10.060] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp (602 symbols, 3517 refs, 37 files)
I[15:25:10.060] Failed to compile C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp, index may be incomplete
V[15:25:10.090] Trying to fix unresolved name "clawservo" in scopes: []
V[15:25:10.090] Dex query tree: false
V[15:25:10.091] Trying to fix unresolved name "clawservo" in scopes: []
V[15:25:10.092] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp version 1:
  symbol slab: 5 symbols, 5384 bytes
  ref slab: 10 symbols, 22 refs, 4544 bytes
  relations slab: 0 relations, 24 bytes
V[15:25:10.092] Build dynamic index for main-file symbols with estimated memory usage of 14352 bytes
I[15:25:10.092] --> textDocument/publishDiagnostics
V[15:25:10.092] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[{"code":"undeclared_var_use","message":"Use of undeclared identifier 'clawservo'","range":{"end":{"character":17,"line":25},"start":{"character":8,"line":25}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'clawservo'","range":{"end":{"character":17,"line":30},"start":{"character":8,"line":30}},"relatedInformation":[],"severity":1,"source":"clang"}],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp","version":1}}

V[15:25:10.092] ASTWorker running DocumentSymbols on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:25:10.092] --> reply:textDocument/documentSymbol("2") 331 ms
V[15:25:10.092] >>> {"id":"2","jsonrpc":"2.0","result":[{"detail":"Servo","kind":13,"name":"myservo","range":{"end":{"character":13,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":13,"line":6},"start":{"character":6,"line":6}}},{"detail":"int","kind":13,"name":"pos","range":{"end":{"character":11,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":7,"line":8},"start":{"character":4,"line":8}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":11},"start":{"character":0,"line":11}},"selectionRange":{"end":{"character":10,"line":11},"start":{"character":5,"line":11}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":13},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":1,"line":19},"start":{"character":0,"line":15}},"selectionRange":{"end":{"character":10,"line":15},"start":{"character":5,"line":15}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":33},"start":{"character":0,"line":21}},"selectionRange":{"end":{"character":9,"line":21},"start":{"character":5,"line":21}}}]}

I[15:25:10.562] --> $/progress
V[15:25:10.562] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"2/27","percentage":7}}}

I[15:25:10.562] --> $/progress
V[15:25:10.562] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"2/27","percentage":7}}}

V[15:25:10.564] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp (digest:=FDB5BCAAB3E73FCE)
I[15:25:10.627] --> $/progress
V[15:25:10.627] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"3/27","percentage":11}}}

I[15:25:10.627] --> $/progress
V[15:25:10.627] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"3/27","percentage":11}}}

V[15:25:10.629] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c (digest:=C16B0ED8B1C5BB9F)
I[15:25:10.648] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp (363 symbols, 3016 refs, 36 files)
I[15:25:10.657] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c (1 symbols, 1 refs, 1 files)
I[15:25:10.711] --> $/progress
V[15:25:10.711] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"4/27","percentage":14}}}

I[15:25:10.711] --> $/progress
V[15:25:10.711] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"4/27","percentage":14}}}

V[15:25:10.713] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c (digest:=5D6C1534064234DD)
I[15:25:10.786] --> $/progress
V[15:25:10.786] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"5/27","percentage":18}}}

I[15:25:10.786] --> $/progress
V[15:25:10.786] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"5/27","percentage":18}}}

V[15:25:10.788] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp (digest:=D7FFC6931C21680C)
I[15:25:10.814] --> $/progress
V[15:25:10.814] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"6/27","percentage":22}}}

I[15:25:10.814] --> $/progress
V[15:25:10.814] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"6/27","percentage":22}}}

V[15:25:10.815] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp (digest:=55BA50D4FF04E609)
I[15:25:10.827] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c (230 symbols, 2640 refs, 25 files)
V[15:25:10.860] BackgroundIndex: building version 1 after indexing enough files
V[15:25:10.870] BackgroundIndex: serving version 1 (1458658 bytes)
I[15:25:10.871] --> $/progress
V[15:25:10.871] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"7/27","percentage":25}}}

I[15:25:10.871] --> $/progress
V[15:25:10.871] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"7/27","percentage":25}}}

V[15:25:10.872] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c (digest:=343A7ACAD5FD2414)
I[15:25:10.884] --> $/progress
V[15:25:10.884] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"8/27","percentage":29}}}

I[15:25:10.884] --> $/progress
V[15:25:10.884] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"8/27","percentage":29}}}

V[15:25:10.887] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp (digest:=4A1244E54C0CAC04)
I[15:25:10.896] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp (393 symbols, 2994 refs, 37 files)
I[15:25:10.916] --> $/progress
V[15:25:10.916] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"9/27","percentage":33}}}

I[15:25:10.916] --> $/progress
V[15:25:10.916] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"9/27","percentage":33}}}

V[15:25:10.918] Indexing C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp (digest:=5D030F3B876540A2)
I[15:25:10.931] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp (544 symbols, 3306 refs, 36 files)
I[15:25:10.932] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp (42 symbols, 134 refs, 3 files)
I[15:25:10.955] --> $/progress
V[15:25:10.955] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"10/27","percentage":37}}}

I[15:25:10.955] --> $/progress
V[15:25:10.955] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"10/27","percentage":37}}}

V[15:25:10.958] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c (digest:=0A36B38756A4F148)
I[15:25:10.963] --> $/progress
V[15:25:10.963] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"11/27","percentage":40}}}

I[15:25:10.963] --> $/progress
V[15:25:10.963] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"11/27","percentage":40}}}

I[15:25:10.966] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c (308 symbols, 2892 refs, 25 files)
V[15:25:10.966] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp (digest:=293923F15565174B)
V[15:25:11.075] Ignored diagnostic. G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYC0076拍照麦克轮WiFi小车\ZYC0076\4_Arduino_Code\2_servo_Angle\2_servo_Angle.ino:19:9:use of undeclared identifier 'clawservo'
V[15:25:11.076] Ignored diagnostic. G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYC0076拍照麦克轮WiFi小车\ZYC0076\4_Arduino_Code\2_servo_Angle\2_servo_Angle.ino:24:9:use of undeclared identifier 'clawservo'
I[15:25:11.077] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp (299 symbols, 2470 refs, 18 files)
I[15:25:11.088] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c (309 symbols, 2688 refs, 25 files)
I[15:25:11.094] Indexed C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp (623 symbols, 3485 refs, 37 files)
I[15:25:11.094] Failed to compile C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp, index may be incomplete
I[15:25:11.150] --> $/progress
V[15:25:11.151] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"12/27","percentage":44}}}

I[15:25:11.151] --> $/progress
V[15:25:11.151] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"12/27","percentage":44}}}

V[15:25:11.156] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp (digest:=3DD4F70FCF8C4FA6)
I[15:25:11.210] --> $/progress
V[15:25:11.210] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"13/27","percentage":48}}}

I[15:25:11.210] --> $/progress
V[15:25:11.210] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"13/27","percentage":48}}}

V[15:25:11.212] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp (digest:=313C4893EB7ADBE6)
I[15:25:11.265] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp (600 symbols, 3461 refs, 37 files)
I[15:25:11.282] --> $/progress
V[15:25:11.282] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"14/27","percentage":51}}}

I[15:25:11.282] --> $/progress
V[15:25:11.282] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"14/27","percentage":51}}}

V[15:25:11.287] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp (digest:=81BB1157C290C33B)
I[15:25:11.312] --> $/progress
V[15:25:11.312] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"15/27","percentage":55}}}

I[15:25:11.312] --> $/progress
V[15:25:11.312] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"15/27","percentage":55}}}

V[15:25:11.314] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp (digest:=38075D39C713EC91)
I[15:25:11.355] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp (46 symbols, 139 refs, 3 files)
I[15:25:11.361] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp (602 symbols, 3436 refs, 35 files)
I[15:25:11.403] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp (600 symbols, 3583 refs, 35 files)
I[15:25:11.439] --> $/progress
V[15:25:11.439] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"16/27","percentage":59}}}

I[15:25:11.439] --> $/progress
V[15:25:11.439] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"16/27","percentage":59}}}

V[15:25:11.450] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c (digest:=5E8D23E876F6F446)
I[15:25:11.490] --> $/progress
V[15:25:11.490] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"17/27","percentage":62}}}

I[15:25:11.490] --> $/progress
V[15:25:11.490] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"17/27","percentage":62}}}

V[15:25:11.492] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp (digest:=1C31198B0754810E)
I[15:25:11.532] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c (307 symbols, 2637 refs, 25 files)
I[15:25:11.629] --> $/progress
V[15:25:11.629] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"18/27","percentage":66}}}

I[15:25:11.629] --> $/progress
V[15:25:11.629] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"18/27","percentage":66}}}

V[15:25:11.632] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp (digest:=365287FBD658A80E)
I[15:25:11.634] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp (613 symbols, 3659 refs, 35 files)
I[15:25:11.733] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp (601 symbols, 3490 refs, 37 files)
I[15:25:12.084] --> $/progress
V[15:25:12.084] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"19/27","percentage":70}}}

I[15:25:12.085] --> $/progress
V[15:25:12.085] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"19/27","percentage":70}}}

V[15:25:12.090] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp (digest:=487C94A1A1F49B6C)
I[15:25:12.150] --> $/progress
V[15:25:12.150] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"20/27","percentage":74}}}

I[15:25:12.150] --> $/progress
V[15:25:12.150] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"20/27","percentage":74}}}

I[15:25:12.150] --> $/progress
V[15:25:12.150] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"21/27","percentage":77}}}

I[15:25:12.150] --> $/progress
V[15:25:12.150] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"21/27","percentage":77}}}

V[15:25:12.153] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp (digest:=F68AA83B5BAAD75D)
I[15:25:12.192] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp (61 symbols, 201 refs, 5 files)
I[15:25:12.197] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp (600 symbols, 3461 refs, 37 files)
V[15:25:12.226] System include extraction: target extracted: "avr"
V[15:25:12.226] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[15:25:12.226] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[15:25:12.226] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[15:25:12.226] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-gcc.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[15:25:12.228] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S (digest:=87583F1C920AA889)
I[15:25:12.278] --> $/progress
V[15:25:12.278] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"22/27","percentage":81}}}

V[15:25:12.279] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:54:1:expected identifier or '('
V[15:25:12.280] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:62:23:expected identifier or '('
V[15:25:12.280] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:63:23:expected identifier or '('
V[15:25:12.280] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:64:23:expected identifier or '('
V[15:25:12.280] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:65:23:expected identifier or '('
V[15:25:12.280] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:66:23:expected identifier or '('
V[15:25:12.280] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:67:23:expected identifier or '('
V[15:25:12.280] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:72:37:expected identifier or '('
V[15:25:12.281] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:73:31:expected ';' after top level declarator
V[15:25:12.281] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:79:23:expected identifier or '('
V[15:25:12.281] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:83:32:expected identifier or '('
V[15:25:12.281] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:83:35:expected identifier or '('
V[15:25:12.281] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:84:22:unknown type name 'maxloops'
V[15:25:12.281] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:85:8:expected ';' after top level declarator
V[15:25:12.281] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:85:22:unknown type name 'maxloops'
V[15:25:12.281] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:86:8:expected ';' after top level declarator
V[15:25:12.281] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:86:22:unknown type name 'maxloops'
V[15:25:12.281] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:87:9:expected ';' after top level declarator
V[15:25:12.281] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:87:18:expected identifier or '('
V[15:25:12.281] Ignored diagnostic. too many errors emitted, stopping now
I[15:25:12.285] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S (12 symbols, 937 refs, 9 files)
I[15:25:12.285] Failed to compile C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S, index may be incomplete
I[15:25:12.292] --> $/progress
V[15:25:12.292] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"23/27","percentage":85}}}

I[15:25:12.296] --> $/progress
V[15:25:12.296] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"24/27","percentage":88}}}

I[15:25:12.440] --> $/progress
V[15:25:12.440] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"25/27","percentage":92}}}

I[15:25:12.555] --> $/progress
V[15:25:12.555] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"26/27","percentage":96}}}

V[15:25:12.608] BackgroundIndex: building version 2 when background indexer is idle
V[15:25:12.619] BackgroundIndex: serving version 2 (1799474 bytes)
I[15:25:12.620] --> $/progress
V[15:25:12.620] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[15:25:34.328] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:25:34.328] <-- textDocument/didSave
I[15:25:34.328] File version went from 1 to 1
V[15:25:34.329] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\n#include    <Servo.h>\n\n#define servo_PIN    9\n\nServo myservo;\n\nint pos = 0;\n\n#line 9 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid setup();\n#line 15 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid loop();\n#line 9 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid setup()\n{\n    myservo.attach(servo_PIN);\n    myservo.write(90);\n}\n\nvoid loop()\n{\n    for (pos = 170; pos >= 10; pos -= 1) \n    { \n        clawservo.write(pos);    \n        delay(15);\n    } \n    for (pos = 10; pos <= 170; pos += 1) \n    { \n        clawservo.write(pos);            \n        delay(15);                     \n    }\n}\n\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp","version":2}}}

I[15:25:34.329] <-- textDocument/didChange
V[15:25:34.329] ASTWorker skipping Update (1) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:25:34.396] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\compile_commands.json
V[15:25:34.396] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482
I[15:25:34.396] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp version 2 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" "-ID:\\Program Files\\Arduino\\libraries\\Servo\\src" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp"
I[15:25:34.399] --> window/workDoneProgress/create(1)
V[15:25:34.399] >>> {"id":1,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[15:25:34.399] Enqueueing 26 commands for indexing
V[15:25:34.400] <<< {"id":1,"jsonrpc":"2.0","result":null}

I[15:25:34.400] <-- reply(1)
I[15:25:34.400] --> $/progress
V[15:25:34.400] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[15:25:34.400] --> $/progress
V[15:25:34.400] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[15:25:34.422] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 2_servo_Angle.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -I "D:\\Program Files\\Arduino\\libraries\\Servo\\src" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp"
V[15:25:34.425] BackgroundIndex: building version 3 after loading index from disk
V[15:25:34.429] Reusing preamble version 1 for version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
V[15:25:34.435] BackgroundIndex: serving version 3 (1795846 bytes)
I[15:25:34.448] --> $/progress
V[15:25:34.448] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[15:25:34.448] --> $/progress
V[15:25:34.448] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[15:25:53.199] <<< {"id":"3","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":1,"line":19},"start":{"character":1,"line":19}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:25:53.199] <-- textDocument/codeAction("3")
V[15:25:53.203] ASTWorker running EnumerateTweaks on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:25:53.203] --> reply:textDocument/codeAction("3") 3 ms
V[15:25:53.203] >>> {"id":"3","jsonrpc":"2.0","result":[]}

V[15:25:55.787] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:25:55.787] <-- textDocument/didSave
I[15:25:55.787] File version went from 2 to 2
V[15:25:55.787] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\n#include    <Servo.h>\n\n#define servo_PIN    9\n\nServo myservo;\n\nint pos = 0;\n\n#line 9 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid setup();\n#line 15 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid loop();\n#line 9 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid setup()\n{\n    myservo.attach(servo_PIN);\n    myservo.write(90);\n}\n\nvoid loop()\n{\n    for (pos = 170; pos >= 10; pos -= 1) \n    { \n        clawservo.write(pos);    \n        delay(15);\n    } \n    for (pos = 10; pos <= 170; pos += 1) \n    { \n        clawservo.write(pos);            \n        delay(15);                     \n    }\n}\n\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp","version":3}}}

I[15:25:55.788] <-- textDocument/didChange
V[15:25:55.788] ASTWorker skipping Update (2) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:25:55.861] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\compile_commands.json
V[15:25:55.861] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482
I[15:25:55.861] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp version 3 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" "-ID:\\Program Files\\Arduino\\libraries\\Servo\\src" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp"
I[15:25:55.864] --> window/workDoneProgress/create(2)
V[15:25:55.864] >>> {"id":2,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[15:25:55.864] Enqueueing 26 commands for indexing
V[15:25:55.864] <<< {"id":2,"jsonrpc":"2.0","result":null}

I[15:25:55.864] <-- reply(2)
I[15:25:55.864] --> $/progress
V[15:25:55.864] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[15:25:55.864] --> $/progress
V[15:25:55.864] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[15:25:55.887] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 2_servo_Angle.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -I "D:\\Program Files\\Arduino\\libraries\\Servo\\src" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp"
V[15:25:55.890] BackgroundIndex: building version 4 after loading index from disk
V[15:25:55.894] Reusing preamble version 1 for version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
V[15:25:55.900] BackgroundIndex: serving version 4 (1795846 bytes)
I[15:25:55.913] --> $/progress
V[15:25:55.913] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[15:25:55.913] --> $/progress
V[15:25:55.913] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[15:26:12.295] <<< {"id":"4","jsonrpc":"2.0","method":"textDocument/documentHighlight","params":{"position":{"character":9,"line":17},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:12.295] <-- textDocument/documentHighlight("4")
V[15:26:12.298] ASTWorker running Highlights on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:12.298] --> reply:textDocument/documentHighlight("4") 3 ms
V[15:26:12.298] >>> {"id":"4","jsonrpc":"2.0","result":[{"kind":1,"range":{"end":{"character":13,"line":6},"start":{"character":6,"line":6}}},{"kind":1,"range":{"end":{"character":11,"line":17},"start":{"character":4,"line":17}}},{"kind":1,"range":{"end":{"character":11,"line":18},"start":{"character":4,"line":18}}}]}

V[15:26:12.720] <<< {"id":"5","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":11,"line":17},"start":{"character":4,"line":17}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:12.720] <-- textDocument/codeAction("5")
V[15:26:12.720] ASTWorker running EnumerateTweaks on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:12.720] --> reply:textDocument/codeAction("5") 0 ms
V[15:26:12.720] >>> {"id":"5","jsonrpc":"2.0","result":[]}

V[15:26:12.993] <<< {"id":"6","jsonrpc":"2.0","method":"textDocument/definition","params":{"position":{"character":9,"line":18},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:12.993] <-- textDocument/definition("6")
V[15:26:12.993] ASTWorker running Definitions on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:12.993] --> reply:textDocument/definition("6") 0 ms
V[15:26:12.993] >>> {"id":"6","jsonrpc":"2.0","result":[{"range":{"end":{"character":13,"line":6},"start":{"character":6,"line":6}},"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}]}

V[15:26:14.036] <<< {"id":"7","jsonrpc":"2.0","method":"textDocument/documentHighlight","params":{"position":{"character":12,"line":25},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:14.036] <-- textDocument/documentHighlight("7")
V[15:26:14.036] ASTWorker running Highlights on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:14.036] --> reply:textDocument/documentHighlight("7") 0 ms
V[15:26:14.036] >>> {"id":"7","jsonrpc":"2.0","result":[]}

V[15:26:14.420] <<< {"id":"8","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":17,"line":25},"start":{"character":8,"line":25}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:14.420] <-- textDocument/codeAction("8")
V[15:26:14.420] ASTWorker running EnumerateTweaks on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:14.420] --> reply:textDocument/codeAction("8") 0 ms
V[15:26:14.421] >>> {"id":"8","jsonrpc":"2.0","result":[]}

V[15:26:14.523] <<< {"id":"9","jsonrpc":"2.0","method":"textDocument/definition","params":{"position":{"character":12,"line":25},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:14.523] <-- textDocument/definition("9")
V[15:26:14.523] ASTWorker running Definitions on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:14.523] --> reply:textDocument/definition("9") 0 ms
V[15:26:14.523] >>> {"id":"9","jsonrpc":"2.0","result":[]}

V[15:26:14.725] <<< {"id":"10","jsonrpc":"2.0","method":"textDocument/definition","params":{"position":{"character":16,"line":30},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:14.725] <-- textDocument/definition("10")
V[15:26:14.725] ASTWorker running Definitions on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:14.725] --> reply:textDocument/definition("10") 0 ms
V[15:26:14.725] >>> {"id":"10","jsonrpc":"2.0","result":[]}

V[15:26:15.218] <<< {"id":"11","jsonrpc":"2.0","method":"textDocument/definition","params":{"position":{"character":16,"line":31},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:15.218] <-- textDocument/definition("11")
V[15:26:15.218] ASTWorker running Definitions on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:15.219] --> reply:textDocument/definition("11") 0 ms
V[15:26:15.219] >>> {"id":"11","jsonrpc":"2.0","result":[{"range":{"end":{"character":10,"line":105},"start":{"character":5,"line":105}},"uri":"file:///C:/Users/Administrator/AppData/Local/Arduino15/packages/arduino/hardware/avr/1.8.5/cores/arduino/wiring.c"}]}

V[15:26:15.369] <<< {"id":"12","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":16,"line":31},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:15.369] <-- textDocument/hover("12")
V[15:26:15.369] ASTWorker running Hover on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:15.373] --> reply:textDocument/hover("12") 3 ms
V[15:26:15.373] >>> {"id":"12","jsonrpc":"2.0","result":{"contents":{"kind":"markdown","value":"### function `delay`  \n\n---\n→ `void`  \nParameters:  \n- `unsigned long ms`\n\n---\n```cpp\nvoid delay(unsigned long ms)\n```"},"range":{"end":{"character":17,"line":31},"start":{"character":16,"line":31}}}}

V[15:26:15.932] <<< {"id":"13","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":16,"line":31},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:15.932] <-- textDocument/hover("13")
V[15:26:15.932] ASTWorker running Hover on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:15.935] --> reply:textDocument/hover("13") 3 ms
V[15:26:15.935] >>> {"id":"13","jsonrpc":"2.0","result":{"contents":{"kind":"markdown","value":"### function `delay`  \n\n---\n→ `void`  \nParameters:  \n- `unsigned long ms`\n\n---\n```cpp\nvoid delay(unsigned long ms)\n```"},"range":{"end":{"character":17,"line":31},"start":{"character":16,"line":31}}}}

V[15:26:16.040] <<< {"id":"14","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":17,"line":25},"start":{"character":8,"line":25}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:16.040] <-- textDocument/codeAction("14")
V[15:26:16.040] ASTWorker running EnumerateTweaks on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:16.040] --> reply:textDocument/codeAction("14") 0 ms
V[15:26:16.040] >>> {"id":"14","jsonrpc":"2.0","result":[]}

V[15:26:16.217] <<< {"id":"15","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:16.217] <-- textDocument/documentSymbol("15")
V[15:26:16.217] ASTWorker running DocumentSymbols on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:16.217] --> reply:textDocument/documentSymbol("15") 0 ms
V[15:26:16.217] >>> {"id":"15","jsonrpc":"2.0","result":[{"detail":"Servo","kind":13,"name":"myservo","range":{"end":{"character":13,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":13,"line":6},"start":{"character":6,"line":6}}},{"detail":"int","kind":13,"name":"pos","range":{"end":{"character":11,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":7,"line":8},"start":{"character":4,"line":8}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":11},"start":{"character":0,"line":11}},"selectionRange":{"end":{"character":10,"line":11},"start":{"character":5,"line":11}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":13},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":1,"line":19},"start":{"character":0,"line":15}},"selectionRange":{"end":{"character":10,"line":15},"start":{"character":5,"line":15}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":33},"start":{"character":0,"line":21}},"selectionRange":{"end":{"character":9,"line":21},"start":{"character":5,"line":21}}}]}

V[15:26:16.249] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"range":{"end":{"character":17,"line":30},"start":{"character":8,"line":30}},"text":"myservo"},{"range":{"end":{"character":17,"line":25},"start":{"character":8,"line":25}},"text":"myservo"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp","version":5}}}

I[15:26:16.249] <-- textDocument/didChange
V[15:26:16.251] <<< {"id":"16","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:16.251] <-- textDocument/documentSymbol("16")
I[15:26:16.252] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp version 5 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" "-ID:\\Program Files\\Arduino\\libraries\\Servo\\src" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp"
V[15:26:16.276] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 2_servo_Angle.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -I "D:\\Program Files\\Arduino\\libraries\\Servo\\src" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp"
V[15:26:16.284] Reusing preamble version 1 for version 5 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
V[15:26:16.301] ASTWorker rebuilding evicted AST to run DocumentSymbols: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp version 5
V[15:26:16.354] ASTWorker running DocumentSymbols on version 5 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:16.355] --> reply:textDocument/documentSymbol("16") 104 ms
V[15:26:16.355] >>> {"id":"16","jsonrpc":"2.0","result":[{"detail":"Servo","kind":13,"name":"myservo","range":{"end":{"character":13,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":13,"line":6},"start":{"character":6,"line":6}}},{"detail":"int","kind":13,"name":"pos","range":{"end":{"character":11,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":7,"line":8},"start":{"character":4,"line":8}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":11},"start":{"character":0,"line":11}},"selectionRange":{"end":{"character":10,"line":11},"start":{"character":5,"line":11}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":13},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":1,"line":19},"start":{"character":0,"line":15}},"selectionRange":{"end":{"character":10,"line":15},"start":{"character":5,"line":15}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":33},"start":{"character":0,"line":21}},"selectionRange":{"end":{"character":9,"line":21},"start":{"character":5,"line":21}}}]}

I[15:26:16.355] Skipping rebuild of the AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp, inputs are the same.
V[15:26:16.356] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp version 5:
  symbol slab: 5 symbols, 5384 bytes
  ref slab: 10 symbols, 28 refs, 4544 bytes
  relations slab: 0 relations, 24 bytes
V[15:26:16.356] Build dynamic index for main-file symbols with estimated memory usage of 14544 bytes
I[15:26:16.356] --> textDocument/publishDiagnostics
V[15:26:16.356] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp","version":5}}

V[15:26:16.463] <<< {"id":"17","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":15,"line":25},"start":{"character":15,"line":25}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:16.463] <-- textDocument/codeAction("17")
V[15:26:16.463] ASTWorker running EnumerateTweaks on version 5 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:16.463] --> reply:textDocument/codeAction("17") 0 ms
V[15:26:16.463] >>> {"id":"17","jsonrpc":"2.0","result":[]}

V[15:26:17.114] <<< {"id":"18","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":5,"line":32},"start":{"character":5,"line":32}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:17.114] <-- textDocument/codeAction("18")
V[15:26:17.114] ASTWorker running EnumerateTweaks on version 5 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:17.114] --> reply:textDocument/codeAction("18") 0 ms
V[15:26:17.114] >>> {"id":"18","jsonrpc":"2.0","result":[]}

V[15:26:20.337] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:20.337] <-- textDocument/didSave
I[15:26:20.337] File version went from 5 to 5
V[15:26:20.337] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\n#include    <Servo.h>\n\n#define servo_PIN    9\n\nServo myservo;\n\nint pos = 0;\n\n#line 9 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid setup();\n#line 15 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid loop();\n#line 9 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid setup()\n{\n    myservo.attach(servo_PIN);\n    myservo.write(90);\n}\n\nvoid loop()\n{\n    for (pos = 170; pos >= 10; pos -= 1) \n    { \n        myservo.write(pos);    \n        delay(15);\n    } \n    for (pos = 10; pos <= 170; pos += 1) \n    { \n        myservo.write(pos);            \n        delay(15);                     \n    }\n}\n\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp","version":6}}}

I[15:26:20.337] <-- textDocument/didChange
V[15:26:20.337] ASTWorker skipping Update (5) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:20.410] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp version 6 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" "-ID:\\Program Files\\Arduino\\libraries\\Servo\\src" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp"
V[15:26:20.435] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 2_servo_Angle.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -I "D:\\Program Files\\Arduino\\libraries\\Servo\\src" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp"
V[15:26:20.443] Reusing preamble version 1 for version 6 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
V[15:26:24.912] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:26:24.912] <-- textDocument/didSave
I[15:26:24.912] File version went from 6 to 6
V[15:26:24.912] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\n#include    <Servo.h>\n\n#define servo_PIN    9\n\nServo myservo;\n\nint pos = 0;\n\n#line 9 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid setup();\n#line 15 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid loop();\n#line 9 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid setup()\n{\n    myservo.attach(servo_PIN);\n    myservo.write(90);\n}\n\nvoid loop()\n{\n    for (pos = 170; pos >= 10; pos -= 1) \n    { \n        myservo.write(pos);    \n        delay(15);\n    } \n    for (pos = 10; pos <= 170; pos += 1) \n    { \n        myservo.write(pos);            \n        delay(15);                     \n    }\n}\n\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp","version":7}}}

I[15:26:24.912] <-- textDocument/didChange
V[15:26:24.912] ASTWorker skipping Update (6) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:26:24.993] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\compile_commands.json
V[15:26:24.993] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482
I[15:26:24.993] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp version 7 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" "-ID:\\Program Files\\Arduino\\libraries\\Servo\\src" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp"
I[15:26:24.998] --> window/workDoneProgress/create(3)
V[15:26:24.998] >>> {"id":3,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[15:26:24.998] Enqueueing 26 commands for indexing
V[15:26:24.998] <<< {"id":3,"jsonrpc":"2.0","result":null}

I[15:26:24.998] <-- reply(3)
I[15:26:24.998] --> $/progress
V[15:26:24.998] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[15:26:24.998] --> $/progress
V[15:26:24.998] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[15:26:25.021] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 2_servo_Angle.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -I "D:\\Program Files\\Arduino\\libraries\\Servo\\src" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp"
V[15:26:25.023] BackgroundIndex: building version 5 after loading index from disk
V[15:26:25.029] Reusing preamble version 1 for version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
V[15:26:25.034] BackgroundIndex: serving version 5 (1795846 bytes)
I[15:26:25.046] --> $/progress
V[15:26:25.046] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[15:26:25.046] --> $/progress
V[15:26:25.046] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[15:32:10.083] <<< {"id":"19","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":22,"line":25},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:32:10.083] <-- textDocument/hover("19")
V[15:32:10.086] ASTWorker running Hover on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:32:10.090] --> reply:textDocument/hover("19") 7 ms
V[15:32:10.090] >>> {"id":"19","jsonrpc":"2.0","result":{"contents":{"kind":"markdown","value":"### variable `pos`  \n\n---\nType: `int`  \nValue = `0`  \nPassed as value  \n\n---\n```cpp\nint pos = 0\n```"},"range":{"end":{"character":25,"line":25},"start":{"character":22,"line":25}}}}

V[15:32:10.721] <<< {"id":"20","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":40,"line":28},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:32:10.721] <-- textDocument/hover("20")
V[15:32:10.721] ASTWorker running Hover on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:32:10.724] --> reply:textDocument/hover("20") 3 ms
V[15:32:10.724] >>> {"id":"20","jsonrpc":"2.0","result":null}

V[15:32:14.510] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:32:14.510] <-- textDocument/didSave
I[15:32:14.510] File version went from 7 to 7
V[15:32:14.510] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\n#include    <Servo.h>\n\n#define servo_PIN    9\n\nServo myservo;\n\nint pos = 0;\n\n#line 9 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid setup();\n#line 15 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid loop();\n#line 9 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYC0076拍照麦克轮WiFi小车\\\\ZYC0076\\\\4_Arduino_Code\\\\2_servo_Angle\\\\2_servo_Angle.ino\"\nvoid setup()\n{\n    myservo.attach(servo_PIN);\n    myservo.write(90);\n}\n\nvoid loop()\n{\n    for (pos = 170; pos >= 10; pos -= 1) \n    { \n        myservo.write(pos);    \n        delay(15);\n    } \n    for (pos = 10; pos <= 170; pos += 1) \n    { \n        myservo.write(pos);            \n        delay(15);                     \n    }\n}\n\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp","version":8}}}

I[15:32:14.510] <-- textDocument/didChange
V[15:32:14.510] ASTWorker skipping Update (7) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:32:14.576] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\compile_commands.json
V[15:32:14.576] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482
I[15:32:14.576] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp version 8 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" "-ID:\\Program Files\\Arduino\\libraries\\Servo\\src" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp"
I[15:32:14.580] --> window/workDoneProgress/create(4)
V[15:32:14.580] >>> {"id":4,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[15:32:14.580] Enqueueing 26 commands for indexing
V[15:32:14.580] <<< {"id":4,"jsonrpc":"2.0","result":null}

I[15:32:14.580] <-- reply(4)
I[15:32:14.580] --> $/progress
V[15:32:14.580] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[15:32:14.580] --> $/progress
V[15:32:14.580] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[15:32:14.603] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 2_servo_Angle.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -I "D:\\Program Files\\Arduino\\libraries\\Servo\\src" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server812076482\\sketch\\2_servo_Angle.ino.cpp"
V[15:32:14.606] BackgroundIndex: building version 6 after loading index from disk
V[15:32:14.610] Reusing preamble version 1 for version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
V[15:32:14.616] BackgroundIndex: serving version 6 (1795846 bytes)
I[15:32:14.630] --> $/progress
V[15:32:14.630] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[15:32:14.630] --> $/progress
V[15:32:14.630] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[15:32:39.725] <<< {"id":"21","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":6,"line":25},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:32:39.725] <-- textDocument/hover("21")
V[15:32:39.728] ASTWorker running Hover on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:32:39.731] --> reply:textDocument/hover("21") 6 ms
V[15:32:39.731] >>> {"id":"21","jsonrpc":"2.0","result":null}

V[15:32:41.632] <<< {"id":"22","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":11,"line":21},"start":{"character":11,"line":21}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:32:41.632] <-- textDocument/codeAction("22")
V[15:32:41.632] ASTWorker running EnumerateTweaks on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:32:41.633] --> reply:textDocument/codeAction("22") 0 ms
V[15:32:41.633] >>> {"id":"22","jsonrpc":"2.0","result":[]}

V[15:32:45.925] <<< {"id":"23","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":12,"line":23},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:32:45.925] <-- textDocument/hover("23")
V[15:32:45.929] ASTWorker running Hover on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:32:45.932] --> reply:textDocument/hover("23") 6 ms
V[15:32:45.932] >>> {"id":"23","jsonrpc":"2.0","result":{"contents":{"kind":"markdown","value":"### variable `pos`  \n\n---\nType: `int`  \nValue = `0`  \n\n---\n```cpp\nint pos = 0\n```"},"range":{"end":{"character":12,"line":23},"start":{"character":9,"line":23}}}}

V[15:33:01.931] <<< {"id":"24","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":22,"line":18},"start":{"character":0,"line":17}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:33:01.931] <-- textDocument/codeAction("24")
V[15:33:01.935] ASTWorker running EnumerateTweaks on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:33:01.935] --> reply:textDocument/codeAction("24") 3 ms
V[15:33:01.935] >>> {"id":"24","jsonrpc":"2.0","result":[{"command":{"arguments":[{"file":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp","selection":{"end":{"character":22,"line":18},"start":{"character":0,"line":17}},"tweakID":"ExtractFunction"}],"command":"clangd.applyTweak","title":"Extract to function"},"kind":"refactor","title":"Extract to function"}]}

V[15:33:04.770] <<< {"id":"25","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":1,"line":19},"start":{"character":1,"line":19}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:33:04.770] <-- textDocument/codeAction("25")
V[15:33:04.770] ASTWorker running EnumerateTweaks on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:33:04.770] --> reply:textDocument/codeAction("25") 0 ms
V[15:33:04.770] >>> {"id":"25","jsonrpc":"2.0","result":[]}

V[15:33:05.559] <<< {"id":"26","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":1,"line":19},"start":{"character":0,"line":15}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:33:05.559] <-- textDocument/codeAction("26")
V[15:33:05.559] ASTWorker running EnumerateTweaks on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:33:05.559] --> reply:textDocument/codeAction("26") 0 ms
V[15:33:05.559] >>> {"id":"26","jsonrpc":"2.0","result":[]}

V[15:33:10.718] <<< {"id":"27","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":22,"line":18},"start":{"character":22,"line":18}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:33:10.718] <-- textDocument/codeAction("27")
V[15:33:10.722] ASTWorker running EnumerateTweaks on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:33:10.722] --> reply:textDocument/codeAction("27") 3 ms
V[15:33:10.722] >>> {"id":"27","jsonrpc":"2.0","result":[]}

V[15:33:13.533] <<< {"id":"28","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":12,"line":25},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:33:13.533] <-- textDocument/hover("28")
V[15:33:13.533] ASTWorker running Hover on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:33:13.536] --> reply:textDocument/hover("28") 3 ms
V[15:33:13.536] >>> {"id":"28","jsonrpc":"2.0","result":{"contents":{"kind":"markdown","value":"### variable `myservo`  \n\n---\nType: `class Servo`  \n\n---\n```cpp\nServo myservo\n```"},"range":{"end":{"character":15,"line":25},"start":{"character":8,"line":25}}}}

V[15:33:35.535] <<< {"id":"29","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":39,"line":30},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:33:35.536] <-- textDocument/hover("29")
V[15:33:35.539] ASTWorker running Hover on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:33:35.542] --> reply:textDocument/hover("29") 6 ms
V[15:33:35.542] >>> {"id":"29","jsonrpc":"2.0","result":null}

V[15:33:35.893] <<< {"id":"30","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":39,"line":30},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:33:35.893] <-- textDocument/hover("30")
V[15:33:35.893] ASTWorker running Hover on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:33:35.896] --> reply:textDocument/hover("30") 3 ms
V[15:33:35.896] >>> {"id":"30","jsonrpc":"2.0","result":null}

V[15:33:36.295] <<< {"id":"31","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":37,"line":30},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:33:36.295] <-- textDocument/hover("31")
V[15:33:36.295] ASTWorker running Hover on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:33:36.298] --> reply:textDocument/hover("31") 3 ms
V[15:33:36.298] >>> {"id":"31","jsonrpc":"2.0","result":null}

V[15:33:39.508] <<< {"id":"32","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":19,"line":31},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:33:39.508] <-- textDocument/hover("32")
V[15:33:39.509] ASTWorker running Hover on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:33:39.512] --> reply:textDocument/hover("32") 3 ms
V[15:33:39.512] >>> {"id":"32","jsonrpc":"2.0","result":null}

V[15:33:41.143] <<< {"id":"33","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":1,"line":33},"start":{"character":0,"line":22}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:33:41.143] <-- textDocument/codeAction("33")
V[15:33:41.147] ASTWorker running EnumerateTweaks on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:33:41.147] --> reply:textDocument/codeAction("33") 3 ms
V[15:33:41.147] >>> {"id":"33","jsonrpc":"2.0","result":[]}

V[15:33:41.616] <<< {"id":"34","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":1,"line":33},"start":{"character":0,"line":21}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server812076482/sketch/2_servo_Angle.ino.cpp"}}}

I[15:33:41.616] <-- textDocument/codeAction("34")
V[15:33:41.616] ASTWorker running EnumerateTweaks on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server812076482\sketch\2_servo_Angle.ino.cpp
I[15:33:41.616] --> reply:textDocument/codeAction("34") 0 ms
V[15:33:41.616] >>> {"id":"34","jsonrpc":"2.0","result":[]}

V[16:46:58.023] <<< {"id":"35","jsonrpc":"2.0","method":"shutdown","params":null}

I[16:46:58.024] <-- shutdown("35")
I[16:46:58.024] --> reply:shutdown("35") 0 ms
V[16:46:58.024] >>> {"id":"35","jsonrpc":"2.0","result":null}

