






Started logging.
10:09:49.839712 Language server launched with arguments:
10:09:49.839712   arg[0] = d:\Program Files\Arduino IDE\resources\app\node_modules\arduino-ide-extension\build\arduino-language-server.exe
10:09:49.839712   arg[1] = -clangd
10:09:49.839712   arg[2] = d:\Program Files\Arduino IDE\resources\app\node_modules\arduino-ide-extension\build\clangd.exe
10:09:49.839712   arg[3] = -cli-daemon-addr
10:09:49.839712   arg[4] = localhost:57938
10:09:49.839712   arg[5] = -cli-daemon-instance
10:09:49.839712   arg[6] = 1
10:09:49.839712   arg[7] = -fqbn
10:09:49.839712   arg[8] = arduino:avr:uno
10:09:50.168439   arg[9] = -skip-libraries-discovery-on-rebuild
10:09:49.850788 listen tcp 127.0.0.1:6060: bind: Only one usage of each socket address (protocol/network address/port) is normally permitted.
10:09:50.168673   arg[10] = -board-name
10:09:50.168796   arg[11] = "Arduino Uno"
10:09:50.168796   arg[12] = -no-real-time-diagnostics
10:09:50.168852   arg[13] = -log
10:09:50.168852   arg[14] = -logpath
10:09:50.168852   arg[15] = g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer
10:09:50.169196 logging to g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\inols.log
10:09:50.174998 LS: : Initial board configuration: arduino:avr:uno
10:09:50.174998 LS: : Language server build path: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897
10:09:50.174998 LS: : Language server build sketch root: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch
10:09:50.174998 LS: : Language server FULL build path: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server323791891
10:09:50.175507 IN Elapsed: 508.7µs
10:09:50.175507 IDE --> LS REQU initialize 0
10:09:50.176015                 initialize 0: write-locked
10:09:50.177032                 initialize 0: write-unlocked
10:09:50.177032 INIT --- : initializing workbench: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer
10:09:50.177032 INIT --- : read-locked
10:09:50.177032 INIT --- : read-unlocked
10:09:50.177564                 initialize 0: initialization parameters: {"capabilities":{"textDocumentSync":{"openClose":true,"change":2,"save":{"includeText":true}},"completionProvider":{"triggerCharacters":[".","\u003c","\u003e",":","\"","/"],"allCommitCharacters":[" ","\t","(",")","[","]","{","}","\u003c","\u003e",":",";",",","+","-","/","*","%","^","\u0026","#","?",".","=","\"","'","|"],"completionItem":{}},"hoverProvider":{},"signatureHelpProvider":{"triggerCharacters":["(",","]},"definitionProvider":{},"documentHighlightProvider":{},"documentSymbolProvider":{},"codeActionProvider":{"codeActionKinds":["quickfix","refactor","info"]},"documentFormattingProvider":{},"documentRangeFormattingProvider":{},"documentOnTypeFormattingProvider":{"firstTriggerCharacter":"\n"},"renameProvider":{},"executeCommandProvider":{"commands":["clangd.applyFix","clangd.applyTweak"]},"workspaceSymbolProvider":{}},"serverInfo":{"name":"arduino-language-server","version":"0.7.1"}}
10:09:50.177564 IDE <-- LS RESP initialize 0
10:09:50.177564 OUT Elapsed: 0s
10:09:50.182196 IN Elapsed: 4.6323ms
10:09:50.182196 IDE --> LS NOTIF initialized
10:09:50.182196                  initialized: Notification is not propagated to clangd
10:09:50.182196 IN Elapsed: 0s
10:09:50.182196 IDE --> LS NOTIF textDocument/didOpen
10:09:50.182196                  textDocument/didOpen: write-locked
10:09:50.182196                  textDocument/didOpen: (throttled: waiting for clangd)
10:09:50.182196                  textDocument/didOpen: unlocked (waiting clangd)
10:09:50.484156 INIT --- : Running build with: {
  "instance": {
    "id": 1
  },
  "fqbn": "arduino:avr:uno",
  "sketch_path": "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣器等等传感器\\Code\\Lesson 6_Passive_Buzzer\\6_Passive_Buzzer",
  "build_path": "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server323791891",
  "verbose": true,
  "create_compilation_database_only": true
}
10:09:52.897710 INIT --- : Compile successful!
10:09:52.901349 INIT --- : Updated 'libraries.cache'. Copied: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server323791891\libraries.cache to C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\libraries.cache
10:09:52.901349 INIT --- : read-locked
10:09:52.901349 INIT --- : read-unlocked
10:09:53.209669 INIT --- : Running build with: {
  "instance": {
    "id": 1
  },
  "fqbn": "arduino:avr:uno",
  "sketch_path": "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣器等等传感器\\Code\\Lesson 6_Passive_Buzzer\\6_Passive_Buzzer",
  "build_path": "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server3760075897",
  "verbose": true,
  "create_compilation_database_only": true,
  "skip_libraries_discovery": true
}
10:09:53.535855 INIT --- : Compile successful!
10:09:53.879793 INIT --- : Arduino Data Dir -> c:\Users\Administrator\AppData\Local\Arduino15
10:09:53.882044 INIT --- :     Starting clangd: d:\Program Files\Arduino IDE\resources\app\node_modules\arduino-ide-extension\build\clangd.exe -log=verbose --compile-commands-dir=C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897 -query-driver=C:\Users\Administrator\AppData\Local\Arduino15\packages\**
10:09:53.926200 logging to g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\inols-clangd.log
10:09:53.926768 logging to g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\inols-clangd-err.log
10:09:53.926768 IDE     LS --> Clangd REQU initialize 1
10:09:53.928424 OUT Elapsed: 1.152ms
10:09:54.007789 IN Elapsed: 79.5181ms
10:09:54.007827 IDE     LS <-- Clangd RESP initialize 1
10:09:54.007827 INIT --- : clangd successfully started: {"capabilities":{"textDocumentSync":{"openClose":true,"change":2,"save":{}},"completionProvider":{"triggerCharacters":[".","\u003c","\u003e",":","\"","/","*"],"allCommitCharacters":[" ","\t","(",")","[","]","{","}","\u003c","\u003e",":",";",",","+","-","/","*","%","^","\u0026","#","?",".","=","\"","'","|"]},"hoverProvider":{},"signatureHelpProvider":{"triggerCharacters":["(",")","{","}","\u003c","\u003e",","]},"declarationProvider":{},"definitionProvider":{},"typeDefinitionProvider":{},"implementationProvider":{},"referencesProvider":{},"documentHighlightProvider":{},"documentSymbolProvider":{},"codeActionProvider":{"codeActionKinds":["quickfix","refactor","info"]},"documentLinkProvider":{},"documentFormattingProvider":{},"documentRangeFormattingProvider":{},"documentOnTypeFormattingProvider":{"firstTriggerCharacter":"\n"},"renameProvider":{"prepareProvider":true},"executeCommandProvider":{"commands":["clangd.applyFix","clangd.applyTweak"]},"selectionRangeProvider":{},"callHierarchyProvider":{},"semanticTokensProvider":{"legend":{"tokenTypes":["variable","variable","parameter","function","method","function","property","variable","class","interface","enum","enumMember","type","type","unknown","namespace","typeParameter","concept","type","macro","comment"],"tokenModifiers":["declaration","deprecated","deduced","readonly","static","abstract","virtual","dependentName","defaultLibrary","usedAsMutableReference","functionScope","classScope","fileScope","globalScope"]},"range":false,"full":{"delta":true}},"workspaceSymbolProvider":{}},"serverInfo":{"name":"clangd","version":"clangd version 14.0.0 windows x86_64-pc-windows-msvc"}}
10:09:54.007827 IDE     LS --> Clangd NOTIF initialized
10:09:54.007827 OUT Elapsed: 0s
10:09:54.007827 INIT --- : Done initializing workbench
10:09:54.007827                  textDocument/didOpen: locked (waiting clangd)
10:09:54.008882                  textDocument/didOpen: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp
10:09:54.012972                  textDocument/didOpen: Increasing .ino tracked files count to 1
10:09:54.014525 IDE     LS --> Clangd NOTIF textDocument/didOpen
10:09:54.014525 OUT Elapsed: 0s
10:09:54.014525                  textDocument/didOpen: write-unlocked
10:09:54.014525 IN Elapsed: 0s
10:09:54.014525 IDE --> LS REQU textDocument/codeAction 1
10:09:54.015027                 textDocument/codeAction 1: read-locked
10:09:54.015073                 textDocument/codeAction 1: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino:14:14)
10:09:54.016162                 textDocument/codeAction 1: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp
10:09:54.019406 IN Elapsed: 11.5791ms
10:09:54.019406 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
10:09:54.019406                             textDocument/publishDiagnostics: Ignored by configuration
10:09:54.020458                 textDocument/codeAction 1:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp:14:14)
10:09:54.020458 IDE     LS --> Clangd REQU textDocument/codeAction 2
10:09:54.020458 OUT Elapsed: 0s
10:09:54.023768 IN Elapsed: 4.3616ms
10:09:54.023768 IDE     LS <-- Clangd REQU window/workDoneProgress/create 0
10:09:54.023768 IDE     LS --> Clangd RESP window/workDoneProgress/create 0
10:09:54.023768 IDE <-- LS REQU window/workDoneProgress/create 1
10:09:54.023768 OUT Elapsed: 0s
10:09:54.023768 OUT Elapsed: 0s
10:09:54.023768 IN Elapsed: 0s
10:09:54.023768 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.023768                             $/progress: backgroundIndexProgress BEGIN indexing, 0.0%
10:09:54.024270 IN Elapsed: 0s
10:09:54.024287 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.024287                             $/progress: backgroundIndexProgress REPORT, 0/1, 0.0%
10:09:54.031385 IN Elapsed: 7.0983ms
10:09:54.031385 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.031385                             $/progress: backgroundIndexProgress REPORT, 0/27, 0.0%
10:09:54.031385 IN Elapsed: 0s
10:09:54.031385 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.031385                             $/progress: backgroundIndexProgress REPORT, 0/27, 0.0%
10:09:54.032383 IN Elapsed: 0s
10:09:54.032383 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.032383                             $/progress: backgroundIndexProgress REPORT, 0/27, 0.0%
10:09:54.032383 IN Elapsed: 0s
10:09:54.032383 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.032383                             $/progress: backgroundIndexProgress REPORT, 0/27, 0.0%
10:09:54.032383 IN Elapsed: 0s
10:09:54.032383 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.032383                             $/progress: backgroundIndexProgress REPORT, 0/27, 0.0%
10:09:54.032383 IN Elapsed: 0s
10:09:54.032383 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.032383                             $/progress: backgroundIndexProgress REPORT, 0/27, 0.0%
10:09:54.032383 IN Elapsed: 0s
10:09:54.032383 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.032383                             $/progress: backgroundIndexProgress REPORT, 1/27, 3.0%
10:09:54.032383 IN Elapsed: 0s
10:09:54.032383 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.032383                             $/progress: backgroundIndexProgress REPORT, 1/27, 3.0%
10:09:54.272863 IN Elapsed: 240.4796ms
10:09:54.272863 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.272863                             $/progress: backgroundIndexProgress REPORT, 2/27, 7.0%
10:09:54.272863 IN Elapsed: 0s
10:09:54.272863 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.272863                             $/progress: backgroundIndexProgress REPORT, 2/27, 7.0%
10:09:54.369847 IN Elapsed: 96.9841ms
10:09:54.370419 IDE     LS <-- Clangd NOTIF textDocument/publishDiagnostics
10:09:54.370419 IN Elapsed: 0s
10:09:54.370419                             textDocument/publishDiagnostics: Ignored by configuration
10:09:54.370934 IDE     LS <-- Clangd RESP textDocument/codeAction 2
10:09:54.370934                 textDocument/codeAction 1: read-unlocked
10:09:54.370934 IDE <-- LS RESP textDocument/codeAction 1
10:09:54.370934 OUT Elapsed: 0s
10:09:54.370934 IN Elapsed: 0s
10:09:54.370934 IDE --> LS REQU textDocument/documentSymbol 2
10:09:54.370934                 textDocument/documentSymbol 2: read-locked
10:09:54.372490                 textDocument/documentSymbol 2: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp
10:09:54.372490 IDE     LS --> Clangd REQU textDocument/documentSymbol 3
10:09:54.372490 OUT Elapsed: 0s
10:09:54.373004 IN Elapsed: 2.5855ms
10:09:54.373004 IDE     LS <-- Clangd RESP textDocument/documentSymbol 3
10:09:54.373004                 textDocument/documentSymbol 2: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp (4 document symbols)
10:09:54.373004                 textDocument/documentSymbol 2:   > convert SymbolKind:Function 3:0-3:12
10:09:54.375641                 textDocument/documentSymbol 2: Range is in PREPROCESSED section of the sketch
10:09:54.375641                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp:3:0-3:12 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino:0:0-0:12 (.ino)
10:09:54.375641                 textDocument/documentSymbol 2:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
10:09:54.375641                 textDocument/documentSymbol 2:   > convert SymbolKind:Function 5:0-5:11
10:09:54.376154 IN Elapsed: 3.1497ms
10:09:54.376154 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.376154                             $/progress: backgroundIndexProgress REPORT, 3/27, 11.0%
10:09:54.376154 IN Elapsed: 0s
10:09:54.376154 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.376154                             $/progress: backgroundIndexProgress REPORT, 3/27, 11.0%
10:09:54.377176                 textDocument/documentSymbol 2: Range is in PREPROCESSED section of the sketch
10:09:54.377176                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp:5:0-5:11 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino:3:0-3:11 (.ino)
10:09:54.377176                 textDocument/documentSymbol 2:     symbol is in the preprocessed section of the sketch.ino.cpp, skipping
10:09:54.377176                 textDocument/documentSymbol 2:   > convert SymbolKind:Function 7:0-9:1
10:09:54.378778                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp:7:0-9:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino:0:0-2:1 (.ino)
10:09:54.380840                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp:7:5-7:10 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino:0:5-0:10 (.ino)
10:09:54.380840                 textDocument/documentSymbol 2: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp (0 document symbols)
10:09:54.380840                 textDocument/documentSymbol 2:   > convert SymbolKind:Function 10:0-23:1
10:09:54.382376                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp:10:0-23:1 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino:3:0-16:1 (.ino)
10:09:54.383908                 textDocument/documentSymbol 2: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp:10:5-10:9 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino:3:5-3:9 (.ino)
10:09:54.383908                 textDocument/documentSymbol 2: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp (0 document symbols)
10:09:54.383908                 textDocument/documentSymbol 2: read-unlocked
10:09:54.384449 IDE <-- LS RESP textDocument/documentSymbol 2
10:09:54.384449 OUT Elapsed: 0s
10:09:54.384449 IN Elapsed: 0s
10:09:54.384449 IN Elapsed: 0s
10:09:54.384449 IDE --> LS NOTIF ino/didCompleteBuild
10:09:54.384449                  ino/didCompleteBuild: write-locked
10:09:54.384449 IDE --> LS RESP window/workDoneProgress/create 1
10:09:54.384961 IDE <-- LS NOTIF $/progress
10:09:54.384961 OUT Elapsed: 0s
10:09:54.384961 IDE <-- LS NOTIF $/progress
10:09:54.384961 OUT Elapsed: 0s
10:09:54.388580                  ino/didCompleteBuild: Updated 'libraries.cache'. Copied: C:\Users\Administrator\AppData\Local\Temp\arduino-sketch-B7D75423FE3B2E58A952023D0891E8C4\libraries.cache to C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\libraries.cache
10:09:54.388580                  ino/didCompleteBuild: write-unlocked
10:09:54.561092 IN Elapsed: 184.9383ms
10:09:54.561749 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.562273                             $/progress: backgroundIndexProgress REPORT, 4/27, 14.0%
10:09:54.562273 IN Elapsed: 0s
10:09:54.562273 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.562273                             $/progress: backgroundIndexProgress REPORT, 4/27, 14.0%
10:09:54.562273 IDE <-- LS NOTIF $/progress
10:09:54.562810 OUT Elapsed: 0s
10:09:54.562810 IDE <-- LS NOTIF $/progress
10:09:54.562810 OUT Elapsed: 0s
10:09:54.892118 IN Elapsed: 329.3078ms
10:09:54.892118 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.892118                             $/progress: backgroundIndexProgress REPORT, 5/27, 18.0%
10:09:54.892118 IDE <-- LS NOTIF $/progress
10:09:54.892118 OUT Elapsed: 0s
10:09:54.892118 IN Elapsed: 0s
10:09:54.892118 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.892118                             $/progress: backgroundIndexProgress REPORT, 5/27, 18.0%
10:09:54.892632 IDE <-- LS NOTIF $/progress
10:09:54.892632 OUT Elapsed: 0s
10:09:54.921931 IN Elapsed: 29.299ms
10:09:54.921931 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.921931                             $/progress: backgroundIndexProgress REPORT, 6/27, 22.0%
10:09:54.921931 IN Elapsed: 0s
10:09:54.921931 IDE <-- LS NOTIF $/progress
10:09:54.921931 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.921931                             $/progress: backgroundIndexProgress REPORT, 6/27, 22.0%
10:09:54.921931 OUT Elapsed: 0s
10:09:54.921931 IDE <-- LS NOTIF $/progress
10:09:54.921931 OUT Elapsed: 0s
10:09:54.962468 IN Elapsed: 40.5361ms
10:09:54.962468 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.962468                             $/progress: backgroundIndexProgress REPORT, 7/27, 25.0%
10:09:54.962468 IN Elapsed: 0s
10:09:54.962468 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.962468                             $/progress: backgroundIndexProgress REPORT, 7/27, 25.0%
10:09:54.962468 IDE <-- LS NOTIF $/progress
10:09:54.962970 OUT Elapsed: 502.7µs
10:09:54.962979 IDE <-- LS NOTIF $/progress
10:09:54.962979 OUT Elapsed: 0s
10:09:54.976117 IN Elapsed: 13.1383ms
10:09:54.976620 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.976629                             $/progress: backgroundIndexProgress REPORT, 8/27, 29.0%
10:09:54.976629 IN Elapsed: 0s
10:09:54.976629 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.976629                             $/progress: backgroundIndexProgress REPORT, 8/27, 29.0%
10:09:54.976629 IDE <-- LS NOTIF $/progress
10:09:54.976629 OUT Elapsed: 0s
10:09:54.976629 IN Elapsed: 0s
10:09:54.976629 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.976629                             $/progress: backgroundIndexProgress REPORT, 9/27, 33.0%
10:09:54.976629 IN Elapsed: 0s
10:09:54.976629 IDE     LS <-- Clangd NOTIF $/progress
10:09:54.977142                             $/progress: backgroundIndexProgress REPORT, 9/27, 33.0%
10:09:54.977142 IDE <-- LS NOTIF $/progress
10:09:54.977142 OUT Elapsed: 0s
10:09:54.977142 IDE <-- LS NOTIF $/progress
10:09:54.978869 OUT Elapsed: 1.7274ms
10:09:55.020888 IN Elapsed: 43.7462ms
10:09:55.020888 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.020888                             $/progress: backgroundIndexProgress REPORT, 10/27, 37.0%
10:09:55.020888 IN Elapsed: 0s
10:09:55.020888 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.021407                             $/progress: backgroundIndexProgress REPORT, 10/27, 37.0%
10:09:55.020888 IDE <-- LS NOTIF $/progress
10:09:55.021407 OUT Elapsed: 0s
10:09:55.021407 IDE <-- LS NOTIF $/progress
10:09:55.021407 OUT Elapsed: 0s
10:09:55.073092 IN Elapsed: 51.6857ms
10:09:55.073605 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.073605                             $/progress: backgroundIndexProgress REPORT, 11/27, 40.0%
10:09:55.073605 IN Elapsed: 0s
10:09:55.073605 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.073605                             $/progress: backgroundIndexProgress REPORT, 11/27, 40.0%
10:09:55.073605 IDE <-- LS NOTIF $/progress
10:09:55.073605 OUT Elapsed: 0s
10:09:55.073605 IDE <-- LS NOTIF $/progress
10:09:55.073605 OUT Elapsed: 0s
10:09:55.081328 IN Elapsed: 7.7235ms
10:09:55.081328 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.081328                             $/progress: backgroundIndexProgress REPORT, 12/27, 44.0%
10:09:55.081328 IDE <-- LS NOTIF $/progress
10:09:55.081328 IN Elapsed: 0s
10:09:55.081840 OUT Elapsed: 0s
10:09:55.081840 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.081840                             $/progress: backgroundIndexProgress REPORT, 12/27, 44.0%
10:09:55.081840 IDE <-- LS NOTIF $/progress
10:09:55.081840 OUT Elapsed: 0s
10:09:55.121880 IN Elapsed: 40.0407ms
10:09:55.121880 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.121880                             $/progress: backgroundIndexProgress REPORT, 13/27, 48.0%
10:09:55.121880 IN Elapsed: 0s
10:09:55.121880 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.121880                             $/progress: backgroundIndexProgress REPORT, 13/27, 48.0%
10:09:55.121880 IDE <-- LS NOTIF $/progress
10:09:55.121880 OUT Elapsed: 0s
10:09:55.128993 IN Elapsed: 7.1131ms
10:09:55.128993 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.128993                             $/progress: backgroundIndexProgress REPORT, 14/27, 51.0%
10:09:55.128993 IN Elapsed: 0s
10:09:55.128993 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.128993                             $/progress: backgroundIndexProgress REPORT, 14/27, 51.0%
10:09:55.128993 IDE <-- LS NOTIF $/progress
10:09:55.128993 OUT Elapsed: 0s
10:09:55.128993 IDE <-- LS NOTIF $/progress
10:09:55.128993 OUT Elapsed: 0s
10:09:55.130059 IN Elapsed: 1.0658ms
10:09:55.130059 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.130573                             $/progress: backgroundIndexProgress REPORT, 15/27, 55.0%
10:09:55.130573 IN Elapsed: 0s
10:09:55.130573 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.130573                             $/progress: backgroundIndexProgress REPORT, 15/27, 55.0%
10:09:55.130573 IDE <-- LS NOTIF $/progress
10:09:55.130573 OUT Elapsed: 0s
10:09:55.130573 IDE <-- LS NOTIF $/progress
10:09:55.130573 OUT Elapsed: 0s
10:09:55.135916 IN Elapsed: 5.3425ms
10:09:55.135916 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.135916                             $/progress: backgroundIndexProgress REPORT, 16/27, 59.0%
10:09:55.135916 IN Elapsed: 0s
10:09:55.136427 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.136427                             $/progress: backgroundIndexProgress REPORT, 16/27, 59.0%
10:09:55.136427 IDE <-- LS NOTIF $/progress
10:09:55.137457 OUT Elapsed: 1.0302ms
10:09:55.232489 IN Elapsed: 96.0619ms
10:09:55.232489 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.232489                             $/progress: backgroundIndexProgress REPORT, 17/27, 62.0%
10:09:55.232489 IN Elapsed: 0s
10:09:55.232489 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.232489 IDE <-- LS NOTIF $/progress
10:09:55.232489 OUT Elapsed: 0s
10:09:55.232489                             $/progress: backgroundIndexProgress REPORT, 17/27, 62.0%
10:09:55.232489 IDE <-- LS NOTIF $/progress
10:09:55.233001 OUT Elapsed: 512.4µs
10:09:55.241222 IN Elapsed: 8.7329ms
10:09:55.241725 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.241974                             $/progress: backgroundIndexProgress REPORT, 18/27, 66.0%
10:09:55.241974 IN Elapsed: 0s
10:09:55.242512 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.242512                             $/progress: backgroundIndexProgress REPORT, 18/27, 66.0%
10:09:55.242512 IDE <-- LS NOTIF $/progress
10:09:55.243028 OUT Elapsed: 515.6µs
10:09:55.256100 IN Elapsed: 13.5878ms
10:09:55.256100 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.256100                             $/progress: backgroundIndexProgress REPORT, 19/27, 70.0%
10:09:55.256100 IN Elapsed: 0s
10:09:55.256100 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.256100                             $/progress: backgroundIndexProgress REPORT, 19/27, 70.0%
10:09:55.256100 IDE <-- LS NOTIF $/progress
10:09:55.256100 OUT Elapsed: 0s
10:09:55.256100 IDE <-- LS NOTIF $/progress
10:09:55.256614 OUT Elapsed: 0s
10:09:55.258896 IN Elapsed: 2.796ms
10:09:55.258896 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.258896                             $/progress: backgroundIndexProgress REPORT, 20/27, 74.0%
10:09:55.258896 IN Elapsed: 0s
10:09:55.258896 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.258896                             $/progress: backgroundIndexProgress REPORT, 20/27, 74.0%
10:09:55.258896 IDE <-- LS NOTIF $/progress
10:09:55.259407 OUT Elapsed: 510.5µs
10:09:55.259407 IDE <-- LS NOTIF $/progress
10:09:55.259407 OUT Elapsed: 0s
10:09:55.262993 IN Elapsed: 3.5868ms
10:09:55.262993 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.262993                             $/progress: backgroundIndexProgress REPORT, 21/27, 77.0%
10:09:55.262993 IN Elapsed: 0s
10:09:55.262993 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.262993                             $/progress: backgroundIndexProgress REPORT, 21/27, 77.0%
10:09:55.262993 IDE <-- LS NOTIF $/progress
10:09:55.262993 OUT Elapsed: 0s
10:09:55.263506 IDE <-- LS NOTIF $/progress
10:09:55.263506 OUT Elapsed: 0s
10:09:55.293207 IN Elapsed: 29.7005ms
10:09:55.293207 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.293207                             $/progress: backgroundIndexProgress REPORT, 22/27, 81.0%
10:09:55.293207 IDE <-- LS NOTIF $/progress
10:09:55.293207 OUT Elapsed: 0s
10:09:55.304622 IN Elapsed: 11.4149ms
10:09:55.304622 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.304622                             $/progress: backgroundIndexProgress REPORT, 23/27, 85.0%
10:09:55.305413 IDE <-- LS NOTIF $/progress
10:09:55.305929 OUT Elapsed: 516.8µs
10:09:55.364736 IN Elapsed: 60.1146ms
10:09:55.364736 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.364736                             $/progress: backgroundIndexProgress REPORT, 24/27, 88.0%
10:09:55.364736 IDE <-- LS NOTIF $/progress
10:09:55.364736 OUT Elapsed: 0s
10:09:55.373567 IN Elapsed: 8.8306ms
10:09:55.373567 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.373567                             $/progress: backgroundIndexProgress REPORT, 25/27, 92.0%
10:09:55.374079 IDE <-- LS NOTIF $/progress
10:09:55.374079 OUT Elapsed: 0s
10:09:55.375106 IN Elapsed: 1.0276ms
10:09:55.375106 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.375106                             $/progress: backgroundIndexProgress REPORT, 26/27, 96.0%
10:09:55.375106 IDE <-- LS NOTIF $/progress
10:09:55.375106 OUT Elapsed: 0s
10:09:55.394956 IN Elapsed: 19.8499ms
10:09:55.395075 IDE     LS <-- Clangd NOTIF $/progress
10:09:55.394956 SKETCH REBUILD: : Sketch rebuild started
10:09:55.395075                             $/progress: backgroundIndexProgress END 
10:09:55.395075 SKETCH REBUILD: : read-locked
10:09:55.395075 SKETCH REBUILD: : read-unlocked
10:09:55.394956 IDE <-- LS REQU window/workDoneProgress/create 2
10:09:55.395075 OUT Elapsed: 0s
10:09:55.395628 IN Elapsed: 1.0070479s
10:09:55.395628 IDE --> LS RESP window/workDoneProgress/create 2
10:09:55.395628 IDE <-- LS NOTIF $/progress
10:09:55.395628 OUT Elapsed: 0s
10:09:55.710630 SKETCH REBUILD: : Running build with: {
  "instance": {
    "id": 1
  },
  "fqbn": "arduino:avr:uno",
  "sketch_path": "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣器等等传感器\\Code\\Lesson 6_Passive_Buzzer\\6_Passive_Buzzer",
  "build_path": "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server3760075897",
  "verbose": true,
  "create_compilation_database_only": true,
  "source_override": {
    "6_Passive_Buzzer.ino": "void setup()\r\n{\r\n}\r\nvoid loop()\r\n{\r\n  for(int i=200;i\u003c=800;i++)  //Increase the frequency from 200HZ to 800HZ in a loop\r\n  {\r\n    pinMode(8,OUTPUT);\r\n    tone(8,i);  //Output frequency on port 8 delay(5);    //This frequency is maintained for 5 milliseconds\r\n  }\r\n  delay(4000);  //Hold for 4 seconds at the highest frequency\r\n  for(int i=800;i\u003e=200;i--)\r\n  {\r\n    pinMode(8,OUTPUT); tone(8,i);\r\n    delay(10);\r\n  }\r\n}\r\n"
  },
  "skip_libraries_discovery": true
}
10:09:56.183122 SKETCH REBUILD: : Compile successful!
10:09:56.212819 SKETCH REBUILD: : write-locked
10:09:56.216923   > Current sketchmapper content:
10:09:56.217920   0: #include <Arduino.h>                                         | /not-ino:0                                         
10:09:56.217920   1: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:09:56.217920   2: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:09:56.217920   3: void setup();                                                | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:0 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:0
10:09:56.217920   4: #line 4 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:09:56.217920   5: void loop();                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:3 G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:3
10:09:56.217920   6: #line 1 "G:\\11.ZhiYi\\5.Tutorial\\1.tutorial\\ZYA0008蜂鸣     | /not-ino:0                                         
10:09:56.217920   7: void setup()                                                 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:0                          
10:09:56.217920   8: {                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:1                          
10:09:56.217920   9: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:2                          
10:09:56.217920  10: void loop()                                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:3                          
10:09:56.217920  11: {                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:4                          
10:09:56.217920  12:   for(int i=200;i<=800;i++)  //Increase the frequency from 2 | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:5                          
10:09:56.217920  13:   {                                                          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:6                          
10:09:56.217920  14:     pinMode(8,OUTPUT);                                       | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:7                          
10:09:56.217920  15:     tone(8,i);  //Output frequency on port 8 delay(5);    // | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:8                          
10:09:56.217920  16:   }                                                          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:9                          
10:09:56.217920  17:   delay(4000);  //Hold for 4 seconds at the highest frequenc | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:10                          
10:09:56.217920  18:   for(int i=800;i>=200;i--)                                  | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:11                          
10:09:56.217920  19:   {                                                          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:12                          
10:09:56.217920  20:     pinMode(8,OUTPUT); tone(8,i);                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:13                          
10:09:56.217920  21:     delay(10);                                               | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:14                          
10:09:56.217920  22:   }                                                          | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:15                          
10:09:56.217920  23: }                                                            | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:16                          
10:09:56.217920  24:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:17                          
10:09:56.217920  25:                                                              | G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer\6_Passive_Buzzer.ino:18                          
10:09:56.217920 SKETCH REBUILD: : Sending 'didSave' notification to Clangd
10:09:56.217920 IDE     LS --> Clangd NOTIF textDocument/didSave
10:09:56.217920 OUT Elapsed: 0s
10:09:56.217920 SKETCH REBUILD: : Sending full-text 'didChange' notification to Clangd
10:09:56.217920 IDE     LS --> Clangd NOTIF textDocument/didChange
10:09:56.217920 OUT Elapsed: 0s
10:09:56.217920 SKETCH REBUILD: : write-unlocked
10:09:56.217920 IDE <-- LS NOTIF $/progress
10:09:56.217920 OUT Elapsed: 0s
10:09:56.217920 IDE <-- LS NOTIF $/progress
10:09:56.218917 OUT Elapsed: 0s
10:22:43.384651 IN Elapsed: 12m47.9890231s
10:22:43.384651 IDE --> LS REQU textDocument/codeAction 3
10:22:43.384651                 textDocument/codeAction 3: read-locked
10:22:43.384651                 textDocument/codeAction 3: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino:13:33)
10:22:43.385726                 textDocument/codeAction 3: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp
10:22:43.388904                 textDocument/codeAction 3:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp:13:33)
10:22:43.388904 IDE     LS --> Clangd REQU textDocument/codeAction 4
10:22:43.388904 OUT Elapsed: 0s
10:22:43.393602 IN Elapsed: 12m47.9985276s
10:22:43.393602 IDE     LS <-- Clangd RESP textDocument/codeAction 4
10:22:43.393602                 textDocument/codeAction 3: read-unlocked
10:22:43.393602 IDE <-- LS RESP textDocument/codeAction 3
10:22:43.393602 OUT Elapsed: 0s
10:22:47.991709 IN Elapsed: 4.5981065s
10:22:47.991709 IDE --> LS REQU textDocument/documentHighlight 4
10:22:47.991709                 textDocument/documentHighlight 4: read-locked
10:22:47.993299                 textDocument/documentHighlight 4: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp
10:22:47.996632                 textDocument/documentHighlight 4: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino:8:6 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp:15:6
10:22:47.996632 IDE     LS --> Clangd REQU textDocument/documentHighlight 5
10:22:47.997148 OUT Elapsed: 516.6µs
10:22:47.997148 IN Elapsed: 4.6035461s
10:22:47.997148 IDE     LS <-- Clangd RESP textDocument/documentHighlight 5
10:22:47.999193                 textDocument/documentHighlight 4: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp:15:4-15:8 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino:8:4-8:8 (.ino)
10:22:48.000738                 textDocument/documentHighlight 4: Range: file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp:20:23-20:27 -> file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino:13:23-13:27 (.ino)
10:22:48.000738                 textDocument/documentHighlight 4: read-unlocked
10:22:48.000738 IDE <-- LS RESP textDocument/documentHighlight 4
10:22:48.000738 OUT Elapsed: 0s
10:22:48.345424 IN Elapsed: 344.6857ms
10:22:48.345424 IDE --> LS REQU textDocument/codeAction 5
10:22:48.345424                 textDocument/codeAction 5: read-locked
10:22:48.345424                 textDocument/codeAction 5: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino:8:4)
10:22:48.346513                 textDocument/codeAction 5: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp
10:22:48.350325                 textDocument/codeAction 5:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp:8:4)
10:22:48.350357 IDE     LS --> Clangd REQU textDocument/codeAction 6
10:22:48.350357 OUT Elapsed: 0s
10:22:48.350357 IN Elapsed: 353.2083ms
10:22:48.350357 IDE     LS <-- Clangd RESP textDocument/codeAction 6
10:22:48.350357                 textDocument/codeAction 5: read-unlocked
10:22:48.350860 IDE <-- LS RESP textDocument/codeAction 5
10:22:48.350910 OUT Elapsed: 50.6µs
10:22:49.518841 IN Elapsed: 1.1679311s
10:22:49.518841 IDE --> LS REQU textDocument/codeAction 6
10:22:49.518841                 textDocument/codeAction 6: read-locked
10:22:49.518841                 textDocument/codeAction 6: --> codeAction(file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino:14:14)
10:22:49.520393                 textDocument/codeAction 6: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp
10:22:49.523883                 textDocument/codeAction 6:     --> codeAction(file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp:14:14)
10:22:49.523883 IDE     LS --> Clangd REQU textDocument/codeAction 7
10:22:49.523883 OUT Elapsed: 0s
10:22:49.527658 IN Elapsed: 1.1773017s
10:22:49.527658 IDE     LS <-- Clangd RESP textDocument/codeAction 7
10:22:49.527658                 textDocument/codeAction 6: read-unlocked
10:22:49.527658 IDE <-- LS RESP textDocument/codeAction 6
10:22:49.527658 OUT Elapsed: 0s
10:22:53.836537 IN Elapsed: 4.308879s
10:22:53.836698 IDE --> LS REQU textDocument/hover 7
10:22:53.836763                 textDocument/hover 7: read-locked
10:22:53.837917                 textDocument/hover 7: URI: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp
10:22:53.841135                 textDocument/hover 7: file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer/6_Passive_Buzzer.ino:5:31 -> file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp:12:31
10:22:53.841135 IDE     LS --> Clangd REQU textDocument/hover 8
10:22:53.841135 OUT Elapsed: 0s
10:22:53.844358 IN Elapsed: 4.3166999s
10:22:53.844871 IDE     LS <-- Clangd RESP textDocument/hover 8
10:22:53.844871                 textDocument/hover 7: null response
10:22:53.844871                 textDocument/hover 7: read-unlocked
10:22:53.844871 IDE <-- LS RESP textDocument/hover 7
10:22:53.844871 OUT Elapsed: 0s
10:22:54.834593 IN Elapsed: 989.7217ms
10:22:54.834593 IDE --> LS REQU shutdown 8
10:22:54.834593 IDE     LS --> Clangd REQU shutdown 9
10:22:54.834593 OUT Elapsed: 0s
10:22:54.834593 IN Elapsed: 989.7217ms
10:22:54.834593 IDE     LS <-- Clangd RESP shutdown 9
10:22:54.834593 IDE <-- LS RESP shutdown 8
10:22:54.834593 OUT Elapsed: 0s
10:22:54.835107 IN Elapsed: 514.1µs
10:22:54.835107 IDE --> LS NOTIF exit
10:22:54.835107 IDE     LS --> Clangd NOTIF exit
10:22:54.835610 OUT Elapsed: 502.7µs
10:22:54.835610                  exit: Arduino Language Server is shutting down.
