






Started logging.
I[09:58:37.800] clangd version 14.0.0
I[09:58:37.801] Features: windows
I[09:58:37.801] PID: 13836
I[09:58:37.801] Working directory: g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer
I[09:58:37.801] argv[0]: d:\Program Files\Arduino IDE\resources\app\node_modules\arduino-ide-extension\build\clangd.exe
I[09:58:37.801] argv[1]: -log=verbose
I[09:58:37.801] argv[2]: --compile-commands-dir=C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764
I[09:58:37.801] argv[3]: -query-driver=C:\Users\Administrator\AppData\Local\Arduino15\packages\**
V[09:58:37.809] User config file is C:\Users\Administrator\AppData\Local\clangd\config.yaml
I[09:58:37.809] Starting LSP over stdin/stdout
V[09:58:37.810] <<< {"id":"1","jsonrpc":"2.0","method":"initialize","params":{"capabilities":{"textDocument":{"codeAction":{"codeActionLiteralSupport":{"codeActionKind":{"valueSet":["","quickfix","refactor","refactor.extract","refactor.inline","refactor.rewrite","source","source.organizeImports"]}},"dynamicRegistration":true,"isPreferredSupport":true},"codeLens":{"dynamicRegistration":true},"colorProvider":{"dynamicRegistration":true},"completion":{"completionItem":{"commitCharactersSupport":true,"deprecatedSupport":true,"documentationFormat":["markdown","plaintext"],"preselectSupport":true,"snippetSupport":true,"tagSupport":{"valueSet":[1]}},"completionItemKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25]},"contextSupport":true,"dynamicRegistration":true},"declaration":{"dynamicRegistration":true,"linkSupport":true},"definition":{"dynamicRegistration":true,"linkSupport":true},"documentHighlight":{"dynamicRegistration":true},"documentLink":{"dynamicRegistration":true,"tooltipSupport":true},"documentSymbol":{"dynamicRegistration":true,"hierarchicalDocumentSymbolSupport":true,"symbolKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26]}},"foldingRange":{"dynamicRegistration":true,"lineFoldingOnly":true,"rangeLimit":5000},"formatting":{"dynamicRegistration":true},"hover":{"contentFormat":["markdown","plaintext"],"dynamicRegistration":true},"implementation":{"dynamicRegistration":true,"linkSupport":true},"onTypeFormatting":{"dynamicRegistration":true},"publishDiagnostics":{"relatedInformation":true,"tagSupport":{"valueSet":[1,2]}},"rangeFormatting":{"dynamicRegistration":true},"references":{"dynamicRegistration":true},"rename":{"dynamicRegistration":true,"prepareSupport":true},"selectionRange":{"dynamicRegistration":true},"signatureHelp":{"contextSupport":true,"dynamicRegistration":true,"signatureInformation":{"documentationFormat":["markdown","plaintext"],"parameterInformation":{"labelOffsetSupport":true}}},"synchronization":{"didSave":true,"dynamicRegistration":true,"willSave":true,"willSaveWaitUntil":true},"typeDefinition":{"dynamicRegistration":true,"linkSupport":true}},"window":{"workDoneProgress":true},"workspace":{"applyEdit":true,"configuration":true,"didChangeConfiguration":{"dynamicRegistration":true},"didChangeWatchedFiles":{"dynamicRegistration":true},"executeCommand":{"dynamicRegistration":true},"symbol":{"dynamicRegistration":true,"symbolKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26]}},"workspaceEdit":{"documentChanges":true,"failureHandling":"textOnlyTransactional","resourceOperations":["create","rename","delete"]},"workspaceFolders":true}},"clientInfo":{"name":"vscode","version":"1.53.2"},"initializationOptions":{},"processId":13004,"rootPath":"C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch","rootUri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch","trace":"off","workspaceFolders":[{"name":"5_Active_buzzer","uri":"file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer"}]}}

I[09:58:37.810] <-- initialize("1")
I[09:58:37.870] --> reply:initialize("1") 60 ms
V[09:58:37.870] >>> {"id":"1","jsonrpc":"2.0","result":{"capabilities":{"astProvider":true,"callHierarchyProvider":true,"clangdInlayHintsProvider":true,"codeActionProvider":{"codeActionKinds":["quickfix","refactor","info"]},"compilationDatabase":{"automaticReload":true},"completionProvider":{"allCommitCharacters":[" ","\t","(",")","[","]","{","}","<",">",":",";",",","+","-","/","*","%","^","&","#","?",".","=","\"","'","|"],"resolveProvider":false,"triggerCharacters":[".","<",">",":","\"","/","*"]},"declarationProvider":true,"definitionProvider":true,"documentFormattingProvider":true,"documentHighlightProvider":true,"documentLinkProvider":{"resolveProvider":false},"documentOnTypeFormattingProvider":{"firstTriggerCharacter":"\n","moreTriggerCharacter":[]},"documentRangeFormattingProvider":true,"documentSymbolProvider":true,"executeCommandProvider":{"commands":["clangd.applyFix","clangd.applyTweak"]},"hoverProvider":true,"implementationProvider":true,"memoryUsageProvider":true,"referencesProvider":true,"renameProvider":{"prepareProvider":true},"selectionRangeProvider":true,"semanticTokensProvider":{"full":{"delta":true},"legend":{"tokenModifiers":["declaration","deprecated","deduced","readonly","static","abstract","virtual","dependentName","defaultLibrary","usedAsMutableReference","functionScope","classScope","fileScope","globalScope"],"tokenTypes":["variable","variable","parameter","function","method","function","property","variable","class","interface","enum","enumMember","type","type","unknown","namespace","typeParameter","concept","type","macro","comment"]},"range":false},"signatureHelpProvider":{"triggerCharacters":["(",")","{","}","<",">",","]},"textDocumentSync":{"change":2,"openClose":true,"save":true},"typeDefinitionProvider":true,"typeHierarchyProvider":true,"workspaceSymbolProvider":true},"serverInfo":{"name":"clangd","version":"clangd version 14.0.0 windows x86_64-pc-windows-msvc"}}}

V[09:58:37.871] <<< {"jsonrpc":"2.0","method":"initialized","params":{}}

I[09:58:37.871] <-- initialized
V[09:58:37.877] <<< {"jsonrpc":"2.0","method":"textDocument/didOpen","params":{"textDocument":{"languageId":"cpp","text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\n\n#include \"pitches.h\"// notes in the melody:\nint melody[] = {\nNOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};\nint duration = 500;  // 500 miliseconds \n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup();\n#line 7 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid loop();\n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup() {  }\nvoid loop() {\nfor (int thisNote = 0; thisNote < 12; thisNote++) {\n// pin12 output the voice, every scale is 0.5 sencond \ntone(12, melody[thisNote], duration);\ndelay(100);\n// Output the voice after several minutes\ndelay(100);\n} // restart after two seconds \ndelay(200);\n}\n\n","uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":1}}}

I[09:58:37.877] <-- textDocument/didOpen
V[09:58:37.881] config note at C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\.clangd:1:0: Parsing config fragment
V[09:58:37.881] config note at C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\.clangd:1:0: Parsed 1 fragments from file
V[09:58:37.881] Config fragment: compiling C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\.clangd:1 -> 0x0000028D41AA9E10 (trusted=false)
I[09:58:37.882] --> textDocument/publishDiagnostics
V[09:58:37.882] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/.clangd"}}

I[09:58:37.883] Loaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\compile_commands.json
V[09:58:37.883] <<< {"id":"2","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":11,"line":21},"start":{"character":11,"line":21}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:58:37.883] <-- textDocument/codeAction("2")
V[09:58:37.883] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764
I[09:58:37.886] --> window/workDoneProgress/create(0)
V[09:58:37.886] >>> {"id":0,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[09:58:37.886] Enqueueing 26 commands for indexing
V[09:58:37.887] <<< {"id":0,"jsonrpc":"2.0","result":null}

I[09:58:37.887] <-- reply(0)
I[09:58:37.887] --> $/progress
V[09:58:37.887] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[09:58:37.887] --> $/progress
V[09:58:37.887] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[09:58:37.888] Failed to load shard: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
V[09:58:37.888] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp
V[09:58:37.888] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp
V[09:58:37.888] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c
V[09:58:37.888] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c
V[09:58:37.888] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp
V[09:58:37.888] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp
V[09:58:37.888] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp
V[09:58:37.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp
V[09:58:37.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp
V[09:58:37.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp
V[09:58:37.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S
V[09:58:37.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp
V[09:58:37.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp
V[09:58:37.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c
V[09:58:37.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp
V[09:58:37.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp
V[09:58:37.889] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp
V[09:58:37.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp
V[09:58:37.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c
V[09:58:37.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c
V[09:58:37.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp
V[09:58:37.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp
V[09:58:37.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c
V[09:58:37.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp
V[09:58:37.890] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c
I[09:58:37.895] --> $/progress
V[09:58:37.895] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[09:58:37.895] --> $/progress
V[09:58:37.895] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[09:58:37.895] --> $/progress
V[09:58:37.895] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[09:58:37.895] --> $/progress
V[09:58:37.895] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[09:58:37.895] --> $/progress
V[09:58:37.895] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[09:58:37.895] --> $/progress
V[09:58:37.895] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[09:58:37.895] --> $/progress
V[09:58:37.895] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[09:58:37.895] --> $/progress
V[09:58:37.895] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

V[09:58:38.005] System include extraction: target extracted: "avr"
V[09:58:38.005] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[09:58:38.005] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[09:58:38.005] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[09:58:38.005] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
I[09:58:38.006] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 1 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[09:58:38.015] System include extraction: target extracted: "avr"
V[09:58:38.015] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[09:58:38.015] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[09:58:38.015] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[09:58:38.015] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[09:58:38.017] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp (digest:=FDB5BCAAB3E73FCE)
V[09:58:38.026] System include extraction: target extracted: "avr"
V[09:58:38.026] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[09:58:38.026] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[09:58:38.026] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[09:58:38.026] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-gcc.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[09:58:38.029] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c (digest:=5D6C1534064234DD)
V[09:58:38.032] System include extraction: target extracted: "avr"
V[09:58:38.032] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[09:58:38.032] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[09:58:38.032] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[09:58:38.032] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[09:58:38.033] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[09:58:38.033] Building first preamble for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 1
V[09:58:38.033] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp (digest:=487C94A1A1F49B6C)
V[09:58:38.043] System include extraction: target extracted: "avr"
V[09:58:38.043] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[09:58:38.043] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[09:58:38.043] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[09:58:38.043] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[09:58:38.045] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp (digest:=3DD4F70FCF8C4FA6)
V[09:58:38.049] System include extraction: target extracted: "avr"
V[09:58:38.049] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[09:58:38.049] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[09:58:38.049] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[09:58:38.049] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[09:58:38.052] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp (digest:=81BB1157C290C33B)
V[09:58:38.052] System include extraction: target extracted: "avr"
V[09:58:38.052] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[09:58:38.052] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[09:58:38.052] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[09:58:38.052] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[09:58:38.059] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp (digest:=6DDB6ED4F4E34E63)
V[09:58:38.119] indexed preamble AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 1:
  symbol slab: 2499 symbols, 711406 bytes
  ref slab: 0 symbols, 0 refs, 136 bytes
  relations slab: 9 relations, 177 bytes
V[09:58:38.148] Build dynamic index for header symbols with estimated memory usage of 2158018 bytes
V[09:58:38.152] Built preamble of size 427916 for file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 1
I[09:58:38.163] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c (312 symbols, 2775 refs, 25 files)
I[09:58:38.170] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp (600 symbols, 3432 refs, 36 files)
I[09:58:38.195] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp (602 symbols, 3499 refs, 37 files)
I[09:58:38.197] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp (602 symbols, 3499 refs, 37 files)
V[09:58:38.212] Trying to fix unresolved name "NOTE_C5" in scopes: []
V[09:58:38.212] Dex query tree: false
V[09:58:38.213] Trying to fix unresolved name "NOTE_D5" in scopes: []
V[09:58:38.213] Dex query tree: false
V[09:58:38.213] Trying to fix unresolved name "NOTE_E5" in scopes: []
V[09:58:38.213] Dex query tree: false
V[09:58:38.214] Trying to fix unresolved name "NOTE_F5" in scopes: []
V[09:58:38.214] Dex query tree: false
V[09:58:38.214] Trying to fix unresolved name "NOTE_G5" in scopes: []
V[09:58:38.214] Dex query tree: false
V[09:58:38.214] Trying to fix unresolved name "NOTE_A5" in scopes: []
V[09:58:38.215] Trying to fix unresolved name "NOTE_B5" in scopes: []
V[09:58:38.215] Trying to fix unresolved name "NOTE_C6" in scopes: []
V[09:58:38.217] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 1:
  symbol slab: 4 symbols, 5152 bytes
  ref slab: 6 symbols, 12 refs, 4376 bytes
  relations slab: 0 relations, 24 bytes
V[09:58:38.217] Build dynamic index for main-file symbols with estimated memory usage of 13400 bytes
I[09:58:38.217] --> textDocument/publishDiagnostics
V[09:58:38.217] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[{"code":"pp_file_not_found","message":"'pitches.h' file not found","range":{"end":{"character":20,"line":3},"start":{"character":9,"line":3}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C5'","range":{"end":{"character":7,"line":5},"start":{"character":0,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_D5'","range":{"end":{"character":16,"line":5},"start":{"character":9,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_E5'","range":{"end":{"character":25,"line":5},"start":{"character":18,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_F5'","range":{"end":{"character":34,"line":5},"start":{"character":27,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_G5'","range":{"end":{"character":43,"line":5},"start":{"character":36,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_A5'","range":{"end":{"character":52,"line":5},"start":{"character":45,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_B5'","range":{"end":{"character":61,"line":5},"start":{"character":54,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C6'","range":{"end":{"character":70,"line":5},"start":{"character":63,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"}],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":1}}

V[09:58:38.217] ASTWorker running EnumerateTweaks on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:58:38.217] --> reply:textDocument/codeAction("2") 334 ms
V[09:58:38.218] >>> {"id":"2","jsonrpc":"2.0","result":[]}

V[09:58:38.219] <<< {"id":"3","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:58:38.219] <-- textDocument/documentSymbol("3")
V[09:58:38.219] ASTWorker running DocumentSymbols on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:58:38.219] --> reply:textDocument/documentSymbol("3") 0 ms
V[09:58:38.219] >>> {"id":"3","jsonrpc":"2.0","result":[{"detail":"int[]","kind":13,"name":"melody","range":{"end":{"character":12,"line":4},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

I[09:58:38.221] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp (620 symbols, 3567 refs, 36 files)
I[09:58:38.226] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp (600 symbols, 3583 refs, 35 files)
I[09:58:38.707] --> $/progress
V[09:58:38.707] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"2/27","percentage":7}}}

I[09:58:38.707] --> $/progress
V[09:58:38.707] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"2/27","percentage":7}}}

V[09:58:38.711] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp (digest:=38075D39C713EC91)
I[09:58:38.757] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp (46 symbols, 139 refs, 3 files)
I[09:58:38.763] --> $/progress
V[09:58:38.763] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"3/27","percentage":11}}}

I[09:58:38.763] --> $/progress
V[09:58:38.763] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"3/27","percentage":11}}}

V[09:58:38.765] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp (digest:=365287FBD658A80E)
I[09:58:38.806] --> $/progress
V[09:58:38.806] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"4/27","percentage":14}}}

I[09:58:38.806] --> $/progress
V[09:58:38.806] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"4/27","percentage":14}}}

V[09:58:38.809] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp (digest:=7D1D0E442CF15FC1)
I[09:58:38.851] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp (4 symbols, 2292 refs, 37 files)
I[09:58:38.897] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp (12 symbols, 2468 refs, 38 files)
I[09:58:38.906] --> $/progress
V[09:58:38.906] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"5/27","percentage":18}}}

I[09:58:38.906] --> $/progress
V[09:58:38.906] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"5/27","percentage":18}}}

I[09:58:38.912] --> $/progress
V[09:58:38.912] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"6/27","percentage":22}}}

I[09:58:38.912] --> $/progress
V[09:58:38.912] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"6/27","percentage":22}}}

V[09:58:38.915] BackgroundIndex: building version 1 after indexing enough files
V[09:58:38.927] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp (digest:=D7FFC6931C21680C)
V[09:58:38.927] BackgroundIndex: serving version 1 (1447822 bytes)
I[09:58:38.928] --> $/progress
V[09:58:38.928] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"7/27","percentage":25}}}

I[09:58:38.928] --> $/progress
V[09:58:38.928] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"7/27","percentage":25}}}

V[09:58:38.930] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp (digest:=313C4893EB7ADBE6)
V[09:58:38.932] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp (digest:=E3E9F11672EDD20A)
I[09:58:39.014] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp (0 symbols, 2251 refs, 37 files)
I[09:58:39.014] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp (4 symbols, 2226 refs, 35 files)
I[09:58:39.021] --> $/progress
V[09:58:39.021] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"8/27","percentage":29}}}

I[09:58:39.021] --> $/progress
V[09:58:39.021] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"8/27","percentage":29}}}

I[09:58:39.024] --> $/progress
V[09:58:39.024] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"9/27","percentage":33}}}

I[09:58:39.024] --> $/progress
V[09:58:39.024] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"9/27","percentage":33}}}

V[09:58:39.026] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c (digest:=0A36B38756A4F148)
V[09:58:39.033] Ignored diagnostic. c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include\avr/wdt.h:464:12:value '64' out of range for constraint 'I'
V[09:58:39.034] Ignored diagnostic. c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include\avr/wdt.h:507:23:value '64' out of range for constraint 'I'
I[09:58:39.041] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp (2 symbols, 2301 refs, 37 files)
I[09:58:39.041] Failed to compile C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp, index may be incomplete
I[09:58:39.054] --> $/progress
V[09:58:39.054] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"10/27","percentage":37}}}

I[09:58:39.054] --> $/progress
V[09:58:39.054] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"10/27","percentage":37}}}

V[09:58:39.056] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c (digest:=C16B0ED8B1C5BB9F)
I[09:58:39.059] --> $/progress
V[09:58:39.059] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"11/27","percentage":40}}}

I[09:58:39.059] --> $/progress
V[09:58:39.059] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"11/27","percentage":40}}}

V[09:58:39.061] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c (digest:=343A7ACAD5FD2414)
I[09:58:39.076] --> $/progress
V[09:58:39.076] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"12/27","percentage":44}}}

I[09:58:39.076] --> $/progress
V[09:58:39.076] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"12/27","percentage":44}}}

V[09:58:39.079] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp (digest:=1C31198B0754810E)
I[09:58:39.082] --> $/progress
V[09:58:39.082] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"13/27","percentage":48}}}

I[09:58:39.082] --> $/progress
V[09:58:39.082] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"13/27","percentage":48}}}

V[09:58:39.085] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp (digest:=293923F15565174B)
I[09:58:39.089] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c (1 symbols, 1 refs, 1 files)
V[09:58:39.094] System include extraction: target extracted: "avr"
V[09:58:39.094] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[09:58:39.094] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[09:58:39.094] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[09:58:39.094] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-gcc.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
I[09:58:39.095] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c (4 symbols, 2166 refs, 25 files)
I[09:58:39.096] --> $/progress
V[09:58:39.096] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"14/27","percentage":51}}}

I[09:58:39.096] --> $/progress
V[09:58:39.096] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"14/27","percentage":51}}}

V[09:58:39.096] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S (digest:=87583F1C920AA889)
V[09:58:39.098] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c (digest:=B0774BE9D28D49CB)
I[09:58:39.103] --> $/progress
V[09:58:39.103] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"15/27","percentage":55}}}

I[09:58:39.103] --> $/progress
V[09:58:39.103] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"15/27","percentage":55}}}

V[09:58:39.106] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c (digest:=5E8D23E876F6F446)
V[09:58:39.135] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:54:1:expected identifier or '('
V[09:58:39.136] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:62:23:expected identifier or '('
V[09:58:39.136] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:63:23:expected identifier or '('
V[09:58:39.136] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:64:23:expected identifier or '('
V[09:58:39.136] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:65:23:expected identifier or '('
V[09:58:39.136] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:66:23:expected identifier or '('
V[09:58:39.136] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:67:23:expected identifier or '('
V[09:58:39.136] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:72:37:expected identifier or '('
I[09:58:39.136] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c (4 symbols, 2340 refs, 25 files)
V[09:58:39.137] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:73:31:expected ';' after top level declarator
V[09:58:39.137] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:79:23:expected identifier or '('
V[09:58:39.137] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:83:32:expected identifier or '('
V[09:58:39.137] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:83:35:expected identifier or '('
V[09:58:39.138] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:84:22:unknown type name 'maxloops'
V[09:58:39.138] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:85:8:expected ';' after top level declarator
V[09:58:39.138] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:85:22:unknown type name 'maxloops'
V[09:58:39.138] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:86:8:expected ';' after top level declarator
V[09:58:39.139] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:86:22:unknown type name 'maxloops'
V[09:58:39.139] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:87:9:expected ';' after top level declarator
V[09:58:39.139] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:87:18:expected identifier or '('
V[09:58:39.139] Ignored diagnostic. too many errors emitted, stopping now
I[09:58:39.142] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S (12 symbols, 937 refs, 9 files)
I[09:58:39.142] Failed to compile C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S, index may be incomplete
I[09:58:39.144] --> $/progress
V[09:58:39.144] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"16/27","percentage":59}}}

I[09:58:39.144] --> $/progress
V[09:58:39.144] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"16/27","percentage":59}}}

V[09:58:39.147] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp (digest:=F68AA83B5BAAD75D)
I[09:58:39.148] --> $/progress
V[09:58:39.148] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"17/27","percentage":62}}}

I[09:58:39.148] --> $/progress
V[09:58:39.148] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"17/27","percentage":62}}}

V[09:58:39.150] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp (digest:=F7D59D2B49112307)
I[09:58:39.161] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c (2 symbols, 2141 refs, 25 files)
I[09:58:39.163] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp (84 symbols, 1925 refs, 18 files)
I[09:58:39.167] --> $/progress
V[09:58:39.167] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"18/27","percentage":66}}}

I[09:58:39.167] --> $/progress
V[09:58:39.167] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"18/27","percentage":66}}}

I[09:58:39.168] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c (2 symbols, 2115 refs, 25 files)
V[09:58:39.169] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c (digest:=BC32CF542FD8D605)
I[09:58:39.176] --> $/progress
V[09:58:39.176] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"19/27","percentage":70}}}

I[09:58:39.176] --> $/progress
V[09:58:39.176] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"19/27","percentage":70}}}

I[09:58:39.178] --> $/progress
V[09:58:39.178] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"20/27","percentage":74}}}

I[09:58:39.178] --> $/progress
V[09:58:39.178] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"20/27","percentage":74}}}

V[09:58:39.180] Indexing C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp (digest:=17390AE5437DD899)
V[09:58:39.181] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp (digest:=4A1244E54C0CAC04)
I[09:58:39.183] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp (15 symbols, 2449 refs, 35 files)
I[09:58:39.191] --> $/progress
V[09:58:39.191] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"21/27","percentage":77}}}

I[09:58:39.191] --> $/progress
V[09:58:39.191] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"21/27","percentage":77}}}

V[09:58:39.194] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp (digest:=55BA50D4FF04E609)
I[09:58:39.198] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp (21 symbols, 150 refs, 5 files)
I[09:58:39.216] --> $/progress
V[09:58:39.216] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"22/27","percentage":81}}}

I[09:58:39.224] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp (2 symbols, 83 refs, 3 files)
I[09:58:39.229] --> $/progress
V[09:58:39.229] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"23/27","percentage":85}}}

I[09:58:39.229] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c (4 symbols, 2201 refs, 25 files)
I[09:58:39.232] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp (15 symbols, 2336 refs, 35 files)
I[09:58:39.236] --> $/progress
V[09:58:39.236] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"24/27","percentage":88}}}

I[09:58:39.239] --> $/progress
V[09:58:39.239] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"25/27","percentage":92}}}

V[09:58:39.247] Ignored diagnostic. G:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer\5_Active_buzzer.ino:2:10:'pitches.h' file not found
I[09:58:39.252] Indexed C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp (4 symbols, 2226 refs, 35 files)
I[09:58:39.252] Failed to compile C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp, index may be incomplete
I[09:58:39.258] --> $/progress
V[09:58:39.258] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"26/27","percentage":96}}}

I[09:58:39.264] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp (0 symbols, 2222 refs, 36 files)
V[09:58:39.270] BackgroundIndex: building version 2 when background indexer is idle
V[09:58:39.280] BackgroundIndex: serving version 2 (1767862 bytes)
I[09:58:39.281] --> $/progress
V[09:58:39.281] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[09:59:32.963] <<< {"id":"4","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":6,"line":16},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:32.963] <-- textDocument/hover("4")
V[09:59:32.967] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:32.971] --> reply:textDocument/hover("4") 7 ms
V[09:59:32.971] >>> {"id":"4","jsonrpc":"2.0","result":null}

V[09:59:33.030] <<< {"id":"5","jsonrpc":"2.0","method":"textDocument/documentHighlight","params":{"position":{"character":6,"line":16},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:33.030] <-- textDocument/documentHighlight("5")
V[09:59:33.030] ASTWorker running Highlights on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:33.030] --> reply:textDocument/documentHighlight("5") 0 ms
V[09:59:33.030] >>> {"id":"5","jsonrpc":"2.0","result":[]}

V[09:59:33.454] <<< {"id":"6","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":7,"line":16},"start":{"character":5,"line":16}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:33.454] <-- textDocument/codeAction("6")
V[09:59:33.454] ASTWorker running EnumerateTweaks on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:33.455] --> reply:textDocument/codeAction("6") 0 ms
V[09:59:33.455] >>> {"id":"6","jsonrpc":"2.0","result":[{"command":{"arguments":[{"file":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","selection":{"end":{"character":7,"line":16},"start":{"character":5,"line":16}},"tweakID":"ExtractVariable"}],"command":"clangd.applyTweak","title":"Extract subexpression to variable"},"kind":"refactor","title":"Extract subexpression to variable"}]}

V[09:59:52.307] <<< {"id":"7","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:52.307] <-- textDocument/documentSymbol("7")
V[09:59:52.311] ASTWorker running DocumentSymbols on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:52.311] --> reply:textDocument/documentSymbol("7") 3 ms
V[09:59:52.311] >>> {"id":"7","jsonrpc":"2.0","result":[{"detail":"int[]","kind":13,"name":"melody","range":{"end":{"character":12,"line":4},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

V[09:59:52.335] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"range":{"end":{"character":7,"line":16},"start":{"character":5,"line":16}},"text":"1"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":2}}}

I[09:59:52.335] <-- textDocument/didChange
V[09:59:52.337] <<< {"id":"8","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:52.337] <-- textDocument/documentSymbol("8")
I[09:59:52.338] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 2 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[09:59:52.362] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[09:59:52.370] Reusing preamble version 1 for version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
V[09:59:52.387] ASTWorker rebuilding evicted AST to run DocumentSymbols: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 2
V[09:59:52.439] Trying to fix unresolved name "NOTE_C5" in scopes: []
V[09:59:52.439] Dex query tree: false
V[09:59:52.439] Dex query tree: false
V[09:59:52.439] Trying to fix unresolved name "NOTE_D5" in scopes: []
V[09:59:52.439] Dex query tree: false
V[09:59:52.439] Dex query tree: false
V[09:59:52.440] Trying to fix unresolved name "NOTE_E5" in scopes: []
V[09:59:52.440] Dex query tree: false
V[09:59:52.440] Dex query tree: false
V[09:59:52.440] Trying to fix unresolved name "NOTE_F5" in scopes: []
V[09:59:52.440] Dex query tree: false
V[09:59:52.440] Dex query tree: false
V[09:59:52.441] Trying to fix unresolved name "NOTE_G5" in scopes: []
V[09:59:52.441] Dex query tree: false
V[09:59:52.441] Dex query tree: false
V[09:59:52.441] Trying to fix unresolved name "NOTE_A5" in scopes: []
V[09:59:52.442] Trying to fix unresolved name "NOTE_B5" in scopes: []
V[09:59:52.442] Trying to fix unresolved name "NOTE_C6" in scopes: []
V[09:59:52.443] ASTWorker running DocumentSymbols on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:52.443] --> reply:textDocument/documentSymbol("8") 106 ms
V[09:59:52.443] >>> {"id":"8","jsonrpc":"2.0","result":[{"detail":"int[]","kind":13,"name":"melody","range":{"end":{"character":12,"line":4},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

I[09:59:52.443] Skipping rebuild of the AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp, inputs are the same.
V[09:59:52.444] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 2:
  symbol slab: 4 symbols, 5152 bytes
  ref slab: 6 symbols, 12 refs, 4376 bytes
  relations slab: 0 relations, 24 bytes
V[09:59:52.444] Build dynamic index for main-file symbols with estimated memory usage of 13400 bytes
I[09:59:52.444] --> textDocument/publishDiagnostics
V[09:59:52.444] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[{"code":"pp_file_not_found","message":"'pitches.h' file not found","range":{"end":{"character":20,"line":3},"start":{"character":9,"line":3}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C5'","range":{"end":{"character":7,"line":5},"start":{"character":0,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_D5'","range":{"end":{"character":16,"line":5},"start":{"character":9,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_E5'","range":{"end":{"character":25,"line":5},"start":{"character":18,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_F5'","range":{"end":{"character":34,"line":5},"start":{"character":27,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_G5'","range":{"end":{"character":43,"line":5},"start":{"character":36,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_A5'","range":{"end":{"character":52,"line":5},"start":{"character":45,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_B5'","range":{"end":{"character":61,"line":5},"start":{"character":54,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C6'","range":{"end":{"character":70,"line":5},"start":{"character":63,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"}],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":2}}

V[09:59:52.465] <<< {"id":"9","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:52.465] <-- textDocument/documentSymbol("9")
V[09:59:52.465] ASTWorker running DocumentSymbols on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:52.465] --> reply:textDocument/documentSymbol("9") 0 ms
V[09:59:52.465] >>> {"id":"9","jsonrpc":"2.0","result":[{"detail":"int[]","kind":13,"name":"melody","range":{"end":{"character":12,"line":4},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

V[09:59:52.490] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"range":{"end":{"character":6,"line":16},"start":{"character":6,"line":16}},"text":"4"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":3}}}

I[09:59:52.490] <-- textDocument/didChange
V[09:59:52.492] <<< {"id":"10","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:52.492] <-- textDocument/documentSymbol("10")
I[09:59:52.492] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 3 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[09:59:52.516] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[09:59:52.526] Reusing preamble version 1 for version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
V[09:59:52.542] ASTWorker rebuilding evicted AST to run DocumentSymbols: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 3
V[09:59:52.591] Trying to fix unresolved name "NOTE_C5" in scopes: []
V[09:59:52.591] Dex query tree: false
V[09:59:52.591] Dex query tree: false
V[09:59:52.591] Trying to fix unresolved name "NOTE_D5" in scopes: []
V[09:59:52.591] Dex query tree: false
V[09:59:52.591] Dex query tree: false
V[09:59:52.592] Trying to fix unresolved name "NOTE_E5" in scopes: []
V[09:59:52.592] Dex query tree: false
V[09:59:52.592] Dex query tree: false
V[09:59:52.592] Trying to fix unresolved name "NOTE_F5" in scopes: []
V[09:59:52.592] Dex query tree: false
V[09:59:52.592] Dex query tree: false
V[09:59:52.593] Trying to fix unresolved name "NOTE_G5" in scopes: []
V[09:59:52.593] Dex query tree: false
V[09:59:52.593] Dex query tree: false
V[09:59:52.593] Trying to fix unresolved name "NOTE_A5" in scopes: []
V[09:59:52.593] Trying to fix unresolved name "NOTE_B5" in scopes: []
V[09:59:52.594] Trying to fix unresolved name "NOTE_C6" in scopes: []
V[09:59:52.594] ASTWorker running DocumentSymbols on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:52.595] --> reply:textDocument/documentSymbol("10") 102 ms
V[09:59:52.595] >>> {"id":"10","jsonrpc":"2.0","result":[{"detail":"int[]","kind":13,"name":"melody","range":{"end":{"character":12,"line":4},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

I[09:59:52.595] Skipping rebuild of the AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp, inputs are the same.
V[09:59:52.596] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 3:
  symbol slab: 4 symbols, 5152 bytes
  ref slab: 6 symbols, 12 refs, 4376 bytes
  relations slab: 0 relations, 24 bytes
V[09:59:52.596] Build dynamic index for main-file symbols with estimated memory usage of 13400 bytes
I[09:59:52.596] --> textDocument/publishDiagnostics
V[09:59:52.596] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[{"code":"pp_file_not_found","message":"'pitches.h' file not found","range":{"end":{"character":20,"line":3},"start":{"character":9,"line":3}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C5'","range":{"end":{"character":7,"line":5},"start":{"character":0,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_D5'","range":{"end":{"character":16,"line":5},"start":{"character":9,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_E5'","range":{"end":{"character":25,"line":5},"start":{"character":18,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_F5'","range":{"end":{"character":34,"line":5},"start":{"character":27,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_G5'","range":{"end":{"character":43,"line":5},"start":{"character":36,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_A5'","range":{"end":{"character":52,"line":5},"start":{"character":45,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_B5'","range":{"end":{"character":61,"line":5},"start":{"character":54,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C6'","range":{"end":{"character":70,"line":5},"start":{"character":63,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"}],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":3}}

V[09:59:52.765] <<< {"id":"11","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":7,"line":16},"start":{"character":7,"line":16}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:52.765] <-- textDocument/codeAction("11")
V[09:59:52.765] ASTWorker running EnumerateTweaks on version 3 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:52.766] --> reply:textDocument/codeAction("11") 0 ms
V[09:59:52.766] >>> {"id":"11","jsonrpc":"2.0","result":[]}

V[09:59:55.232] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:55.232] <-- textDocument/didSave
I[09:59:55.232] File version went from 3 to 3
V[09:59:55.232] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\n\n#include \"pitches.h\"// notes in the melody:\nint melody[] = {\nNOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};\nint duration = 500;  // 500 miliseconds \n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup();\n#line 7 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid loop();\n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup() {  }\nvoid loop() {\nfor (int thisNote = 0; thisNote < 12; thisNote++) {\n// pin12 output the voice, every scale is 0.5 sencond \ntone(14, melody[thisNote], duration);\ndelay(100);\n// Output the voice after several minutes\ndelay(100);\n} // restart after two seconds \ndelay(200);\n}\n\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":4}}}

I[09:59:55.232] <-- textDocument/didChange
V[09:59:55.232] ASTWorker skipping Update (3) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:55.307] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 4 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[09:59:55.355] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[09:59:55.362] Reusing preamble version 1 for version 4 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
V[09:59:56.017] <<< {"id":"12","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:56.017] <-- textDocument/documentSymbol("12")
V[09:59:56.017] ASTWorker running DocumentSymbols on version 4 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:56.017] --> reply:textDocument/documentSymbol("12") 0 ms
V[09:59:56.017] >>> {"id":"12","jsonrpc":"2.0","result":[{"detail":"int[]","kind":13,"name":"melody","range":{"end":{"character":12,"line":4},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

V[09:59:56.042] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"range":{"end":{"character":7,"line":16},"start":{"character":5,"line":16}},"text":"12"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":5}}}

I[09:59:56.042] <-- textDocument/didChange
I[09:59:56.110] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 5 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[09:59:56.134] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[09:59:56.141] Reusing preamble version 1 for version 5 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
V[09:59:56.190] Trying to fix unresolved name "NOTE_C5" in scopes: []
V[09:59:56.190] Dex query tree: false
V[09:59:56.190] Dex query tree: false
V[09:59:56.191] Trying to fix unresolved name "NOTE_D5" in scopes: []
V[09:59:56.191] Dex query tree: false
V[09:59:56.191] Dex query tree: false
V[09:59:56.191] Trying to fix unresolved name "NOTE_E5" in scopes: []
V[09:59:56.191] Dex query tree: false
V[09:59:56.191] Dex query tree: false
V[09:59:56.192] Trying to fix unresolved name "NOTE_F5" in scopes: []
V[09:59:56.192] Dex query tree: false
V[09:59:56.192] Dex query tree: false
V[09:59:56.192] Trying to fix unresolved name "NOTE_G5" in scopes: []
V[09:59:56.192] Dex query tree: false
V[09:59:56.192] Dex query tree: false
V[09:59:56.193] Trying to fix unresolved name "NOTE_A5" in scopes: []
V[09:59:56.193] Trying to fix unresolved name "NOTE_B5" in scopes: []
V[09:59:56.193] Trying to fix unresolved name "NOTE_C6" in scopes: []
V[09:59:56.195] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 5:
  symbol slab: 4 symbols, 5152 bytes
  ref slab: 6 symbols, 12 refs, 4376 bytes
  relations slab: 0 relations, 24 bytes
V[09:59:56.195] Build dynamic index for main-file symbols with estimated memory usage of 13400 bytes
I[09:59:56.195] --> textDocument/publishDiagnostics
V[09:59:56.195] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[{"code":"pp_file_not_found","message":"'pitches.h' file not found","range":{"end":{"character":20,"line":3},"start":{"character":9,"line":3}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C5'","range":{"end":{"character":7,"line":5},"start":{"character":0,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_D5'","range":{"end":{"character":16,"line":5},"start":{"character":9,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_E5'","range":{"end":{"character":25,"line":5},"start":{"character":18,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_F5'","range":{"end":{"character":34,"line":5},"start":{"character":27,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_G5'","range":{"end":{"character":43,"line":5},"start":{"character":36,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_A5'","range":{"end":{"character":52,"line":5},"start":{"character":45,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_B5'","range":{"end":{"character":61,"line":5},"start":{"character":54,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C6'","range":{"end":{"character":70,"line":5},"start":{"character":63,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"}],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":5}}

V[09:59:56.273] <<< {"id":"13","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":7,"line":16},"start":{"character":5,"line":16}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:56.273] <-- textDocument/codeAction("13")
V[09:59:56.273] ASTWorker running EnumerateTweaks on version 5 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:56.273] --> reply:textDocument/codeAction("13") 0 ms
V[09:59:56.273] >>> {"id":"13","jsonrpc":"2.0","result":[{"command":{"arguments":[{"file":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","selection":{"end":{"character":7,"line":16},"start":{"character":5,"line":16}},"tweakID":"ExtractVariable"}],"command":"clangd.applyTweak","title":"Extract subexpression to variable"},"kind":"refactor","title":"Extract subexpression to variable"}]}

V[09:59:57.529] <<< {"id":"14","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:57.529] <-- textDocument/documentSymbol("14")
V[09:59:57.532] ASTWorker running DocumentSymbols on version 5 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:57.532] --> reply:textDocument/documentSymbol("14") 3 ms
V[09:59:57.532] >>> {"id":"14","jsonrpc":"2.0","result":[{"detail":"int[]","kind":13,"name":"melody","range":{"end":{"character":12,"line":4},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

V[09:59:57.556] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"range":{"end":{"character":7,"line":16},"start":{"character":5,"line":16}},"text":"1"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":6}}}

I[09:59:57.556] <-- textDocument/didChange
V[09:59:57.558] <<< {"id":"15","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:57.558] <-- textDocument/documentSymbol("15")
I[09:59:57.559] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\compile_commands.json
V[09:59:57.559] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764
I[09:59:57.559] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 6 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
I[09:59:57.562] --> window/workDoneProgress/create(1)
V[09:59:57.562] >>> {"id":1,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[09:59:57.562] Enqueueing 26 commands for indexing
V[09:59:57.563] <<< {"id":1,"jsonrpc":"2.0","result":null}

I[09:59:57.563] <-- reply(1)
I[09:59:57.563] --> $/progress
V[09:59:57.563] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[09:59:57.563] --> $/progress
V[09:59:57.563] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[09:59:57.585] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[09:59:57.586] BackgroundIndex: building version 3 after loading index from disk
V[09:59:57.594] Reusing preamble version 1 for version 6 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
V[09:59:57.597] BackgroundIndex: serving version 3 (1767862 bytes)
I[09:59:57.610] --> $/progress
V[09:59:57.610] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[09:59:57.610] --> $/progress
V[09:59:57.610] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[09:59:57.610] ASTWorker rebuilding evicted AST to run DocumentSymbols: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 6
V[09:59:57.666] Trying to fix unresolved name "NOTE_C5" in scopes: []
V[09:59:57.666] Dex query tree: false
V[09:59:57.666] Dex query tree: false
V[09:59:57.666] Trying to fix unresolved name "NOTE_D5" in scopes: []
V[09:59:57.666] Dex query tree: false
V[09:59:57.666] Dex query tree: false
V[09:59:57.667] Trying to fix unresolved name "NOTE_E5" in scopes: []
V[09:59:57.667] Dex query tree: false
V[09:59:57.667] Dex query tree: false
V[09:59:57.668] Trying to fix unresolved name "NOTE_F5" in scopes: []
V[09:59:57.668] Dex query tree: false
V[09:59:57.668] Dex query tree: false
V[09:59:57.668] Trying to fix unresolved name "NOTE_G5" in scopes: []
V[09:59:57.668] Dex query tree: false
V[09:59:57.668] Dex query tree: false
V[09:59:57.668] Trying to fix unresolved name "NOTE_A5" in scopes: []
V[09:59:57.669] Trying to fix unresolved name "NOTE_B5" in scopes: []
V[09:59:57.669] Trying to fix unresolved name "NOTE_C6" in scopes: []
V[09:59:57.670] ASTWorker running DocumentSymbols on version 6 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:57.670] --> reply:textDocument/documentSymbol("15") 112 ms
V[09:59:57.670] >>> {"id":"15","jsonrpc":"2.0","result":[{"detail":"int[]","kind":13,"name":"melody","range":{"end":{"character":12,"line":4},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

I[09:59:57.670] Skipping rebuild of the AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp, inputs are the same.
V[09:59:57.671] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 6:
  symbol slab: 4 symbols, 5152 bytes
  ref slab: 6 symbols, 12 refs, 4376 bytes
  relations slab: 0 relations, 24 bytes
V[09:59:57.672] Build dynamic index for main-file symbols with estimated memory usage of 13400 bytes
I[09:59:57.672] --> textDocument/publishDiagnostics
V[09:59:57.672] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[{"code":"pp_file_not_found","message":"'pitches.h' file not found","range":{"end":{"character":20,"line":3},"start":{"character":9,"line":3}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C5'","range":{"end":{"character":7,"line":5},"start":{"character":0,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_D5'","range":{"end":{"character":16,"line":5},"start":{"character":9,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_E5'","range":{"end":{"character":25,"line":5},"start":{"character":18,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_F5'","range":{"end":{"character":34,"line":5},"start":{"character":27,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_G5'","range":{"end":{"character":43,"line":5},"start":{"character":36,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_A5'","range":{"end":{"character":52,"line":5},"start":{"character":45,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_B5'","range":{"end":{"character":61,"line":5},"start":{"character":54,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C6'","range":{"end":{"character":70,"line":5},"start":{"character":63,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"}],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":6}}

V[09:59:57.777] <<< {"id":"16","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":6,"line":16},"start":{"character":6,"line":16}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:57.777] <-- textDocument/codeAction("16")
V[09:59:57.777] ASTWorker running EnumerateTweaks on version 6 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:57.777] --> reply:textDocument/codeAction("16") 0 ms
V[09:59:57.777] >>> {"id":"16","jsonrpc":"2.0","result":[]}

V[09:59:57.910] <<< {"id":"17","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:57.910] <-- textDocument/documentSymbol("17")
V[09:59:57.910] ASTWorker running DocumentSymbols on version 6 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:57.910] --> reply:textDocument/documentSymbol("17") 0 ms
V[09:59:57.911] >>> {"id":"17","jsonrpc":"2.0","result":[{"detail":"int[]","kind":13,"name":"melody","range":{"end":{"character":12,"line":4},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

V[09:59:57.936] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"range":{"end":{"character":6,"line":16},"start":{"character":6,"line":16}},"text":"4"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":7}}}

I[09:59:57.936] <-- textDocument/didChange
V[09:59:57.937] <<< {"id":"18","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:57.937] <-- textDocument/documentSymbol("18")
I[09:59:57.938] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 7 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[09:59:57.962] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[09:59:57.970] Reusing preamble version 1 for version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
V[09:59:57.986] ASTWorker rebuilding evicted AST to run DocumentSymbols: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 7
V[09:59:58.034] Trying to fix unresolved name "NOTE_C5" in scopes: []
V[09:59:58.034] Dex query tree: false
V[09:59:58.034] Dex query tree: false
V[09:59:58.035] Trying to fix unresolved name "NOTE_D5" in scopes: []
V[09:59:58.035] Dex query tree: false
V[09:59:58.035] Dex query tree: false
V[09:59:58.035] Trying to fix unresolved name "NOTE_E5" in scopes: []
V[09:59:58.035] Dex query tree: false
V[09:59:58.035] Dex query tree: false
V[09:59:58.036] Trying to fix unresolved name "NOTE_F5" in scopes: []
V[09:59:58.036] Dex query tree: false
V[09:59:58.036] Dex query tree: false
V[09:59:58.036] Trying to fix unresolved name "NOTE_G5" in scopes: []
V[09:59:58.036] Dex query tree: false
V[09:59:58.036] Dex query tree: false
V[09:59:58.037] Trying to fix unresolved name "NOTE_A5" in scopes: []
V[09:59:58.037] Trying to fix unresolved name "NOTE_B5" in scopes: []
V[09:59:58.037] Trying to fix unresolved name "NOTE_C6" in scopes: []
V[09:59:58.038] ASTWorker running DocumentSymbols on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:58.038] --> reply:textDocument/documentSymbol("18") 101 ms
V[09:59:58.038] >>> {"id":"18","jsonrpc":"2.0","result":[{"detail":"int[]","kind":13,"name":"melody","range":{"end":{"character":12,"line":4},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

I[09:59:58.038] Skipping rebuild of the AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp, inputs are the same.
V[09:59:58.039] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 7:
  symbol slab: 4 symbols, 5152 bytes
  ref slab: 6 symbols, 12 refs, 4376 bytes
  relations slab: 0 relations, 24 bytes
V[09:59:58.039] Build dynamic index for main-file symbols with estimated memory usage of 13400 bytes
I[09:59:58.039] --> textDocument/publishDiagnostics
V[09:59:58.039] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[{"code":"pp_file_not_found","message":"'pitches.h' file not found","range":{"end":{"character":20,"line":3},"start":{"character":9,"line":3}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C5'","range":{"end":{"character":7,"line":5},"start":{"character":0,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_D5'","range":{"end":{"character":16,"line":5},"start":{"character":9,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_E5'","range":{"end":{"character":25,"line":5},"start":{"character":18,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_F5'","range":{"end":{"character":34,"line":5},"start":{"character":27,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_G5'","range":{"end":{"character":43,"line":5},"start":{"character":36,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_A5'","range":{"end":{"character":52,"line":5},"start":{"character":45,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_B5'","range":{"end":{"character":61,"line":5},"start":{"character":54,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C6'","range":{"end":{"character":70,"line":5},"start":{"character":63,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"}],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":7}}

V[09:59:58.171] <<< {"id":"19","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":7,"line":16},"start":{"character":7,"line":16}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[09:59:58.171] <-- textDocument/codeAction("19")
V[09:59:58.171] ASTWorker running EnumerateTweaks on version 7 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[09:59:58.171] --> reply:textDocument/codeAction("19") 0 ms
V[09:59:58.171] >>> {"id":"19","jsonrpc":"2.0","result":[]}

V[10:00:00.663] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:00:00.663] <-- textDocument/didSave
I[10:00:00.663] File version went from 7 to 7
V[10:00:00.663] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\n\n#include \"pitches.h\"// notes in the melody:\nint melody[] = {\nNOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};\nint duration = 500;  // 500 miliseconds \n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup();\n#line 7 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid loop();\n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup() {  }\nvoid loop() {\nfor (int thisNote = 0; thisNote < 12; thisNote++) {\n// pin12 output the voice, every scale is 0.5 sencond \ntone(14, melody[thisNote], duration);\ndelay(100);\n// Output the voice after several minutes\ndelay(100);\n} // restart after two seconds \ndelay(200);\n}\n\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":8}}}

I[10:00:00.663] <-- textDocument/didChange
V[10:00:00.663] ASTWorker skipping Update (7) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:00:00.736] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 8 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[10:00:00.760] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[10:00:00.767] Reusing preamble version 1 for version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
V[10:00:14.753] <<< {"id":"20","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":7,"line":16},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:00:14.753] <-- textDocument/hover("20")
V[10:00:14.756] ASTWorker running Hover on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:00:14.765] --> reply:textDocument/hover("20") 12 ms
V[10:00:14.765] >>> {"id":"20","jsonrpc":"2.0","result":{"contents":{"kind":"markdown","value":"### function `tone`  \n\n---\n→ `void`  \nParameters:  \n- `uint8_t _pin`\n- `unsigned int frequency`\n- `unsigned long duration = 0`\n\nfrequency (in hertz) and duration (in milliseconds).  \n\n---\n```cpp\nvoid tone(uint8_t _pin, unsigned int frequency, unsigned long duration = 0)\n```"},"range":{"end":{"character":8,"line":16},"start":{"character":7,"line":16}}}}

V[10:00:15.048] <<< {"id":"21","jsonrpc":"2.0","method":"textDocument/documentHighlight","params":{"position":{"character":7,"line":16},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:00:15.048] <-- textDocument/documentHighlight("21")
V[10:00:15.048] ASTWorker running Highlights on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:00:15.048] --> reply:textDocument/documentHighlight("21") 0 ms
V[10:00:15.048] >>> {"id":"21","jsonrpc":"2.0","result":[{"kind":1,"range":{"end":{"character":4,"line":16},"start":{"character":0,"line":16}}}]}

V[10:00:15.401] <<< {"id":"22","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":7,"line":16},"start":{"character":6,"line":16}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:00:15.401] <-- textDocument/codeAction("22")
V[10:00:15.402] ASTWorker running EnumerateTweaks on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:00:15.402] --> reply:textDocument/codeAction("22") 0 ms
V[10:00:15.402] >>> {"id":"22","jsonrpc":"2.0","result":[{"command":{"arguments":[{"file":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","selection":{"end":{"character":7,"line":16},"start":{"character":6,"line":16}},"tweakID":"ExtractVariable"}],"command":"clangd.applyTweak","title":"Extract subexpression to variable"},"kind":"refactor","title":"Extract subexpression to variable"}]}

V[10:00:15.694] <<< {"id":"23","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":5,"line":16},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:00:15.694] <-- textDocument/hover("23")
V[10:00:15.695] ASTWorker running Hover on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:00:15.698] --> reply:textDocument/hover("23") 3 ms
V[10:00:15.698] >>> {"id":"23","jsonrpc":"2.0","result":null}

V[10:00:16.303] <<< {"id":"24","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:00:16.303] <-- textDocument/documentSymbol("24")
V[10:00:16.303] ASTWorker running DocumentSymbols on version 8 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:00:16.303] --> reply:textDocument/documentSymbol("24") 0 ms
V[10:00:16.304] >>> {"id":"24","jsonrpc":"2.0","result":[{"detail":"int[]","kind":13,"name":"melody","range":{"end":{"character":12,"line":4},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

V[10:00:16.328] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"range":{"end":{"character":7,"line":16},"start":{"character":6,"line":16}},"text":"2"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":9}}}

I[10:00:16.328] <-- textDocument/didChange
V[10:00:16.329] <<< {"id":"25","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:00:16.329] <-- textDocument/documentSymbol("25")
I[10:00:16.331] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\compile_commands.json
V[10:00:16.331] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764
I[10:00:16.331] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 9 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
I[10:00:16.334] --> window/workDoneProgress/create(2)
V[10:00:16.334] >>> {"id":2,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[10:00:16.334] Enqueueing 26 commands for indexing
V[10:00:16.334] <<< {"id":2,"jsonrpc":"2.0","result":null}

I[10:00:16.334] <-- reply(2)
I[10:00:16.334] --> $/progress
V[10:00:16.334] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[10:00:16.334] --> $/progress
V[10:00:16.334] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[10:00:16.357] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[10:00:16.359] BackgroundIndex: building version 4 after loading index from disk
V[10:00:16.365] Reusing preamble version 1 for version 9 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
V[10:00:16.369] BackgroundIndex: serving version 4 (1767862 bytes)
V[10:00:16.381] ASTWorker rebuilding evicted AST to run DocumentSymbols: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 9
I[10:00:16.382] --> $/progress
V[10:00:16.382] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[10:00:16.382] --> $/progress
V[10:00:16.382] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[10:00:16.432] Trying to fix unresolved name "NOTE_C5" in scopes: []
V[10:00:16.432] Dex query tree: false
V[10:00:16.432] Dex query tree: false
V[10:00:16.432] Trying to fix unresolved name "NOTE_D5" in scopes: []
V[10:00:16.432] Dex query tree: false
V[10:00:16.432] Dex query tree: false
V[10:00:16.433] Trying to fix unresolved name "NOTE_E5" in scopes: []
V[10:00:16.433] Dex query tree: false
V[10:00:16.433] Dex query tree: false
V[10:00:16.433] Trying to fix unresolved name "NOTE_F5" in scopes: []
V[10:00:16.433] Dex query tree: false
V[10:00:16.433] Dex query tree: false
V[10:00:16.434] Trying to fix unresolved name "NOTE_G5" in scopes: []
V[10:00:16.434] Dex query tree: false
V[10:00:16.434] Dex query tree: false
V[10:00:16.434] Trying to fix unresolved name "NOTE_A5" in scopes: []
V[10:00:16.434] Trying to fix unresolved name "NOTE_B5" in scopes: []
V[10:00:16.435] Trying to fix unresolved name "NOTE_C6" in scopes: []
V[10:00:16.436] ASTWorker running DocumentSymbols on version 9 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:00:16.436] --> reply:textDocument/documentSymbol("25") 106 ms
V[10:00:16.436] >>> {"id":"25","jsonrpc":"2.0","result":[{"detail":"int[]","kind":13,"name":"melody","range":{"end":{"character":12,"line":4},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

I[10:00:16.436] Skipping rebuild of the AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp, inputs are the same.
V[10:00:16.437] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 9:
  symbol slab: 4 symbols, 5152 bytes
  ref slab: 6 symbols, 12 refs, 4376 bytes
  relations slab: 0 relations, 24 bytes
V[10:00:16.437] Build dynamic index for main-file symbols with estimated memory usage of 13400 bytes
I[10:00:16.437] --> textDocument/publishDiagnostics
V[10:00:16.437] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[{"code":"pp_file_not_found","message":"'pitches.h' file not found","range":{"end":{"character":20,"line":3},"start":{"character":9,"line":3}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C5'","range":{"end":{"character":7,"line":5},"start":{"character":0,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_D5'","range":{"end":{"character":16,"line":5},"start":{"character":9,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_E5'","range":{"end":{"character":25,"line":5},"start":{"character":18,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_F5'","range":{"end":{"character":34,"line":5},"start":{"character":27,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_G5'","range":{"end":{"character":43,"line":5},"start":{"character":36,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_A5'","range":{"end":{"character":52,"line":5},"start":{"character":45,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_B5'","range":{"end":{"character":61,"line":5},"start":{"character":54,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C6'","range":{"end":{"character":70,"line":5},"start":{"character":63,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"}],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":9}}

V[10:00:16.557] <<< {"id":"26","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":7,"line":16},"start":{"character":7,"line":16}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:00:16.557] <-- textDocument/codeAction("26")
V[10:00:16.557] ASTWorker running EnumerateTweaks on version 9 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:00:16.557] --> reply:textDocument/codeAction("26") 0 ms
V[10:00:16.557] >>> {"id":"26","jsonrpc":"2.0","result":[]}

V[10:00:17.466] <<< {"id":"27","jsonrpc":"2.0","method":"textDocument/documentHighlight","params":{"position":{"character":19,"line":20},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:00:17.466] <-- textDocument/documentHighlight("27")
V[10:00:17.466] ASTWorker running Highlights on version 9 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:00:17.466] --> reply:textDocument/documentHighlight("27") 0 ms
V[10:00:17.466] >>> {"id":"27","jsonrpc":"2.0","result":[]}

V[10:00:17.720] <<< {"id":"28","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":19,"line":20},"start":{"character":19,"line":20}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:00:17.720] <-- textDocument/codeAction("28")
V[10:00:17.720] ASTWorker running EnumerateTweaks on version 9 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:00:17.720] --> reply:textDocument/codeAction("28") 0 ms
V[10:00:17.720] >>> {"id":"28","jsonrpc":"2.0","result":[]}

V[10:00:18.138] <<< {"id":"29","jsonrpc":"2.0","method":"textDocument/definition","params":{"position":{"character":19,"line":20},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:00:18.138] <-- textDocument/definition("29")
V[10:00:18.139] ASTWorker running Definitions on version 9 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:00:18.139] --> reply:textDocument/definition("29") 0 ms
V[10:00:18.139] >>> {"id":"29","jsonrpc":"2.0","result":[]}

V[10:00:18.402] <<< {"id":"30","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:00:18.402] <-- textDocument/documentSymbol("30")
V[10:00:18.402] ASTWorker running DocumentSymbols on version 9 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:00:18.402] --> reply:textDocument/documentSymbol("30") 0 ms
V[10:00:18.402] >>> {"id":"30","jsonrpc":"2.0","result":[{"detail":"int[]","kind":13,"name":"melody","range":{"end":{"character":12,"line":4},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

V[10:00:18.429] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"range":{"end":{"character":7,"line":16},"start":{"character":6,"line":16}},"text":"4"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":10}}}

I[10:00:18.429] <-- textDocument/didChange
I[10:00:18.501] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 10 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[10:00:18.532] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[10:00:18.541] Reusing preamble version 1 for version 10 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
V[10:00:18.592] Trying to fix unresolved name "NOTE_C5" in scopes: []
V[10:00:18.592] Dex query tree: false
V[10:00:18.592] Dex query tree: false
V[10:00:18.593] Trying to fix unresolved name "NOTE_D5" in scopes: []
V[10:00:18.593] Dex query tree: false
V[10:00:18.593] Dex query tree: false
V[10:00:18.593] Trying to fix unresolved name "NOTE_E5" in scopes: []
V[10:00:18.593] Dex query tree: false
V[10:00:18.593] Dex query tree: false
V[10:00:18.594] Trying to fix unresolved name "NOTE_F5" in scopes: []
V[10:00:18.594] Dex query tree: false
V[10:00:18.594] Dex query tree: false
V[10:00:18.594] <<< {"id":"31","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:00:18.594] <-- textDocument/documentSymbol("31")
V[10:00:18.594] Trying to fix unresolved name "NOTE_G5" in scopes: []
V[10:00:18.594] Dex query tree: false
V[10:00:18.594] Dex query tree: false
V[10:00:18.595] Trying to fix unresolved name "NOTE_A5" in scopes: []
V[10:00:18.595] Trying to fix unresolved name "NOTE_B5" in scopes: []
V[10:00:18.596] Trying to fix unresolved name "NOTE_C6" in scopes: []
V[10:00:18.597] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 10:
  symbol slab: 4 symbols, 5152 bytes
  ref slab: 6 symbols, 12 refs, 4376 bytes
  relations slab: 0 relations, 24 bytes
V[10:00:18.597] Build dynamic index for main-file symbols with estimated memory usage of 13400 bytes
I[10:00:18.597] --> textDocument/publishDiagnostics
V[10:00:18.598] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[{"code":"pp_file_not_found","message":"'pitches.h' file not found","range":{"end":{"character":20,"line":3},"start":{"character":9,"line":3}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C5'","range":{"end":{"character":7,"line":5},"start":{"character":0,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_D5'","range":{"end":{"character":16,"line":5},"start":{"character":9,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_E5'","range":{"end":{"character":25,"line":5},"start":{"character":18,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_F5'","range":{"end":{"character":34,"line":5},"start":{"character":27,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_G5'","range":{"end":{"character":43,"line":5},"start":{"character":36,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_A5'","range":{"end":{"character":52,"line":5},"start":{"character":45,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_B5'","range":{"end":{"character":61,"line":5},"start":{"character":54,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C6'","range":{"end":{"character":70,"line":5},"start":{"character":63,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"}],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":10}}

V[10:00:18.598] ASTWorker running DocumentSymbols on version 10 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:00:18.598] --> reply:textDocument/documentSymbol("31") 3 ms
V[10:00:18.598] >>> {"id":"31","jsonrpc":"2.0","result":[{"detail":"int[]","kind":13,"name":"melody","range":{"end":{"character":12,"line":4},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

V[10:00:18.623] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"range":{"end":{"character":7,"line":16},"start":{"character":5,"line":16}},"text":"12"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":11}}}

I[10:00:18.623] <-- textDocument/didChange
I[10:00:18.688] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 11 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[10:00:18.713] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[10:00:18.721] Reusing preamble version 1 for version 11 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
V[10:00:18.773] Trying to fix unresolved name "NOTE_C5" in scopes: []
V[10:00:18.773] Dex query tree: false
V[10:00:18.773] Dex query tree: false
V[10:00:18.774] Trying to fix unresolved name "NOTE_D5" in scopes: []
V[10:00:18.774] Dex query tree: false
V[10:00:18.774] Dex query tree: false
V[10:00:18.774] Trying to fix unresolved name "NOTE_E5" in scopes: []
V[10:00:18.774] Dex query tree: false
V[10:00:18.774] Dex query tree: false
V[10:00:18.774] Trying to fix unresolved name "NOTE_F5" in scopes: []
V[10:00:18.774] Dex query tree: false
V[10:00:18.774] Dex query tree: false
V[10:00:18.775] Trying to fix unresolved name "NOTE_G5" in scopes: []
V[10:00:18.775] Dex query tree: false
V[10:00:18.775] Dex query tree: false
V[10:00:18.775] Trying to fix unresolved name "NOTE_A5" in scopes: []
V[10:00:18.776] Trying to fix unresolved name "NOTE_B5" in scopes: []
V[10:00:18.776] Trying to fix unresolved name "NOTE_C6" in scopes: []
V[10:00:18.778] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 11:
  symbol slab: 4 symbols, 5152 bytes
  ref slab: 6 symbols, 12 refs, 4376 bytes
  relations slab: 0 relations, 24 bytes
V[10:00:18.778] Build dynamic index for main-file symbols with estimated memory usage of 13400 bytes
I[10:00:18.778] --> textDocument/publishDiagnostics
V[10:00:18.778] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[{"code":"pp_file_not_found","message":"'pitches.h' file not found","range":{"end":{"character":20,"line":3},"start":{"character":9,"line":3}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C5'","range":{"end":{"character":7,"line":5},"start":{"character":0,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_D5'","range":{"end":{"character":16,"line":5},"start":{"character":9,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_E5'","range":{"end":{"character":25,"line":5},"start":{"character":18,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_F5'","range":{"end":{"character":34,"line":5},"start":{"character":27,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_G5'","range":{"end":{"character":43,"line":5},"start":{"character":36,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_A5'","range":{"end":{"character":52,"line":5},"start":{"character":45,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_B5'","range":{"end":{"character":61,"line":5},"start":{"character":54,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"},{"code":"undeclared_var_use","message":"Use of undeclared identifier 'NOTE_C6'","range":{"end":{"character":70,"line":5},"start":{"character":63,"line":5}},"relatedInformation":[],"severity":1,"source":"clang"}],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":11}}

V[10:00:18.848] <<< {"id":"32","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":7,"line":16},"start":{"character":5,"line":16}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:00:18.848] <-- textDocument/codeAction("32")
V[10:00:18.848] ASTWorker running EnumerateTweaks on version 11 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:00:18.848] --> reply:textDocument/codeAction("32") 0 ms
V[10:00:18.848] >>> {"id":"32","jsonrpc":"2.0","result":[{"command":{"arguments":[{"file":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","selection":{"end":{"character":7,"line":16},"start":{"character":5,"line":16}},"tweakID":"ExtractVariable"}],"command":"clangd.applyTweak","title":"Extract subexpression to variable"},"kind":"refactor","title":"Extract subexpression to variable"}]}

V[10:00:21.358] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:00:21.358] <-- textDocument/didSave
I[10:00:21.358] File version went from 11 to 11
V[10:00:21.358] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\n\n#include \"pitches.h\"// notes in the melody:\nint melody[] = {\nNOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};\nint duration = 500;  // 500 miliseconds \n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup();\n#line 7 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid loop();\n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup() {  }\nvoid loop() {\nfor (int thisNote = 0; thisNote < 12; thisNote++) {\n// pin12 output the voice, every scale is 0.5 sencond \ntone(12, melody[thisNote], duration);\ndelay(100);\n// Output the voice after several minutes\ndelay(100);\n} // restart after two seconds \ndelay(200);\n}\n\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":12}}}

I[10:00:21.358] <-- textDocument/didChange
V[10:00:21.358] ASTWorker skipping Update (11) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:00:21.421] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\compile_commands.json
V[10:00:21.421] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764
I[10:00:21.421] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 12 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
I[10:00:21.425] --> window/workDoneProgress/create(3)
V[10:00:21.425] >>> {"id":3,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[10:00:21.425] Enqueueing 26 commands for indexing
V[10:00:21.425] <<< {"id":3,"jsonrpc":"2.0","result":null}

I[10:00:21.425] <-- reply(3)
I[10:00:21.425] --> $/progress
V[10:00:21.425] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[10:00:21.425] --> $/progress
V[10:00:21.425] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[10:00:21.447] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[10:00:21.448] BackgroundIndex: building version 5 after loading index from disk
V[10:00:21.455] Reusing preamble version 1 for version 12 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
V[10:00:21.459] BackgroundIndex: serving version 5 (1767862 bytes)
I[10:00:21.471] --> $/progress
V[10:00:21.471] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[10:00:21.471] --> $/progress
V[10:00:21.471] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[10:02:07.144] <<< {"id":"33","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":11,"line":12},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:02:07.144] <-- textDocument/hover("33")
V[10:02:07.147] ASTWorker running Hover on version 12 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:02:07.150] --> reply:textDocument/hover("33") 6 ms
V[10:02:07.150] >>> {"id":"33","jsonrpc":"2.0","result":null}

V[10:02:10.636] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:02:10.636] <-- textDocument/didSave
I[10:02:10.636] File version went from 12 to 12
V[10:02:10.636] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\n\n#include \"pitches.h\"// notes in the melody:\nint melody[] = {\nNOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};\nint duration = 500;  // 500 miliseconds \n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup();\n#line 7 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid loop();\n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup() {  }\nvoid loop() {\nfor (int thisNote = 0; thisNote < 12; thisNote++) {\n// pin12 output the voice, every scale is 0.5 sencond \ntone(12, melody[thisNote], duration);\ndelay(100);\n// Output the voice after several minutes\ndelay(100);\n} // restart after two seconds \ndelay(200);\n}\n\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":13}}}

I[10:02:10.636] <-- textDocument/didChange
V[10:02:10.636] ASTWorker skipping Update (12) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:02:10.697] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\compile_commands.json
V[10:02:10.697] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764
I[10:02:10.697] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 13 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
I[10:02:10.700] --> window/workDoneProgress/create(4)
V[10:02:10.700] >>> {"id":4,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[10:02:10.700] Enqueueing 26 commands for indexing
V[10:02:10.700] <<< {"id":4,"jsonrpc":"2.0","result":null}

I[10:02:10.700] <-- reply(4)
I[10:02:10.700] --> $/progress
V[10:02:10.700] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[10:02:10.700] --> $/progress
V[10:02:10.700] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[10:02:10.721] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[10:02:10.723] BackgroundIndex: building version 6 after loading index from disk
V[10:02:10.729] Reusing preamble version 1 for version 13 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
V[10:02:10.733] BackgroundIndex: serving version 6 (1767862 bytes)
I[10:02:10.745] --> $/progress
V[10:02:10.745] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[10:02:10.745] --> $/progress
V[10:02:10.745] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[10:02:25.679] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:02:25.679] <-- textDocument/didSave
I[10:02:25.679] File version went from 13 to 13
V[10:02:25.679] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\n\n#include \"pitches.h\"// notes in the melody:\nint melody[] = {\nNOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};\nint duration = 500;  // 500 miliseconds \n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup();\n#line 7 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid loop();\n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup() {  }\nvoid loop() {\nfor (int thisNote = 0; thisNote < 12; thisNote++) {\n// pin12 output the voice, every scale is 0.5 sencond \ntone(12, melody[thisNote], duration);\ndelay(100);\n// Output the voice after several minutes\ndelay(100);\n} // restart after two seconds \ndelay(200);\n}\n\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp","version":14}}}

I[10:02:25.679] <-- textDocument/didChange
V[10:02:25.679] ASTWorker skipping Update (13) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:02:25.745] Reloaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\compile_commands.json
V[10:02:25.745] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764
I[10:02:25.745] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp version 14 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
I[10:02:25.748] --> window/workDoneProgress/create(5)
V[10:02:25.748] >>> {"id":5,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[10:02:25.748] Enqueueing 26 commands for indexing
V[10:02:25.749] <<< {"id":5,"jsonrpc":"2.0","result":null}

I[10:02:25.749] <-- reply(5)
I[10:02:25.749] --> $/progress
V[10:02:25.749] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[10:02:25.749] --> $/progress
V[10:02:25.749] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[10:02:25.770] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server4028959764\\sketch\\5_Active_buzzer.ino.cpp"
V[10:02:25.771] BackgroundIndex: building version 7 after loading index from disk
V[10:02:25.777] Reusing preamble version 1 for version 14 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
V[10:02:25.781] BackgroundIndex: serving version 7 (1767862 bytes)
I[10:02:25.794] --> $/progress
V[10:02:25.794] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

I[10:02:25.794] --> $/progress
V[10:02:25.794] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[10:02:47.654] <<< {"id":"34","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":11,"line":21},"start":{"character":11,"line":21}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:02:47.654] <-- textDocument/codeAction("34")
V[10:02:47.658] ASTWorker running EnumerateTweaks on version 14 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:02:47.658] --> reply:textDocument/codeAction("34") 3 ms
V[10:02:47.658] >>> {"id":"34","jsonrpc":"2.0","result":[]}

V[10:02:53.272] <<< {"id":"35","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":1,"line":22},"start":{"character":1,"line":22}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:02:53.272] <-- textDocument/codeAction("35")
V[10:02:53.275] ASTWorker running EnumerateTweaks on version 14 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:02:53.275] --> reply:textDocument/codeAction("35") 3 ms
V[10:02:53.275] >>> {"id":"35","jsonrpc":"2.0","result":[]}

V[10:03:35.476] <<< {"id":"36","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":34,"line":3},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server4028959764/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:03:35.476] <-- textDocument/hover("36")
V[10:03:35.480] ASTWorker running Hover on version 14 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server4028959764\sketch\5_Active_buzzer.ino.cpp
I[10:03:35.483] --> reply:textDocument/hover("36") 6 ms
V[10:03:35.483] >>> {"id":"36","jsonrpc":"2.0","result":null}

V[10:03:36.652] <<< {"id":"37","jsonrpc":"2.0","method":"shutdown","params":null}

I[10:03:36.652] <-- shutdown("37")
I[10:03:36.652] --> reply:shutdown("37") 0 ms
V[10:03:36.652] >>> {"id":"37","jsonrpc":"2.0","result":null}








Started logging.
I[10:03:50.772] clangd version 14.0.0
I[10:03:50.774] Features: windows
I[10:03:50.774] PID: 3676
I[10:03:50.774] Working directory: g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 5_Active_buzzer\5_Active_buzzer
I[10:03:50.774] argv[0]: d:\Program Files\Arduino IDE\resources\app\node_modules\arduino-ide-extension\build\clangd.exe
I[10:03:50.774] argv[1]: -log=verbose
I[10:03:50.774] argv[2]: --compile-commands-dir=C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420
I[10:03:50.774] argv[3]: -query-driver=C:\Users\Administrator\AppData\Local\Arduino15\packages\**
V[10:03:50.781] User config file is C:\Users\Administrator\AppData\Local\clangd\config.yaml
I[10:03:50.781] Starting LSP over stdin/stdout
V[10:03:50.781] <<< {"id":"1","jsonrpc":"2.0","method":"initialize","params":{"capabilities":{"textDocument":{"codeAction":{"codeActionLiteralSupport":{"codeActionKind":{"valueSet":["","quickfix","refactor","refactor.extract","refactor.inline","refactor.rewrite","source","source.organizeImports"]}},"dynamicRegistration":true,"isPreferredSupport":true},"codeLens":{"dynamicRegistration":true},"colorProvider":{"dynamicRegistration":true},"completion":{"completionItem":{"commitCharactersSupport":true,"deprecatedSupport":true,"documentationFormat":["markdown","plaintext"],"preselectSupport":true,"snippetSupport":true,"tagSupport":{"valueSet":[1]}},"completionItemKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25]},"contextSupport":true,"dynamicRegistration":true},"declaration":{"dynamicRegistration":true,"linkSupport":true},"definition":{"dynamicRegistration":true,"linkSupport":true},"documentHighlight":{"dynamicRegistration":true},"documentLink":{"dynamicRegistration":true,"tooltipSupport":true},"documentSymbol":{"dynamicRegistration":true,"hierarchicalDocumentSymbolSupport":true,"symbolKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26]}},"foldingRange":{"dynamicRegistration":true,"lineFoldingOnly":true,"rangeLimit":5000},"formatting":{"dynamicRegistration":true},"hover":{"contentFormat":["markdown","plaintext"],"dynamicRegistration":true},"implementation":{"dynamicRegistration":true,"linkSupport":true},"onTypeFormatting":{"dynamicRegistration":true},"publishDiagnostics":{"relatedInformation":true,"tagSupport":{"valueSet":[1,2]}},"rangeFormatting":{"dynamicRegistration":true},"references":{"dynamicRegistration":true},"rename":{"dynamicRegistration":true,"prepareSupport":true},"selectionRange":{"dynamicRegistration":true},"signatureHelp":{"contextSupport":true,"dynamicRegistration":true,"signatureInformation":{"documentationFormat":["markdown","plaintext"],"parameterInformation":{"labelOffsetSupport":true}}},"synchronization":{"didSave":true,"dynamicRegistration":true,"willSave":true,"willSaveWaitUntil":true},"typeDefinition":{"dynamicRegistration":true,"linkSupport":true}},"window":{"workDoneProgress":true},"workspace":{"applyEdit":true,"configuration":true,"didChangeConfiguration":{"dynamicRegistration":true},"didChangeWatchedFiles":{"dynamicRegistration":true},"executeCommand":{"dynamicRegistration":true},"symbol":{"dynamicRegistration":true,"symbolKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26]}},"workspaceEdit":{"documentChanges":true,"failureHandling":"textOnlyTransactional","resourceOperations":["create","rename","delete"]},"workspaceFolders":true}},"clientInfo":{"name":"vscode","version":"1.53.2"},"initializationOptions":{},"processId":8684,"rootPath":"C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420\\sketch","rootUri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch","trace":"off","workspaceFolders":[{"name":"5_Active_buzzer","uri":"file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%205_Active_buzzer/5_Active_buzzer"}]}}

I[10:03:50.781] <-- initialize("1")
I[10:03:50.843] --> reply:initialize("1") 62 ms
V[10:03:50.843] >>> {"id":"1","jsonrpc":"2.0","result":{"capabilities":{"astProvider":true,"callHierarchyProvider":true,"clangdInlayHintsProvider":true,"codeActionProvider":{"codeActionKinds":["quickfix","refactor","info"]},"compilationDatabase":{"automaticReload":true},"completionProvider":{"allCommitCharacters":[" ","\t","(",")","[","]","{","}","<",">",":",";",",","+","-","/","*","%","^","&","#","?",".","=","\"","'","|"],"resolveProvider":false,"triggerCharacters":[".","<",">",":","\"","/","*"]},"declarationProvider":true,"definitionProvider":true,"documentFormattingProvider":true,"documentHighlightProvider":true,"documentLinkProvider":{"resolveProvider":false},"documentOnTypeFormattingProvider":{"firstTriggerCharacter":"\n","moreTriggerCharacter":[]},"documentRangeFormattingProvider":true,"documentSymbolProvider":true,"executeCommandProvider":{"commands":["clangd.applyFix","clangd.applyTweak"]},"hoverProvider":true,"implementationProvider":true,"memoryUsageProvider":true,"referencesProvider":true,"renameProvider":{"prepareProvider":true},"selectionRangeProvider":true,"semanticTokensProvider":{"full":{"delta":true},"legend":{"tokenModifiers":["declaration","deprecated","deduced","readonly","static","abstract","virtual","dependentName","defaultLibrary","usedAsMutableReference","functionScope","classScope","fileScope","globalScope"],"tokenTypes":["variable","variable","parameter","function","method","function","property","variable","class","interface","enum","enumMember","type","type","unknown","namespace","typeParameter","concept","type","macro","comment"]},"range":false},"signatureHelpProvider":{"triggerCharacters":["(",")","{","}","<",">",","]},"textDocumentSync":{"change":2,"openClose":true,"save":true},"typeDefinitionProvider":true,"typeHierarchyProvider":true,"workspaceSymbolProvider":true},"serverInfo":{"name":"clangd","version":"clangd version 14.0.0 windows x86_64-pc-windows-msvc"}}}

V[10:03:50.844] <<< {"jsonrpc":"2.0","method":"initialized","params":{}}

I[10:03:50.844] <-- initialized
V[10:03:50.851] <<< {"jsonrpc":"2.0","method":"textDocument/didOpen","params":{"textDocument":{"languageId":"cpp","text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\n\n#include \"pitches.h\"// notes in the melody:\nint melody[] = {\nNOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};\nint duration = 500;  // 500 miliseconds \n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup();\n#line 7 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid loop();\n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup() {  }\nvoid loop() {\nfor (int thisNote = 0; thisNote < 12; thisNote++) {\n// pin12 output the voice, every scale is 0.5 sencond \ntone(12, melody[thisNote], duration);\ndelay(100);\n// Output the voice after several minutes\ndelay(100);\n} // restart after two seconds \ndelay(200);\n}\n\n","uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp","version":1}}}

I[10:03:50.851] <-- textDocument/didOpen
V[10:03:50.855] config note at C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\.clangd:1:0: Parsing config fragment
V[10:03:50.855] config note at C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\.clangd:1:0: Parsed 1 fragments from file
V[10:03:50.855] Config fragment: compiling C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\.clangd:1 -> 0x00000270575076B0 (trusted=false)
I[10:03:50.856] --> textDocument/publishDiagnostics
V[10:03:50.856] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/.clangd"}}

I[10:03:50.857] Loaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\compile_commands.json
V[10:03:50.857] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420
I[10:03:50.860] --> window/workDoneProgress/create(0)
V[10:03:50.860] >>> {"id":0,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[10:03:50.860] Enqueueing 26 commands for indexing
V[10:03:50.861] <<< {"id":0,"jsonrpc":"2.0","result":null}

I[10:03:50.861] <-- reply(0)
I[10:03:50.861] --> $/progress
V[10:03:50.861] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[10:03:50.861] --> $/progress
V[10:03:50.861] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[10:03:50.862] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp
V[10:03:50.862] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp
V[10:03:50.862] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c
V[10:03:50.862] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c
V[10:03:50.862] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp
V[10:03:50.862] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp
V[10:03:50.862] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp
V[10:03:50.862] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp
V[10:03:50.863] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp
V[10:03:50.863] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp
V[10:03:50.863] Failed to load shard: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
V[10:03:50.863] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S
V[10:03:50.863] <<< {"jsonrpc":"2.0","method":"textDocument/didOpen","params":{"textDocument":{"languageId":"cpp","text":"#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\pitches.h\"\n/*************************************************\r\n* Public Constants\r\n*************************************************/\r\n\r\n#define NOTE_B0 31\r\n#define NOTE_C1 33\r\n#define NOTE_CS1 35\r\n#define NOTE_D1 37\r\n#define NOTE_DS1 39\r\n#define NOTE_E1 41\r\n#define NOTE_F1 44\r\n#define NOTE_FS1 46\r\n#define NOTE_G1 49\r\n#define NOTE_GS1 52\r\n#define NOTE_A1 55\r\n#define NOTE_AS1 58\r\n#define NOTE_B1 62\r\n#define NOTE_C2 65\r\n#define NOTE_CS2 69\r\n#define NOTE_D2 73\r\n#define NOTE_DS2 78\r\n#define NOTE_E2 82\r\n#define NOTE_F2 87\r\n#define NOTE_FS2 93\r\n#define NOTE_G2 98\r\n#define NOTE_GS2 104\r\n#define NOTE_A2 110\r\n#define NOTE_AS2 117\r\n#define NOTE_B2 123\r\n#define NOTE_C3 131\r\n#define NOTE_CS3 139\r\n#define NOTE_D3 147\r\n#define NOTE_DS3 156\r\n#define NOTE_E3 165\r\n#define NOTE_F3 175\r\n#define NOTE_FS3 185\r\n#define NOTE_G3 196\r\n#define NOTE_GS3 208\r\n#define NOTE_A3 220\r\n#define NOTE_AS3 233\r\n#define NOTE_B3 247\r\n#define NOTE_C4 262\r\n#define NOTE_CS4 277\r\n#define NOTE_D4 294\r\n#define NOTE_DS4 311\r\n#define NOTE_E4 330\r\n#define NOTE_F4 349\r\n#define NOTE_FS4 370\r\n#define NOTE_G4 392\r\n#define NOTE_GS4 415\r\n#define NOTE_A4 440\r\n#define NOTE_AS4 466\r\n#define NOTE_B4 494\r\n#define NOTE_C5 523\r\n#define NOTE_CS5 554\r\n#define NOTE_D5 587\r\n#define NOTE_DS5 622\r\n#define NOTE_E5 659\r\n#define NOTE_F5 698\r\n#define NOTE_FS5 740\r\n#define NOTE_G5 784\r\n#define NOTE_GS5 831\r\n#define NOTE_A5 880\r\n#define NOTE_AS5 932\r\n#define NOTE_B5 988\r\n#define NOTE_C6 1047\r\n#define NOTE_CS6 1109\r\n#define NOTE_D6 1175\r\n#define NOTE_DS6 1245\r\n#define NOTE_E6 1319\r\n#define NOTE_F6 1397\r\n#define NOTE_FS6 1480\r\n#define NOTE_G6 1568\r\n#define NOTE_GS6 1661\r\n#define NOTE_A6 1760\r\n#define NOTE_AS6 1865\r\n#define NOTE_B6 1976\r\n#define NOTE_C7 2093\r\n#define NOTE_CS7 2217\r\n#define NOTE_D7 2349\r\n#define NOTE_DS7 2489\r\n#define NOTE_E7 2637\r\n#define NOTE_F7 2794\r\n#define NOTE_FS7 2960\r\n#define NOTE_G7 3136\r\n#define NOTE_GS7 3322\r\n#define NOTE_A7 3520\r\n#define NOTE_AS7 3729\r\n#define NOTE_B7 3951\r\n#define NOTE_C8 4186\r\n#define NOTE_CS8 4435\r\n#define NOTE_D8 4699\r\n#define NOTE_DS8 4978\r\n","uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/pitches.h","version":1}}}

I[10:03:50.863] <-- textDocument/didOpen
V[10:03:50.863] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp
V[10:03:50.863] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp
V[10:03:50.863] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c
V[10:03:50.863] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp
V[10:03:50.863] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp
V[10:03:50.864] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp
V[10:03:50.864] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp
V[10:03:50.864] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c
V[10:03:50.864] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c
V[10:03:50.864] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp
V[10:03:50.865] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp
V[10:03:50.865] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp
V[10:03:50.865] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c
V[10:03:50.865] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c
V[10:03:50.868] <<< {"id":"2","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":0,"line":1},"start":{"character":0,"line":1}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/pitches.h"}}}

I[10:03:50.868] <-- textDocument/codeAction("2")
I[10:03:50.870] --> $/progress
V[10:03:50.870] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[10:03:50.870] --> $/progress
V[10:03:50.870] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[10:03:50.870] --> $/progress
V[10:03:50.870] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[10:03:50.870] --> $/progress
V[10:03:50.870] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[10:03:50.870] --> $/progress
V[10:03:50.870] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[10:03:50.871] --> $/progress
V[10:03:50.871] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[10:03:50.871] --> $/progress
V[10:03:50.871] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[10:03:50.871] --> $/progress
V[10:03:50.871] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

V[10:03:51.005] System include extraction: target extracted: "avr"
V[10:03:51.005] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:03:51.005] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:03:51.005] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:03:51.005] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
I[10:03:51.006] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp version 1 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420\\sketch\\5_Active_buzzer.ino.cpp"
V[10:03:51.012] System include extraction: target extracted: "avr"
V[10:03:51.012] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:03:51.012] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:03:51.012] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:03:51.012] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
I[10:03:51.013] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\pitches.h version 1 with command inferred from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -x c++-header -std=gnu++11 -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420\\sketch\\pitches.h"
V[10:03:51.022] System include extraction: target extracted: "avr"
V[10:03:51.022] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:03:51.022] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:03:51.022] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:03:51.022] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-gcc.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:03:51.025] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c (digest:=343A7ACAD5FD2414)
V[10:03:51.033] System include extraction: target extracted: "avr"
V[10:03:51.033] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:03:51.033] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:03:51.033] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:03:51.033] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-gcc.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:03:51.034] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c (digest:=0A36B38756A4F148)
V[10:03:51.037] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420\\sketch\\5_Active_buzzer.ino.cpp"
V[10:03:51.037] Building first preamble for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp version 1
V[10:03:51.041] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name pitches.h -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file pitches.d -MT pitches.o -module-file-deps -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++-header "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420\\sketch\\pitches.h"
V[10:03:51.041] Building first preamble for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\pitches.h version 1
V[10:03:51.063] System include extraction: target extracted: "avr"
V[10:03:51.063] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:03:51.063] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:03:51.063] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:03:51.063] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:03:51.065] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp (digest:=55BA50D4FF04E609)
V[10:03:51.066] indexed preamble AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\pitches.h version 1:
  symbol slab: 93 symbols, 25800 bytes
  ref slab: 0 symbols, 0 refs, 136 bytes
  relations slab: 0 relations, 24 bytes
V[10:03:51.067] System include extraction: target extracted: "avr"
V[10:03:51.067] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:03:51.067] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:03:51.067] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

V[10:03:51.067] Build dynamic index for header symbols with estimated memory usage of 113684 bytes
I[10:03:51.067] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:03:51.068] Built preamble of size 115572 for file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\pitches.h version 1
V[10:03:51.082] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp (digest:=4A1244E54C0CAC04)
V[10:03:51.084] System include extraction: target extracted: "avr"
V[10:03:51.084] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:03:51.084] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:03:51.084] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:03:51.084] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:03:51.085] System include extraction: target extracted: "avr"
V[10:03:51.085] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:03:51.085] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:03:51.085] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:03:51.085] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:03:51.096] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp (digest:=3DD4F70FCF8C4FA6)
V[10:03:51.097] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp (digest:=293923F15565174B)
V[10:03:51.121] indexed preamble AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp version 1:
  symbol slab: 2588 symbols, 736150 bytes
  ref slab: 0 symbols, 0 refs, 136 bytes
  relations slab: 9 relations, 177 bytes
V[10:03:51.134] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\pitches.h version 1:
  symbol slab: 89 symbols, 24872 bytes
  ref slab: 89 symbols, 89 refs, 6488 bytes
  relations slab: 0 relations, 24 bytes
V[10:03:51.134] Build dynamic index for main-file symbols with estimated memory usage of 59976 bytes
I[10:03:51.134] --> textDocument/publishDiagnostics
V[10:03:51.134] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/pitches.h","version":1}}

V[10:03:51.134] ASTWorker running EnumerateTweaks on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\pitches.h
I[10:03:51.134] --> reply:textDocument/codeAction("2") 266 ms
V[10:03:51.134] >>> {"id":"2","jsonrpc":"2.0","result":[]}

V[10:03:51.136] <<< {"id":"3","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:03:51.137] <-- textDocument/documentSymbol("3")
V[10:03:51.152] Build dynamic index for header symbols with estimated memory usage of 2191550 bytes
V[10:03:51.154] Built preamble of size 434172 for file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp version 1
I[10:03:51.163] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp (42 symbols, 134 refs, 3 files)
I[10:03:51.171] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c (311 symbols, 2694 refs, 25 files)
I[10:03:51.181] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c (310 symbols, 2898 refs, 25 files)
V[10:03:51.215] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp version 1:
  symbol slab: 4 symbols, 5152 bytes
  ref slab: 14 symbols, 20 refs, 4688 bytes
  relations slab: 0 relations, 24 bytes
V[10:03:51.215] Build dynamic index for main-file symbols with estimated memory usage of 71384 bytes
I[10:03:51.215] --> textDocument/publishDiagnostics
V[10:03:51.215] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp","version":1}}

V[10:03:51.215] ASTWorker running DocumentSymbols on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
I[10:03:51.215] --> reply:textDocument/documentSymbol("3") 78 ms
V[10:03:51.215] >>> {"id":"3","jsonrpc":"2.0","result":[{"detail":"int[8]","kind":13,"name":"melody","range":{"end":{"character":71,"line":5},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

I[10:03:51.226] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp (299 symbols, 2470 refs, 18 files)
I[10:03:51.229] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp (600 symbols, 3432 refs, 36 files)
I[10:03:51.235] --> $/progress
V[10:03:51.235] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"2/27","percentage":7}}}

I[10:03:51.235] --> $/progress
V[10:03:51.235] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"2/27","percentage":7}}}

V[10:03:51.247] <<< {"id":"4","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":10,"line":13},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:03:51.247] <-- textDocument/hover("4")
V[10:03:51.247] ASTWorker running Hover on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
V[10:03:51.247] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp (digest:=313C4893EB7ADBE6)
I[10:03:51.250] --> reply:textDocument/hover("4") 3 ms
V[10:03:51.250] >>> {"id":"4","jsonrpc":"2.0","result":null}

I[10:03:51.275] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp (602 symbols, 3499 refs, 37 files)
I[10:03:51.380] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp (514 symbols, 3283 refs, 35 files)
I[10:03:51.535] --> $/progress
V[10:03:51.535] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"3/27","percentage":11}}}

I[10:03:51.535] --> $/progress
V[10:03:51.535] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"3/27","percentage":11}}}

V[10:03:51.537] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c (digest:=5D6C1534064234DD)
I[10:03:51.546] --> $/progress
V[10:03:51.546] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"4/27","percentage":14}}}

I[10:03:51.546] --> $/progress
V[10:03:51.546] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"4/27","percentage":14}}}

V[10:03:51.549] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp (digest:=487C94A1A1F49B6C)
I[10:03:51.617] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c (8 symbols, 2247 refs, 25 files)
I[10:03:51.626] --> $/progress
V[10:03:51.626] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"5/27","percentage":18}}}

I[10:03:51.626] --> $/progress
V[10:03:51.626] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"5/27","percentage":18}}}

V[10:03:51.629] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c (digest:=5E8D23E876F6F446)
I[10:03:51.640] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp (76 symbols, 2445 refs, 37 files)
I[10:03:51.646] --> $/progress
V[10:03:51.646] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"6/27","percentage":22}}}

I[10:03:51.646] --> $/progress
V[10:03:51.646] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"6/27","percentage":22}}}

V[10:03:51.648] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp (digest:=38075D39C713EC91)
I[10:03:51.683] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp (46 symbols, 139 refs, 3 files)
I[10:03:51.687] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c (2 symbols, 2115 refs, 25 files)
V[10:03:51.709] BackgroundIndex: building version 1 after indexing enough files
I[10:03:51.709] --> $/progress
V[10:03:51.709] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"7/27","percentage":25}}}

I[10:03:51.709] --> $/progress
V[10:03:51.709] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"7/27","percentage":25}}}

V[10:03:51.713] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c (digest:=B0774BE9D28D49CB)
V[10:03:51.725] BackgroundIndex: serving version 1 (1484146 bytes)
I[10:03:51.726] --> $/progress
V[10:03:51.726] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"8/27","percentage":29}}}

I[10:03:51.726] --> $/progress
V[10:03:51.726] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"8/27","percentage":29}}}

I[10:03:51.728] --> $/progress
V[10:03:51.728] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"9/27","percentage":33}}}

I[10:03:51.728] --> $/progress
V[10:03:51.728] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"9/27","percentage":33}}}

V[10:03:51.729] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c (digest:=C16B0ED8B1C5BB9F)
V[10:03:51.730] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp (digest:=F68AA83B5BAAD75D)
I[10:03:51.751] --> $/progress
V[10:03:51.751] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"10/27","percentage":37}}}

I[10:03:51.751] --> $/progress
V[10:03:51.751] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"10/27","percentage":37}}}

V[10:03:51.753] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c (digest:=BC32CF542FD8D605)
I[10:03:51.769] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c (1 symbols, 1 refs, 1 files)
I[10:03:51.772] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp (21 symbols, 150 refs, 5 files)
I[10:03:51.786] --> $/progress
V[10:03:51.786] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"11/27","percentage":40}}}

I[10:03:51.786] --> $/progress
V[10:03:51.786] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"11/27","percentage":40}}}

V[10:03:51.788] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp (digest:=81BB1157C290C33B)
I[10:03:51.800] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c (2 symbols, 2141 refs, 25 files)
I[10:03:51.818] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c (4 symbols, 2201 refs, 25 files)
I[10:03:51.820] --> $/progress
V[10:03:51.820] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"12/27","percentage":44}}}

I[10:03:51.820] --> $/progress
V[10:03:51.820] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"12/27","percentage":44}}}

I[10:03:51.823] --> $/progress
V[10:03:51.823] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"13/27","percentage":48}}}

I[10:03:51.823] --> $/progress
V[10:03:51.823] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"13/27","percentage":48}}}

V[10:03:51.824] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp (digest:=365287FBD658A80E)
V[10:03:51.826] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp (digest:=6DDB6ED4F4E34E63)
I[10:03:51.833] --> $/progress
V[10:03:51.833] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"14/27","percentage":51}}}

I[10:03:51.833] --> $/progress
V[10:03:51.833] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"14/27","percentage":51}}}

V[10:03:51.836] Indexing C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp (digest:=17390AE5437DD899)
I[10:03:51.881] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp (26 symbols, 2373 refs, 35 files)
I[10:03:51.911] --> $/progress
V[10:03:51.911] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"15/27","percentage":55}}}

I[10:03:51.911] --> $/progress
V[10:03:51.911] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"15/27","percentage":55}}}

I[10:03:51.913] Indexed C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp (4 symbols, 2323 refs, 36 files)
I[10:03:51.915] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp (20 symbols, 2357 refs, 36 files)
I[10:03:51.916] --> $/progress
V[10:03:51.916] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"16/27","percentage":59}}}

I[10:03:51.916] --> $/progress
V[10:03:51.916] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"16/27","percentage":59}}}

V[10:03:51.917] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp (digest:=7D1D0E442CF15FC1)
V[10:03:51.919] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp (digest:=1C31198B0754810E)
I[10:03:51.933] --> $/progress
V[10:03:51.933] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"17/27","percentage":62}}}

I[10:03:51.933] --> $/progress
V[10:03:51.933] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"17/27","percentage":62}}}

I[10:03:51.933] --> $/progress
V[10:03:51.933] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"18/27","percentage":66}}}

I[10:03:51.933] --> $/progress
V[10:03:51.933] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"18/27","percentage":66}}}

V[10:03:51.934] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp (digest:=D7FFC6931C21680C)
V[10:03:51.935] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp (digest:=FDB5BCAAB3E73FCE)
I[10:03:51.940] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp (2 symbols, 2280 refs, 37 files)
I[10:03:51.978] --> $/progress
V[10:03:51.978] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"19/27","percentage":70}}}

I[10:03:51.978] --> $/progress
V[10:03:51.978] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"19/27","percentage":70}}}

V[10:03:51.981] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp (digest:=F7D59D2B49112307)
I[10:03:52.008] --> $/progress
V[10:03:52.008] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"20/27","percentage":74}}}

I[10:03:52.008] --> $/progress
V[10:03:52.008] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"20/27","percentage":74}}}

V[10:03:52.013] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp (digest:=E3E9F11672EDD20A)
I[10:03:52.017] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp (0 symbols, 2222 refs, 36 files)
I[10:03:52.018] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp (0 symbols, 2251 refs, 37 files)
I[10:03:52.021] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp (15 symbols, 2449 refs, 35 files)
I[10:03:52.025] --> $/progress
V[10:03:52.025] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"21/27","percentage":77}}}

I[10:03:52.026] --> $/progress
V[10:03:52.026] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"21/27","percentage":77}}}

I[10:03:52.027] --> $/progress
V[10:03:52.028] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"22/27","percentage":81}}}

I[10:03:52.036] --> $/progress
V[10:03:52.036] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"23/27","percentage":85}}}

I[10:03:52.049] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp (12 symbols, 2468 refs, 38 files)
I[10:03:52.061] --> $/progress
V[10:03:52.061] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"24/27","percentage":88}}}

I[10:03:52.083] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp (15 symbols, 2336 refs, 35 files)
V[10:03:52.089] Ignored diagnostic. c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include\avr/wdt.h:464:12:value '64' out of range for constraint 'I'
I[10:03:52.089] --> $/progress
V[10:03:52.089] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"25/27","percentage":92}}}

V[10:03:52.090] Ignored diagnostic. c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include\avr/wdt.h:507:23:value '64' out of range for constraint 'I'
I[10:03:52.097] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp (2 symbols, 2307 refs, 37 files)
I[10:03:52.097] Failed to compile C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp, index may be incomplete
V[10:03:52.098] System include extraction: target extracted: "avr"
V[10:03:52.098] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:03:52.098] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:03:52.098] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:03:52.098] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-gcc.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:03:52.099] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S (digest:=87583F1C920AA889)
I[10:03:52.112] --> $/progress
V[10:03:52.112] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"26/27","percentage":96}}}

V[10:03:52.131] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:54:1:expected identifier or '('
V[10:03:52.131] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:62:23:expected identifier or '('
V[10:03:52.131] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:63:23:expected identifier or '('
V[10:03:52.131] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:64:23:expected identifier or '('
V[10:03:52.131] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:65:23:expected identifier or '('
V[10:03:52.131] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:66:23:expected identifier or '('
V[10:03:52.131] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:67:23:expected identifier or '('
V[10:03:52.131] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:72:37:expected identifier or '('
V[10:03:52.131] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:73:31:expected ';' after top level declarator
V[10:03:52.131] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:79:23:expected identifier or '('
V[10:03:52.131] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:83:32:expected identifier or '('
V[10:03:52.132] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:83:35:expected identifier or '('
V[10:03:52.132] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:84:22:unknown type name 'maxloops'
V[10:03:52.132] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:85:8:expected ';' after top level declarator
V[10:03:52.132] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:85:22:unknown type name 'maxloops'
V[10:03:52.132] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:86:8:expected ';' after top level declarator
V[10:03:52.132] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:86:22:unknown type name 'maxloops'
V[10:03:52.133] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:87:9:expected ';' after top level declarator
V[10:03:52.133] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:87:18:expected identifier or '('
V[10:03:52.133] Ignored diagnostic. too many errors emitted, stopping now
I[10:03:52.136] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S (12 symbols, 937 refs, 9 files)
I[10:03:52.136] Failed to compile C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S, index may be incomplete
V[10:03:52.160] BackgroundIndex: building version 2 when background indexer is idle
V[10:03:52.171] BackgroundIndex: serving version 2 (1777894 bytes)
I[10:03:52.172] --> $/progress
V[10:03:52.172] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[10:03:53.998] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:03:53.998] <-- textDocument/didSave
I[10:03:53.998] File version went from 1 to 1
I[10:03:53.998] File version went from 1 to 1
V[10:03:53.998] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\n\n#include \"pitches.h\"// notes in the melody:\nint melody[] = {\nNOTE_C5, NOTE_D5, NOTE_E5, NOTE_F5, NOTE_G5, NOTE_A5, NOTE_B5, NOTE_C6};\nint duration = 500;  // 500 miliseconds \n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup();\n#line 7 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid loop();\n#line 6 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 5_Active_buzzer\\\\5_Active_buzzer\\\\5_Active_buzzer.ino\"\nvoid setup() {  }\nvoid loop() {\nfor (int thisNote = 0; thisNote < 12; thisNote++) {\n// pin12 output the voice, every scale is 0.5 sencond \ntone(12, melody[thisNote], duration);\ndelay(100);\n// Output the voice after several minutes\ndelay(100);\n} // restart after two seconds \ndelay(200);\n}\n\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp","version":2}}}

I[10:03:53.999] <-- textDocument/didChange
V[10:03:53.999] ASTWorker skipping Update (1) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
I[10:03:54.064] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp version 2 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420\\sketch\\5_Active_buzzer.ino.cpp"
I[10:03:54.080] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\pitches.h version 1 with command inferred from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -x c++-header -std=gnu++11 -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420\\sketch\\pitches.h"
V[10:03:54.089] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 5_Active_buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420\\sketch\\5_Active_buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420\\sketch\\5_Active_buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420\\sketch\\5_Active_buzzer.ino.cpp"
V[10:03:54.097] Reusing preamble version 1 for version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
V[10:03:54.105] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name pitches.h -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file pitches.d -MT pitches.o -module-file-deps -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++-header "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server687930420\\sketch\\pitches.h"
V[10:03:54.106] Rebuilding invalidated preamble for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\pitches.h version 1 (previous was version 1)
V[10:03:54.121] indexed preamble AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\pitches.h version 1:
  symbol slab: 93 symbols, 25800 bytes
  ref slab: 0 symbols, 0 refs, 136 bytes
  relations slab: 0 relations, 24 bytes
V[10:03:54.144] Build dynamic index for header symbols with estimated memory usage of 2191422 bytes
V[10:03:54.145] Built preamble of size 116228 for file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\pitches.h version 1
V[10:03:54.196] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\pitches.h version 1:
  symbol slab: 89 symbols, 24872 bytes
  ref slab: 89 symbols, 89 refs, 6488 bytes
  relations slab: 0 relations, 24 bytes
V[10:03:54.196] Build dynamic index for main-file symbols with estimated memory usage of 71384 bytes
I[10:03:54.196] --> textDocument/publishDiagnostics
V[10:03:54.196] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/pitches.h","version":1}}

V[10:04:04.255] <<< {"id":"5","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":13,"line":13},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:04:04.255] <-- textDocument/hover("5")
V[10:04:04.259] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
I[10:04:04.262] --> reply:textDocument/hover("5") 6 ms
V[10:04:04.262] >>> {"id":"5","jsonrpc":"2.0","result":null}

V[10:04:06.238] <<< {"id":"6","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/pitches.h"}}}

I[10:04:06.238] <-- textDocument/documentSymbol("6")
V[10:04:06.238] ASTWorker running DocumentSymbols on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\pitches.h
I[10:04:06.238] --> reply:textDocument/documentSymbol("6") 0 ms
V[10:04:06.238] >>> {"id":"6","jsonrpc":"2.0","result":[]}

V[10:04:11.463] <<< {"id":"7","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:04:11.463] <-- textDocument/documentSymbol("7")
V[10:04:11.466] ASTWorker running DocumentSymbols on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
I[10:04:11.467] --> reply:textDocument/documentSymbol("7") 3 ms
V[10:04:11.467] >>> {"id":"7","jsonrpc":"2.0","result":[{"detail":"int[8]","kind":13,"name":"melody","range":{"end":{"character":71,"line":5},"start":{"character":0,"line":4}},"selectionRange":{"end":{"character":10,"line":4},"start":{"character":4,"line":4}}},{"detail":"int","kind":13,"name":"duration","range":{"end":{"character":18,"line":6},"start":{"character":0,"line":6}},"selectionRange":{"end":{"character":12,"line":6},"start":{"character":4,"line":6}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":8},"start":{"character":0,"line":8}},"selectionRange":{"end":{"character":10,"line":8},"start":{"character":5,"line":8}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":10},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":17,"line":12},"start":{"character":0,"line":12}},"selectionRange":{"end":{"character":10,"line":12},"start":{"character":5,"line":12}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":22},"start":{"character":0,"line":13}},"selectionRange":{"end":{"character":9,"line":13},"start":{"character":5,"line":13}}}]}

V[10:04:22.944] <<< {"id":"8","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":17,"line":15},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:04:22.944] <-- textDocument/hover("8")
V[10:04:22.948] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
I[10:04:22.951] --> reply:textDocument/hover("8") 6 ms
V[10:04:22.951] >>> {"id":"8","jsonrpc":"2.0","result":null}

V[10:04:23.352] <<< {"id":"9","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":16,"line":14},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:04:23.352] <-- textDocument/hover("9")
V[10:04:23.352] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
I[10:04:23.356] --> reply:textDocument/hover("9") 3 ms
V[10:04:23.356] >>> {"id":"9","jsonrpc":"2.0","result":{"contents":{"kind":"markdown","value":"### variable `thisNote`  \n\n---\nType: `int`  \nValue = `0`  \n\n---\n```cpp\n// In loop\nint thisNote = 0\n```"},"range":{"end":{"character":17,"line":14},"start":{"character":9,"line":14}}}}

V[10:04:28.292] <<< {"id":"10","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":14,"line":12},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:04:28.292] <-- textDocument/hover("10")
V[10:04:28.296] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
I[10:04:28.299] --> reply:textDocument/hover("10") 6 ms
V[10:04:28.299] >>> {"id":"10","jsonrpc":"2.0","result":null}

V[10:07:26.610] <<< {"id":"11","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":1,"line":22},"start":{"character":1,"line":22}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:07:26.610] <-- textDocument/codeAction("11")
V[10:07:26.613] ASTWorker running EnumerateTweaks on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
I[10:07:26.613] --> reply:textDocument/codeAction("11") 3 ms
V[10:07:26.614] >>> {"id":"11","jsonrpc":"2.0","result":[]}

V[10:07:52.594] <<< {"id":"12","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":1,"line":22},"start":{"character":0,"line":3}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:07:52.595] <-- textDocument/codeAction("12")
V[10:07:52.598] ASTWorker running EnumerateTweaks on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
I[10:07:52.598] --> reply:textDocument/codeAction("12") 3 ms
V[10:07:52.598] >>> {"id":"12","jsonrpc":"2.0","result":[]}

V[10:07:53.352] <<< {"id":"13","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":13,"line":14},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:07:53.352] <-- textDocument/hover("13")
V[10:07:53.352] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
I[10:07:53.356] --> reply:textDocument/hover("13") 3 ms
V[10:07:53.356] >>> {"id":"13","jsonrpc":"2.0","result":{"contents":{"kind":"markdown","value":"### variable `thisNote`  \n\n---\nType: `int`  \nValue = `0`  \n\n---\n```cpp\n// In loop\nint thisNote = 0\n```"},"range":{"end":{"character":17,"line":14},"start":{"character":9,"line":14}}}}

V[10:07:53.555] <<< {"id":"14","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":13,"line":13},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:07:53.555] <-- textDocument/hover("14")
V[10:07:53.555] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
I[10:07:53.558] --> reply:textDocument/hover("14") 3 ms
V[10:07:53.558] >>> {"id":"14","jsonrpc":"2.0","result":null}

V[10:07:54.474] <<< {"id":"15","jsonrpc":"2.0","method":"textDocument/definition","params":{"position":{"character":17,"line":15},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:07:54.474] <-- textDocument/definition("15")
V[10:07:54.474] ASTWorker running Definitions on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
I[10:07:54.474] --> reply:textDocument/definition("15") 0 ms
V[10:07:54.474] >>> {"id":"15","jsonrpc":"2.0","result":[]}

V[10:07:54.994] <<< {"id":"16","jsonrpc":"2.0","method":"textDocument/definition","params":{"position":{"character":26,"line":18},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:07:54.994] <-- textDocument/definition("16")
V[10:07:54.994] ASTWorker running Definitions on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
I[10:07:54.994] --> reply:textDocument/definition("16") 0 ms
V[10:07:54.994] >>> {"id":"16","jsonrpc":"2.0","result":[]}

V[10:07:55.681] <<< {"id":"17","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":11,"line":21},"start":{"character":11,"line":21}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server687930420/sketch/5_Active_buzzer.ino.cpp"}}}

I[10:07:55.681] <-- textDocument/codeAction("17")
V[10:07:55.681] ASTWorker running EnumerateTweaks on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server687930420\sketch\5_Active_buzzer.ino.cpp
I[10:07:55.681] --> reply:textDocument/codeAction("17") 0 ms
V[10:07:55.681] >>> {"id":"17","jsonrpc":"2.0","result":[]}

V[10:22:57.986] <<< {"id":"18","jsonrpc":"2.0","method":"shutdown","params":null}

I[10:22:57.987] <-- shutdown("18")
I[10:22:57.987] --> reply:shutdown("18") 0 ms
V[10:22:57.987] >>> {"id":"18","jsonrpc":"2.0","result":null}

