






Started logging.
I[10:09:53.936] clangd version 14.0.0
I[10:09:53.938] Features: windows
I[10:09:53.938] PID: 18796
I[10:09:53.939] Working directory: g:\11.ZhiYi\5.Tutorial\1.tutorial\ZYA0008蜂鸣器等等传感器\Code\Lesson 6_Passive_Buzzer\6_Passive_Buzzer
I[10:09:53.939] argv[0]: d:\Program Files\Arduino IDE\resources\app\node_modules\arduino-ide-extension\build\clangd.exe
I[10:09:53.939] argv[1]: -log=verbose
I[10:09:53.939] argv[2]: --compile-commands-dir=C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897
I[10:09:53.939] argv[3]: -query-driver=C:\Users\Administrator\AppData\Local\Arduino15\packages\**
V[10:09:53.945] User config file is C:\Users\Administrator\AppData\Local\clangd\config.yaml
I[10:09:53.946] Starting LSP over stdin/stdout
V[10:09:53.946] <<< {"id":"1","jsonrpc":"2.0","method":"initialize","params":{"capabilities":{"textDocument":{"codeAction":{"codeActionLiteralSupport":{"codeActionKind":{"valueSet":["","quickfix","refactor","refactor.extract","refactor.inline","refactor.rewrite","source","source.organizeImports"]}},"dynamicRegistration":true,"isPreferredSupport":true},"codeLens":{"dynamicRegistration":true},"colorProvider":{"dynamicRegistration":true},"completion":{"completionItem":{"commitCharactersSupport":true,"deprecatedSupport":true,"documentationFormat":["markdown","plaintext"],"preselectSupport":true,"snippetSupport":true,"tagSupport":{"valueSet":[1]}},"completionItemKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25]},"contextSupport":true,"dynamicRegistration":true},"declaration":{"dynamicRegistration":true,"linkSupport":true},"definition":{"dynamicRegistration":true,"linkSupport":true},"documentHighlight":{"dynamicRegistration":true},"documentLink":{"dynamicRegistration":true,"tooltipSupport":true},"documentSymbol":{"dynamicRegistration":true,"hierarchicalDocumentSymbolSupport":true,"symbolKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26]}},"foldingRange":{"dynamicRegistration":true,"lineFoldingOnly":true,"rangeLimit":5000},"formatting":{"dynamicRegistration":true},"hover":{"contentFormat":["markdown","plaintext"],"dynamicRegistration":true},"implementation":{"dynamicRegistration":true,"linkSupport":true},"onTypeFormatting":{"dynamicRegistration":true},"publishDiagnostics":{"relatedInformation":true,"tagSupport":{"valueSet":[1,2]}},"rangeFormatting":{"dynamicRegistration":true},"references":{"dynamicRegistration":true},"rename":{"dynamicRegistration":true,"prepareSupport":true},"selectionRange":{"dynamicRegistration":true},"signatureHelp":{"contextSupport":true,"dynamicRegistration":true,"signatureInformation":{"documentationFormat":["markdown","plaintext"],"parameterInformation":{"labelOffsetSupport":true}}},"synchronization":{"didSave":true,"dynamicRegistration":true,"willSave":true,"willSaveWaitUntil":true},"typeDefinition":{"dynamicRegistration":true,"linkSupport":true}},"window":{"workDoneProgress":true},"workspace":{"applyEdit":true,"configuration":true,"didChangeConfiguration":{"dynamicRegistration":true},"didChangeWatchedFiles":{"dynamicRegistration":true},"executeCommand":{"dynamicRegistration":true},"symbol":{"dynamicRegistration":true,"symbolKind":{"valueSet":[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26]}},"workspaceEdit":{"documentChanges":true,"failureHandling":"textOnlyTransactional","resourceOperations":["create","rename","delete"]},"workspaceFolders":true}},"clientInfo":{"name":"vscode","version":"1.53.2"},"initializationOptions":{},"processId":4156,"rootPath":"C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server3760075897\\sketch","rootUri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch","trace":"off","workspaceFolders":[{"name":"6_Passive_Buzzer","uri":"file:///g%3A/11.ZhiYi/5.Tutorial/1.tutorial/ZYA0008%E8%9C%82%E9%B8%A3%E5%99%A8%E7%AD%89%E7%AD%89%E4%BC%A0%E6%84%9F%E5%99%A8/Code/Lesson%206_Passive_Buzzer/6_Passive_Buzzer"}]}}

I[10:09:53.946] <-- initialize("1")
I[10:09:54.007] --> reply:initialize("1") 61 ms
V[10:09:54.007] >>> {"id":"1","jsonrpc":"2.0","result":{"capabilities":{"astProvider":true,"callHierarchyProvider":true,"clangdInlayHintsProvider":true,"codeActionProvider":{"codeActionKinds":["quickfix","refactor","info"]},"compilationDatabase":{"automaticReload":true},"completionProvider":{"allCommitCharacters":[" ","\t","(",")","[","]","{","}","<",">",":",";",",","+","-","/","*","%","^","&","#","?",".","=","\"","'","|"],"resolveProvider":false,"triggerCharacters":[".","<",">",":","\"","/","*"]},"declarationProvider":true,"definitionProvider":true,"documentFormattingProvider":true,"documentHighlightProvider":true,"documentLinkProvider":{"resolveProvider":false},"documentOnTypeFormattingProvider":{"firstTriggerCharacter":"\n","moreTriggerCharacter":[]},"documentRangeFormattingProvider":true,"documentSymbolProvider":true,"executeCommandProvider":{"commands":["clangd.applyFix","clangd.applyTweak"]},"hoverProvider":true,"implementationProvider":true,"memoryUsageProvider":true,"referencesProvider":true,"renameProvider":{"prepareProvider":true},"selectionRangeProvider":true,"semanticTokensProvider":{"full":{"delta":true},"legend":{"tokenModifiers":["declaration","deprecated","deduced","readonly","static","abstract","virtual","dependentName","defaultLibrary","usedAsMutableReference","functionScope","classScope","fileScope","globalScope"],"tokenTypes":["variable","variable","parameter","function","method","function","property","variable","class","interface","enum","enumMember","type","type","unknown","namespace","typeParameter","concept","type","macro","comment"]},"range":false},"signatureHelpProvider":{"triggerCharacters":["(",")","{","}","<",">",","]},"textDocumentSync":{"change":2,"openClose":true,"save":true},"typeDefinitionProvider":true,"typeHierarchyProvider":true,"workspaceSymbolProvider":true},"serverInfo":{"name":"clangd","version":"clangd version 14.0.0 windows x86_64-pc-windows-msvc"}}}

V[10:09:54.008] <<< {"jsonrpc":"2.0","method":"initialized","params":{}}

I[10:09:54.008] <-- initialized
V[10:09:54.014] <<< {"jsonrpc":"2.0","method":"textDocument/didOpen","params":{"textDocument":{"languageId":"cpp","text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 6_Passive_Buzzer\\\\6_Passive_Buzzer\\\\6_Passive_Buzzer.ino\"\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 6_Passive_Buzzer\\\\6_Passive_Buzzer\\\\6_Passive_Buzzer.ino\"\nvoid setup();\n#line 4 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 6_Passive_Buzzer\\\\6_Passive_Buzzer\\\\6_Passive_Buzzer.ino\"\nvoid loop();\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 6_Passive_Buzzer\\\\6_Passive_Buzzer\\\\6_Passive_Buzzer.ino\"\nvoid setup()\n{\n}\nvoid loop()\n{\n  for(int i=200;i<=800;i++)  //Increase the frequency from 200HZ to 800HZ in a loop\n  {\n    pinMode(8,OUTPUT);\n    tone(8,i);  //Output frequency on port 8 delay(5);    //This frequency is maintained for 5 milliseconds\n  }\n  delay(4000);  //Hold for 4 seconds at the highest frequency\n  for(int i=800;i>=200;i--)\n  {\n    pinMode(8,OUTPUT); tone(8,i);\n    delay(10);\n  }\n}\n\n","uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp","version":1}}}

I[10:09:54.014] <-- textDocument/didOpen
V[10:09:54.018] config note at C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\.clangd:1:0: Parsing config fragment
V[10:09:54.018] config note at C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\.clangd:1:0: Parsed 1 fragments from file
V[10:09:54.018] Config fragment: compiling C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\.clangd:1 -> 0x000001F94C779BE0 (trusted=false)
I[10:09:54.019] --> textDocument/publishDiagnostics
V[10:09:54.019] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/.clangd"}}

I[10:09:54.020] Loaded compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\compile_commands.json
V[10:09:54.020] Broadcasting compilation database from C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897
V[10:09:54.020] <<< {"id":"2","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":14,"line":21},"start":{"character":14,"line":21}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp"}}}

I[10:09:54.020] <-- textDocument/codeAction("2")
I[10:09:54.023] --> window/workDoneProgress/create(0)
V[10:09:54.023] >>> {"id":0,"jsonrpc":"2.0","method":"window/workDoneProgress/create","params":{"token":"backgroundIndexProgress"}}

I[10:09:54.023] Enqueueing 26 commands for indexing
V[10:09:54.024] <<< {"id":0,"jsonrpc":"2.0","result":null}

I[10:09:54.024] <-- reply(0)
I[10:09:54.024] --> $/progress
V[10:09:54.024] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"begin","percentage":0,"title":"indexing"}}}

I[10:09:54.024] --> $/progress
V[10:09:54.024] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/1","percentage":0}}}

V[10:09:54.024] Failed to load shard: C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp
V[10:09:54.024] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp
V[10:09:54.025] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp
V[10:09:54.025] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c
V[10:09:54.025] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c
V[10:09:54.025] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp
V[10:09:54.025] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp
V[10:09:54.025] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp
V[10:09:54.025] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp
V[10:09:54.025] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp
V[10:09:54.025] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp
V[10:09:54.025] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S
V[10:09:54.025] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp
V[10:09:54.026] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp
V[10:09:54.026] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp
V[10:09:54.026] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp
V[10:09:54.026] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp
V[10:09:54.026] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c
V[10:09:54.026] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp
V[10:09:54.026] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c
V[10:09:54.026] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c
V[10:09:54.026] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp
V[10:09:54.026] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp
V[10:09:54.027] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c
V[10:09:54.027] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp
V[10:09:54.027] Failed to load shard: C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c
I[10:09:54.031] --> $/progress
V[10:09:54.031] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[10:09:54.032] --> $/progress
V[10:09:54.032] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[10:09:54.032] --> $/progress
V[10:09:54.032] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[10:09:54.032] --> $/progress
V[10:09:54.032] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[10:09:54.032] --> $/progress
V[10:09:54.032] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[10:09:54.032] --> $/progress
V[10:09:54.032] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"0/27","percentage":0}}}

I[10:09:54.032] --> $/progress
V[10:09:54.032] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

I[10:09:54.032] --> $/progress
V[10:09:54.032] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"1/27","percentage":3}}}

V[10:09:54.152] System include extraction: target extracted: "avr"
V[10:09:54.152] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:09:54.152] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:09:54.152] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:09:54.152] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
I[10:09:54.153] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp version 1 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server3760075897\\sketch\\6_Passive_Buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server3760075897\\sketch\\6_Passive_Buzzer.ino.cpp"
V[10:09:54.163] System include extraction: target extracted: "avr"
V[10:09:54.163] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:09:54.163] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:09:54.163] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:09:54.163] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:09:54.165] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp (digest:=3DD4F70FCF8C4FA6)
V[10:09:54.179] System include extraction: target extracted: "avr"
V[10:09:54.179] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:09:54.179] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:09:54.179] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:09:54.179] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:09:54.181] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp (digest:=F68AA83B5BAAD75D)
V[10:09:54.181] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 6_Passive_Buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server3760075897\\sketch\\6_Passive_Buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server3760075897\\sketch\\6_Passive_Buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server3760075897\\sketch\\6_Passive_Buzzer.ino.cpp"
V[10:09:54.181] Building first preamble for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp version 1
V[10:09:54.197] System include extraction: target extracted: "avr"
V[10:09:54.197] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:09:54.197] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:09:54.197] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:09:54.197] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:09:54.199] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp (digest:=6DDB6ED4F4E34E63)
V[10:09:54.224] System include extraction: target extracted: "avr"
V[10:09:54.224] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:09:54.224] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:09:54.224] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:09:54.224] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-gcc.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:09:54.225] System include extraction: target extracted: "avr"
V[10:09:54.225] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:09:54.225] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:09:54.225] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:09:54.225] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-gcc.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
I[10:09:54.227] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\new.cpp (61 symbols, 201 refs, 5 files)
V[10:09:54.228] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c (digest:=343A7ACAD5FD2414)
V[10:09:54.232] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c (digest:=0A36B38756A4F148)
V[10:09:54.246] System include extraction: target extracted: "avr"
V[10:09:54.246] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:09:54.246] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:09:54.246] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:09:54.247] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-g++.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:09:54.263] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp (digest:=38075D39C713EC91)
V[10:09:54.266] indexed preamble AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp version 1:
  symbol slab: 2499 symbols, 711406 bytes
  ref slab: 0 symbols, 0 refs, 136 bytes
  relations slab: 9 relations, 177 bytes
I[10:09:54.272] --> $/progress
V[10:09:54.272] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"2/27","percentage":7}}}

I[10:09:54.272] --> $/progress
V[10:09:54.272] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"2/27","percentage":7}}}

I[10:09:54.297] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial2.cpp (602 symbols, 3499 refs, 37 files)
V[10:09:54.300] Build dynamic index for header symbols with estimated memory usage of 2157986 bytes
V[10:09:54.302] Built preamble of size 428064 for file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp version 1
I[10:09:54.334] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WMath.cpp (46 symbols, 139 refs, 3 files)
I[10:09:54.346] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\IPAddress.cpp (620 symbols, 3567 refs, 36 files)
V[10:09:54.357] System include extraction: target extracted: "avr"
V[10:09:54.357] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include

V[10:09:54.357] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed

V[10:09:54.357] System include extraction: adding  c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include

I[10:09:54.357] System includes extractor: successfully executed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\avr-gcc.exe
	got includes: "c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/include-fixed, c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include"
	got target: "avr"
V[10:09:54.359] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S (digest:=87583F1C920AA889)
V[10:09:54.369] indexed file AST for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp version 1:
  symbol slab: 2 symbols, 4688 bytes
  ref slab: 6 symbols, 12 refs, 4376 bytes
  relations slab: 0 relations, 24 bytes
V[10:09:54.369] Build dynamic index for main-file symbols with estimated memory usage of 12472 bytes
I[10:09:54.369] --> textDocument/publishDiagnostics
V[10:09:54.369] >>> {"jsonrpc":"2.0","method":"textDocument/publishDiagnostics","params":{"diagnostics":[],"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp","version":1}}

V[10:09:54.370] ASTWorker running EnumerateTweaks on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp
I[10:09:54.370] --> reply:textDocument/codeAction("2") 349 ms
V[10:09:54.370] >>> {"id":"2","jsonrpc":"2.0","result":[]}

V[10:09:54.372] <<< {"id":"3","jsonrpc":"2.0","method":"textDocument/documentSymbol","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp"}}}

I[10:09:54.372] <-- textDocument/documentSymbol("3")
V[10:09:54.372] ASTWorker running DocumentSymbols on version 1 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp
I[10:09:54.372] --> reply:textDocument/documentSymbol("3") 0 ms
V[10:09:54.372] >>> {"id":"3","jsonrpc":"2.0","result":[{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":12,"line":3},"start":{"character":0,"line":3}},"selectionRange":{"end":{"character":10,"line":3},"start":{"character":5,"line":3}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":11,"line":5},"start":{"character":0,"line":5}},"selectionRange":{"end":{"character":9,"line":5},"start":{"character":5,"line":5}}},{"detail":"void ()","kind":12,"name":"setup","range":{"end":{"character":1,"line":9},"start":{"character":0,"line":7}},"selectionRange":{"end":{"character":10,"line":7},"start":{"character":5,"line":7}}},{"detail":"void ()","kind":12,"name":"loop","range":{"end":{"character":1,"line":23},"start":{"character":0,"line":10}},"selectionRange":{"end":{"character":9,"line":10},"start":{"character":5,"line":10}}}]}

I[10:09:54.376] --> $/progress
V[10:09:54.376] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"3/27","percentage":11}}}

I[10:09:54.376] --> $/progress
V[10:09:54.376] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"3/27","percentage":11}}}

I[10:09:54.380] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WInterrupts.c (311 symbols, 2694 refs, 25 files)
V[10:09:54.381] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp (digest:=365287FBD658A80E)
I[10:09:54.395] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_digital.c (310 symbols, 2898 refs, 25 files)
V[10:09:54.406] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:54:1:expected identifier or '('
V[10:09:54.406] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:62:23:expected identifier or '('
V[10:09:54.406] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:63:23:expected identifier or '('
V[10:09:54.406] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:64:23:expected identifier or '('
V[10:09:54.406] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:65:23:expected identifier or '('
V[10:09:54.406] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:66:23:expected identifier or '('
V[10:09:54.406] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:67:23:expected identifier or '('
V[10:09:54.406] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:72:37:expected identifier or '('
V[10:09:54.407] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:73:31:expected ';' after top level declarator
V[10:09:54.407] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:79:23:expected identifier or '('
V[10:09:54.407] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:83:32:expected identifier or '('
V[10:09:54.407] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:83:35:expected identifier or '('
V[10:09:54.407] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:84:22:unknown type name 'maxloops'
V[10:09:54.407] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:85:8:expected ';' after top level declarator
V[10:09:54.407] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:85:22:unknown type name 'maxloops'
V[10:09:54.407] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:86:8:expected ';' after top level declarator
V[10:09:54.407] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:86:22:unknown type name 'maxloops'
V[10:09:54.407] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:87:9:expected ';' after top level declarator
V[10:09:54.407] Ignored diagnostic. C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S:87:18:expected identifier or '('
V[10:09:54.407] Ignored diagnostic. too many errors emitted, stopping now
I[10:09:54.411] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S (12 symbols, 937 refs, 9 files)
I[10:09:54.411] Failed to compile C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.S, index may be incomplete
I[10:09:54.481] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial0.cpp (444 symbols, 3194 refs, 37 files)
I[10:09:54.560] --> $/progress
V[10:09:54.560] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"4/27","percentage":14}}}

I[10:09:54.560] --> $/progress
V[10:09:54.560] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"4/27","percentage":14}}}

V[10:09:54.565] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp (digest:=F7D59D2B49112307)
I[10:09:54.660] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Stream.cpp (289 symbols, 2924 refs, 35 files)
I[10:09:54.892] --> $/progress
V[10:09:54.892] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"5/27","percentage":18}}}

I[10:09:54.892] --> $/progress
V[10:09:54.892] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"5/27","percentage":18}}}

V[10:09:54.895] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c (digest:=B0774BE9D28D49CB)
I[10:09:54.921] --> $/progress
V[10:09:54.921] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"6/27","percentage":22}}}

I[10:09:54.921] --> $/progress
V[10:09:54.921] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"6/27","percentage":22}}}

V[10:09:54.923] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp (digest:=293923F15565174B)
V[10:09:54.960] BackgroundIndex: building version 1 after indexing enough files
I[10:09:54.961] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_pulse.c (5 symbols, 2144 refs, 25 files)
I[10:09:54.962] --> $/progress
V[10:09:54.962] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"7/27","percentage":25}}}

I[10:09:54.962] --> $/progress
V[10:09:54.962] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"7/27","percentage":25}}}

V[10:09:54.974] BackgroundIndex: serving version 1 (1475786 bytes)
I[10:09:54.976] --> $/progress
V[10:09:54.976] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"8/27","percentage":29}}}

I[10:09:54.976] --> $/progress
V[10:09:54.976] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"8/27","percentage":29}}}

I[10:09:54.976] --> $/progress
V[10:09:54.976] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"9/27","percentage":33}}}

I[10:09:54.976] --> $/progress
V[10:09:54.976] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"9/27","percentage":33}}}

V[10:09:54.979] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp (digest:=7D1D0E442CF15FC1)
V[10:09:54.981] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp (digest:=1C31198B0754810E)
V[10:09:54.983] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp (digest:=4A1244E54C0CAC04)
I[10:09:55.020] --> $/progress
V[10:09:55.020] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"10/27","percentage":37}}}

I[10:09:55.020] --> $/progress
V[10:09:55.020] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"10/27","percentage":37}}}

V[10:09:55.023] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp (digest:=E3E9F11672EDD20A)
I[10:09:55.033] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\WString.cpp (87 symbols, 1928 refs, 18 files)
I[10:09:55.039] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\abi.cpp (2 symbols, 83 refs, 3 files)
I[10:09:55.069] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial.cpp (15 symbols, 2471 refs, 38 files)
I[10:09:55.070] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Tone.cpp (18 symbols, 2452 refs, 35 files)
I[10:09:55.073] --> $/progress
V[10:09:55.073] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"11/27","percentage":40}}}

I[10:09:55.073] --> $/progress
V[10:09:55.073] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"11/27","percentage":40}}}

V[10:09:55.076] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp (digest:=81BB1157C290C33B)
I[10:09:55.081] --> $/progress
V[10:09:55.081] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"12/27","percentage":44}}}

I[10:09:55.081] --> $/progress
V[10:09:55.081] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"12/27","percentage":44}}}

V[10:09:55.084] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp (digest:=D7FFC6931C21680C)
V[10:09:55.096] Ignored diagnostic. c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include\avr/wdt.h:464:12:value '64' out of range for constraint 'I'
V[10:09:55.097] Ignored diagnostic. c:\users\administrator\appdata\local\arduino15\packages\arduino\tools\avr-gcc\7.3.0-atmel3.6.1-arduino7\bin\../lib/gcc/avr/7.3.0/../../../../avr/include\avr/wdt.h:507:23:value '64' out of range for constraint 'I'
I[10:09:55.109] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp (5 symbols, 2310 refs, 37 files)
I[10:09:55.109] Failed to compile C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\CDC.cpp, index may be incomplete
I[10:09:55.121] --> $/progress
V[10:09:55.121] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"13/27","percentage":48}}}

I[10:09:55.121] --> $/progress
V[10:09:55.121] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"13/27","percentage":48}}}

V[10:09:55.123] Indexing C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp (digest:=15FF7495DB42DB5E)
I[10:09:55.128] --> $/progress
V[10:09:55.128] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"14/27","percentage":51}}}

I[10:09:55.128] --> $/progress
V[10:09:55.129] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"14/27","percentage":51}}}

I[10:09:55.130] --> $/progress
V[10:09:55.130] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"15/27","percentage":55}}}

I[10:09:55.130] --> $/progress
V[10:09:55.130] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"15/27","percentage":55}}}

V[10:09:55.133] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp (digest:=313C4893EB7ADBE6)
V[10:09:55.134] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp (digest:=FDB5BCAAB3E73FCE)
I[10:09:55.136] --> $/progress
V[10:09:55.136] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"16/27","percentage":59}}}

I[10:09:55.136] --> $/progress
V[10:09:55.136] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"16/27","percentage":59}}}

V[10:09:55.139] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c (digest:=5D6C1534064234DD)
I[10:09:55.176] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\Print.cpp (29 symbols, 2376 refs, 35 files)
I[10:09:55.179] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial3.cpp (3 symbols, 2254 refs, 37 files)
I[10:09:55.203] Indexed C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp (5 symbols, 2229 refs, 35 files)
I[10:09:55.206] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring.c (11 symbols, 2250 refs, 25 files)
I[10:09:55.209] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\main.cpp (7 symbols, 2229 refs, 35 files)
I[10:09:55.215] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\PluggableUSB.cpp (3 symbols, 2225 refs, 36 files)
I[10:09:55.232] --> $/progress
V[10:09:55.232] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"17/27","percentage":62}}}

I[10:09:55.232] --> $/progress
V[10:09:55.232] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"17/27","percentage":62}}}

V[10:09:55.235] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp (digest:=487C94A1A1F49B6C)
I[10:09:55.241] --> $/progress
V[10:09:55.241] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"18/27","percentage":66}}}

I[10:09:55.241] --> $/progress
V[10:09:55.241] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"18/27","percentage":66}}}

V[10:09:55.247] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp (digest:=55BA50D4FF04E609)
I[10:09:55.256] --> $/progress
V[10:09:55.256] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"19/27","percentage":70}}}

I[10:09:55.256] --> $/progress
V[10:09:55.256] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"19/27","percentage":70}}}

V[10:09:55.258] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c (digest:=5E8D23E876F6F446)
I[10:09:55.259] --> $/progress
V[10:09:55.259] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"20/27","percentage":74}}}

I[10:09:55.259] --> $/progress
V[10:09:55.259] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"20/27","percentage":74}}}

V[10:09:55.260] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c (digest:=C16B0ED8B1C5BB9F)
I[10:09:55.263] --> $/progress
V[10:09:55.263] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"21/27","percentage":77}}}

I[10:09:55.263] --> $/progress
V[10:09:55.263] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"21/27","percentage":77}}}

V[10:09:55.265] Indexing C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c (digest:=BC32CF542FD8D605)
I[10:09:55.293] --> $/progress
V[10:09:55.293] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"22/27","percentage":81}}}

I[10:09:55.299] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\hooks.c (1 symbols, 1 refs, 1 files)
I[10:09:55.304] --> $/progress
V[10:09:55.304] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"23/27","percentage":85}}}

I[10:09:55.321] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_shift.c (5 symbols, 2118 refs, 25 files)
I[10:09:55.327] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\HardwareSerial1.cpp (3 symbols, 2254 refs, 37 files)
I[10:09:55.328] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\wiring_analog.c (7 symbols, 2204 refs, 25 files)
I[10:09:55.335] Indexed C:\Users\Administrator\AppData\Local\Arduino15\packages\arduino\hardware\avr\1.8.5\cores\arduino\USBCore.cpp (3 symbols, 2225 refs, 36 files)
I[10:09:55.364] --> $/progress
V[10:09:55.364] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"24/27","percentage":88}}}

I[10:09:55.373] --> $/progress
V[10:09:55.373] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"25/27","percentage":92}}}

I[10:09:55.375] --> $/progress
V[10:09:55.375] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"report","message":"26/27","percentage":96}}}

V[10:09:55.384] BackgroundIndex: building version 2 when background indexer is idle
V[10:09:55.394] BackgroundIndex: serving version 2 (1757506 bytes)
I[10:09:55.394] --> $/progress
V[10:09:55.394] >>> {"jsonrpc":"2.0","method":"$/progress","params":{"token":"backgroundIndexProgress","value":{"kind":"end"}}}

V[10:09:56.218] <<< {"jsonrpc":"2.0","method":"textDocument/didSave","params":{"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp"}}}

I[10:09:56.218] <-- textDocument/didSave
I[10:09:56.218] File version went from 1 to 1
V[10:09:56.218] <<< {"jsonrpc":"2.0","method":"textDocument/didChange","params":{"contentChanges":[{"text":"#include <Arduino.h>\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 6_Passive_Buzzer\\\\6_Passive_Buzzer\\\\6_Passive_Buzzer.ino\"\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 6_Passive_Buzzer\\\\6_Passive_Buzzer\\\\6_Passive_Buzzer.ino\"\nvoid setup();\n#line 4 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 6_Passive_Buzzer\\\\6_Passive_Buzzer\\\\6_Passive_Buzzer.ino\"\nvoid loop();\n#line 1 \"G:\\\\11.ZhiYi\\\\5.Tutorial\\\\1.tutorial\\\\ZYA0008蜂鸣器等等传感器\\\\Code\\\\Lesson 6_Passive_Buzzer\\\\6_Passive_Buzzer\\\\6_Passive_Buzzer.ino\"\nvoid setup()\n{\n}\nvoid loop()\n{\n  for(int i=200;i<=800;i++)  //Increase the frequency from 200HZ to 800HZ in a loop\n  {\n    pinMode(8,OUTPUT);\n    tone(8,i);  //Output frequency on port 8 delay(5);    //This frequency is maintained for 5 milliseconds\n  }\n  delay(4000);  //Hold for 4 seconds at the highest frequency\n  for(int i=800;i>=200;i--)\n  {\n    pinMode(8,OUTPUT); tone(8,i);\n    delay(10);\n  }\n}\n\n"}],"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp","version":2}}}

I[10:09:56.218] <-- textDocument/didChange
V[10:09:56.218] ASTWorker skipping Update (1) for C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp
I[10:09:56.292] ASTWorker building file C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp version 2 with command 
[C:\Windows\system32]
"C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\avr-g++.exe" --target=avr --driver-mode=g++ -c -g -Os -w -std=gnu++11 -fpermissive -fno-exceptions -ffunction-sections -fdata-sections -fno-threadsafe-statics -Wno-error=narrowing -MMD -flto -mmcu=atmega328p -DF_CPU=16000000L -DARDUINO=10607 -DARDUINO_AVR_UNO -DARDUINO_ARCH_AVR "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" "-IC:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -o "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server3760075897\\sketch\\6_Passive_Buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -ferror-limit=0 "-resource-dir=d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -- "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server3760075897\\sketch\\6_Passive_Buzzer.ino.cpp"
V[10:09:56.317] Driver produced command: cc1 -cc1 -triple avr -fsyntax-only -flto=full -flto-unit -disable-free -clear-ast-before-backend -disable-llvm-verifier -discard-value-names -main-file-name 6_Passive_Buzzer.ino.cpp -mrelocation-model static -mframe-pointer=all -fmath-errno -ffp-contract=on -fno-rounding-math -mconstructor-aliases -fno-use-init-array -fno-use-cxa-atexit -target-cpu atmega328p -mllvm -treat-scalable-fixed-error-as-warning -debug-info-kind=constructor -dwarf-version=5 -debugger-tuning=gdb -ffunction-sections -fdata-sections "-fcoverage-compilation-dir=C:\\Windows\\system32" -resource-dir "d:\\Program Files\\Arduino IDE\\resources\\app\\node_modules\\arduino-ide-extension\\lib\\clang\\14.0.0" -dependency-file "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server3760075897\\sketch\\6_Passive_Buzzer.ino.cpp.d" -MT "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server3760075897\\sketch\\6_Passive_Buzzer.ino.cpp.o" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/include-fixed" -isystem "c:\\users\\administrator\\appdata\\local\\arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin\\../lib/gcc/avr/7.3.0/../../../../avr/include" -D F_CPU=16000000L -D ARDUINO=10607 -D ARDUINO_AVR_UNO -D ARDUINO_ARCH_AVR -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\cores\\arduino" -I "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\hardware\\avr\\1.8.5\\variants\\standard" -internal-isystem "C:\\Users\\Administrator\\AppData\\Local\\Arduino15\\packages\\arduino\\tools\\avr-gcc\\7.3.0-atmel3.6.1-arduino7\\bin/../lib/gcc/avr/7.3.0/../../../../avr/include" -Os -Wno-error=narrowing -w -std=gnu++11 -fdeprecated-macro "-fdebug-compilation-dir=C:\\Windows\\system32" -ferror-limit 0 -fgnuc-version=4.2.1 -fno-threadsafe-statics -vectorize-loops -vectorize-slp -faddrsig -D__GCC_HAVE_DWARF2_CFI_ASM=1 -x c++ "C:\\Users\\Administrator\\AppData\\Local\\Temp\\arduino-language-server3760075897\\sketch\\6_Passive_Buzzer.ino.cpp"
V[10:09:56.324] Reusing preamble version 1 for version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp
V[10:22:43.389] <<< {"id":"4","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":33,"line":20},"start":{"character":33,"line":20}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp"}}}

I[10:22:43.389] <-- textDocument/codeAction("4")
V[10:22:43.393] ASTWorker running EnumerateTweaks on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp
I[10:22:43.393] --> reply:textDocument/codeAction("4") 3 ms
V[10:22:43.393] >>> {"id":"4","jsonrpc":"2.0","result":[]}

V[10:22:47.997] <<< {"id":"5","jsonrpc":"2.0","method":"textDocument/documentHighlight","params":{"position":{"character":6,"line":15},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp"}}}

I[10:22:47.997] <-- textDocument/documentHighlight("5")
V[10:22:47.997] ASTWorker running Highlights on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp
I[10:22:47.997] --> reply:textDocument/documentHighlight("5") 0 ms
V[10:22:47.997] >>> {"id":"5","jsonrpc":"2.0","result":[{"kind":1,"range":{"end":{"character":8,"line":15},"start":{"character":4,"line":15}}},{"kind":1,"range":{"end":{"character":27,"line":20},"start":{"character":23,"line":20}}}]}

V[10:22:48.350] <<< {"id":"6","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":8,"line":15},"start":{"character":4,"line":15}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp"}}}

I[10:22:48.350] <-- textDocument/codeAction("6")
V[10:22:48.350] ASTWorker running EnumerateTweaks on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp
I[10:22:48.350] --> reply:textDocument/codeAction("6") 0 ms
V[10:22:48.350] >>> {"id":"6","jsonrpc":"2.0","result":[]}

V[10:22:49.524] <<< {"id":"7","jsonrpc":"2.0","method":"textDocument/codeAction","params":{"context":{"diagnostics":[]},"range":{"end":{"character":14,"line":21},"start":{"character":14,"line":21}},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp"}}}

I[10:22:49.524] <-- textDocument/codeAction("7")
V[10:22:49.527] ASTWorker running EnumerateTweaks on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp
I[10:22:49.527] --> reply:textDocument/codeAction("7") 3 ms
V[10:22:49.527] >>> {"id":"7","jsonrpc":"2.0","result":[]}

V[10:22:53.841] <<< {"id":"8","jsonrpc":"2.0","method":"textDocument/hover","params":{"position":{"character":31,"line":12},"textDocument":{"uri":"file:///C:/Users/Administrator/AppData/Local/Temp/arduino-language-server3760075897/sketch/6_Passive_Buzzer.ino.cpp"}}}

I[10:22:53.841] <-- textDocument/hover("8")
V[10:22:53.841] ASTWorker running Hover on version 2 of C:\Users\Administrator\AppData\Local\Temp\arduino-language-server3760075897\sketch\6_Passive_Buzzer.ino.cpp
I[10:22:53.844] --> reply:textDocument/hover("8") 3 ms
V[10:22:53.844] >>> {"id":"8","jsonrpc":"2.0","result":null}

V[10:22:54.834] <<< {"id":"9","jsonrpc":"2.0","method":"shutdown","params":null}

I[10:22:54.834] <-- shutdown("9")
I[10:22:54.834] --> reply:shutdown("9") 0 ms
V[10:22:54.834] >>> {"id":"9","jsonrpc":"2.0","result":null}

